Linmar Scaffolding Limited


 RISK ASSESSMENT                           

Management of Health and Safety at Work Regulation 1999.
Client : Griffiths 



Assessed By : Mr P Morgan  

Date Assessed:    27/03/2019                                  Signature : ____________________

Location of works assessed:  SA1 Swansea
Work Activity

 Assessed: Erect and dismantle access scaffold fixed to quayside wall  
Mark an “ X ” in the appropriate box.
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	Key:
	
	

	Persons at risk
	Severity
	Probability

	A: Linmar Employees
	L: Low
Little chance of injury or health damage
	Re: Remote

	B: Linmar Contractors
	M: Medium 
Some chance of harm – injury- or illness
	Pr: Possible

	C: Other Contractors
	H: High 
Great chance of harm-fatality, major injury or illness causing long term disability. Changing of work method to be considered. if this is not practicable then strict adherence to the methods of control must be applied  
	Li: Likely

	D: Members of Public
	
	

	
	
	


RISK ASSESSMENT

	Depot :     Cardiff


	Client :  Griffiths

	Address:                           
Leckwith Bridge, Leckwith Road, Cardiff

CF11 8AU

Tel : 029 2046 0999
	Location : Swansea

	General Description: Access scaffold fixed to quayside wall


	Are any significant risks identified?
	yes
	X
	no   
	 

	

	Hazards
	Controls
	

	Other contractors
	1.
	 Warning signs to be displayed and barriers to be erected.
	 X

	
	2.
	Good housekeeping to be observed
	

	
	3.
	Other contractors to be made aware of working area at daily site briefing.
	

	
	4.
	All bottom lift of access ladders to be removed at end of shift.
	

	Loading & Unloading
	1.
	Driver to be fully trained in use of lorry mounted crane.
	X

	
	2.
	All boards to be securely bundled.
	

	
	3.
	All tubes to be banded or placed in stillages.
	

	public access.
	1.
	Lift above doorways to be completely boarded
	

	
	2.
	Diversions, barriers and warning notices by griffiths
	

	
	
	
	

	
	4.
	Cordon off the work area directly below .
	

	Working at Heights
	1.
	Only experienced Scaffolders to be used.
	X

	
	2.
	Area around scaffold to be securely barriered of.
	

	
	3.
	Safety notices to be posted.
	

	
	4.
	Adequate PPE to be used.
	

	
	5.
	All scaffolders to work within SG4.10 guidance.
	

	Overhead Cables
	1.
	Area below overhead cables to be barriered of.
	  

	
	2.
	No vehicles or cranes allowed to load or unload within these areas, without permission of Site Supervisor.
	

	
	3.
	Supervisor to inform Scaffolders of danger, (i.e Tool Box Talk).
	

	
	
	
	

	
	
	
	

	Collapse of Scaffold
	1
	Scaffold to be erected by qualified scaffolders in compliance with TG20.13 and design
	X

	
	2
	Client to make his operatives aware of scaffold loadings.
	

	
	3
	Scaffold structure only to be altered by qualified scaffolder.
	

	
	
	
	

	Falling Objects
	1.
	Good housekeeping to be observed at all times.
	

	
	2.
	Warning Signs to be posted.
	

	
	3.
	All surplus materials to be removed.
	

	
	4.
	All passage or gangways to be kept clear.
	

	
	5.
	Barriers to be erected directly below work area if public access area.
	

	
	6.
	Whilst using power tools from the roof they must be securely restrained
	

	
	7.
	Protection erected over doorways
	

	
	
	
	

	Housekeeping
	1.
	Good housekeeping to be observed at all times.
	X

	
	2.
	Scaffolder to ensure that all surpluses on unused material are cleared away and securely stored.
	

	Manual Handling
	1.
	Where possible mechanical device’s to be used. 
	X

	
	2.
	If the load is for heavy or unwieldy and cannot be moved by mechanical means, seek assistance.
	

	Site Vehicles
	1.
	Site vehicles to keep to the recognised roadways or access routes and be vigilant of other road users and pedestrians.
	X

	
	2.
	Audible or visual alarms to be fitted and used at all times.
	

	
	3.
	Only authorised and trained personnel allowed to drive Site vehicles.
	

	Slips, Trips & Falls
	1.
	Good housekeeping to be observed at all times.
	X

	
	2.
	Doorways, passageways to be kept clear.
	

	
	3.
	All tools or equipment to be removed when not in use or required.
	

	Noise
	1.
	All noisy work areas to be clearly sign posted.
	  

	
	2.
	Ear defenders to be used in sign posted areas.
	

	Electricity
	1.
	All tools or equipment to be of 110 volt and fitted with a residual Cut of Device (RCD).
	 

	Ground Conditions
	1.
	Ensure that scaffold is erected on ground and level base.
	

	
	2.
	Client to provide a firm, sound and level base.
	

	
	3.
	Supervisor/Scaffolder to inspect and accept base prior to work start.
	

	Fragile  Roofs
	1
	Roof ladders to be used
	  

	
	2
	Crawl boards 
	

	
	3
	Sole boards fixed to saddles
	

	
	4
	All Labour to Wear Safety Harness’s all TIMES
	

	
	
	
	

	Cutting of Tubes
	1 
	Encourage the use of manual tube cutting device.
	

	
	2
	Only operatives fully trained in the use of mechanical abrasive wheels to use this device.
	

	
	3
	Eye protection and all other PPE to be worn.
	

	
	
	
	

	Working over Water
	1.
	Self-inflating floatation jacket to be worn by scaffolders.
	 X 

	
	2.
	Adhere to method and be attached to retrievable inertia block .
	

	
	
	
	 

	
	
	
	X

	Working from MEWP
	1.
	As attached separate RA.
	

	
	2.
	Appropriate ppe to be worn
	


	Engineer Consultation:
	Yes
	X
	No
	 
	Optima designs

	Method Statement:
	Yes
	 X
	No
	
	

	Date Assessed:
	27th March 2019
	Assessed by: Mr P Morgan

	Date Review:
	 As Required
	Signature:

	Additional equipment to PPE made available to Implement key risk controls.
	1. Floatation jacket

	
	2. Retrievable inertia block 

	
	


	I/We acknowledge that I/We have read, understood and have passed on to others the details on this Risk Assessment and will comply with the control measures stated.

	Signed:
	Name (Print):
	Date:
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