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Authorisation

Environmental Protection Act 1990

Section 37

Notice of Modification of Waste Management Licence

Authorisation Number:

EAWML34024
To: The Company Secretary

Of: Davies Bros (Waste) Ltd, Tythegston Landfill Site, Tythegston, Bridgend, CF32 0NE

Licensed facility:

Davies Bros (Waste) Ltd, Tythegston Landfill Site, Tythegston, Bridgend, CF32 0NE

WHEREAS on the 10 November 1992 the Ogwr Borough Council issued a waste disposal licence in pursuance of its powers under Part II of the Environmental Protection Act 1990 for the above named facility to you.

AND WHEREAS on the 1 April 1996 the powers and duties of all waste regulation authorities in England and Wales transferred to the Environment Agency (“the Agency”) by virtue of section 2 of the Environment Act 1995

AND WHEREAS on 24 June 1996, 14 May 1999, 30 May 2000 and 17 July 2006 the Environment Agency modified the licence.
NOTICE IS HEREBY GIVEN that the Agency modifies the conditions of the said licence in accordance with Section 37(1)(b) of the Environmental Protection Act 1990 and as set out in the Schedule attached to this notice.

This modification shall take effect on 17 July 2006 at 00.01 hours.

Signed



Mark Sabine – Environment Management Team Leader 

Date of signing



Schedule – Conditions Relating To This Modification

1.1 Specified land

1.1.1 The area of land to which this licence relates is that edged in red on Plan DBW/TLS/13 dated November 1993 attached to this licence.  No change shall be permitted to the area of land specified by this licence.

1.2 Specified waste management operations

1.2.1 No waste management operations shall be authorised by this licence unless specified in and undertaken in accordance with the limitations in the following table:

Table 1.1   Specified waste management operations

Specified Waste Management Operation
Permitted Waste Types which may be subject to the Specified Operation
Limits on  Specified Waste Management  Operations

Landfilling
Only approved waste to be used for restoration purposes.
The red lined area on plan DBW/TLS/13 shall be restored with suitable material outlined in the site restoration plan.

Flaring of landfill gas generated from the site
Gas produced from the in-situ waste at the site only


Leachate storage as part of the landfill operation.
Leachate produced from the in-situ waste at the site only.


1.3 Exempt waste management activities

1.3.1 Where wastes are being brought onto the site for waste management activities which are exempt from licensing under the Waste Management Licensing Regulations 1994 or any statutory provisions amending or replacing them, then those wastes shall be kept clearly segregated and identified from wastes which are being kept on the site for the specified waste management operations under these licence conditions.

1.4 Permitted waste types and quantities:

1.4.1 No wastes other than those which are categorised and permitted below shall be accepted at the site.  The total quantity of waste accepted at the landfill shall not exceed 4,999 tonnes per annum. 

Table 1.4   Waste Categories

Inert Wastes (for restoration purposes only)

Permitted

1.5 Exclusion of waste types with specified hazard characteristics

1.5.1 Hazardous wastes, wastes that are liquid or sludge, pressurised gasses in containers, soil containing invasive plant material, or wastes that consist solely or mainly of finely divided metal or of dusts, powders or loose fibres shall not be accepted at the site.  
1.6 Minimum staffing and supervision

1.6.1 Whenever the landfill is open to receive waste for restoration purposes it shall be staffed by an appropriate number of staff at least one of whom should be fully conversant with the requirements of the licence and the working plan regarding:

a waste acceptance and control procedures;

b operational controls and environmental monitoring;

c maintenance;

d record-keeping;

e emergency action plans;

f notifications to the Agency.
1.7 Availability of licence and working plan

1.7.1 A copy of this licence and the working plan shall be kept available on site for reference when required by all site staff carrying out work under the requirements of the licence.

1.8 Understanding of licence and working plan

1.8.1 All site staff shall be, or shall work under the direct supervision of a member of staff who is, fully conversant with those aspects of the licence conditions and working plan, which are relevant to their specific duties.

1.9 Changes In Technically Competent Persons

1.9.1 Any changes in the technically competent management of the site and the name of any incoming person together with evidence that such person has the required technical competence shall be submitted to the Agency in writing within 5 working days of the change in management.

1.10 Notification of relevant convictions

1.10.1 In the event of the Licence Holder and/or any relevant person being convicted of any relevant offence (as defined in Regulation 3 of the Waste Management Licensing Regulations 1994 or any amendment to the aforementioned Regulation) and which is in addition to any already notified to the Agency, then full details shall be provided to the Agency within 14 days of conviction, whether or not the conviction is subsequently appealed.  Such details shall include, in respect of each relevant person (as defined in section 74(7) of the Environmental Protection Act 1990 or any subsequent amendments to that section), the nature of the offence, the place and date of conviction, any sentence, and any fine or other penalty imposed.

1.10.2 In the event that the Licence Holder lodges an appeal against any such conviction, the Licence Holder shall notify the Agency of this within 14 days of the lodging.  The Licence Holder shall notify the Agency of the results of that appeal, within 14 days of the appeal being decided.

1.11 Amendments to the working plan and supporting information

1.11.1 The Licence Holder shall give the Agency prior notice in writing of any proposed change to those sections of the working plan which are specified in Table 1.12 of this waste management licence, and to any appendices, drawings and figures which are referenced in those sections.

 [Note for Agency users (to be deleted from finalised condition):

The table must be Quality Assured prior to issue so as to ensure that all relevant and necessary sections are specified.

The table must include all sections of the working plan which are referenced within the other conditions, except where it is considered that the potential effects on environmental risk of changing the risk management systems specified in the working plan are such that they can be adequately regulated through the more relaxed control of prior notification.  The table may include relevant supporting information such as operating procedures, Construction Quality Assurance Plans, etc, as necessary and appropriate to ensuring that the objectives of the relevant licence conditions will be met.  This is a key set of requirements and should be considered carefully by the officer drafting the conditions.

Referencing of a working plan section, and its listing in the table, implies approval by the Agency of those sections of the working plan as necessary and enforceable standards under the Licence conditions.  This means that those sections must meet the same criteria as conditions under WMP4; i.e. they must provide the necessary information, they must be comprehensive, they must be clear and unambiguous to the users (including the Agency), and they must be sufficient to enable site staff to understand the relevant requirements and to comply with the relevant conditions.  If any section does not meet these criteria, then it should not be referenced, and the default requirements should be specified.] 

Table 1.12 Sections of working plan requiring prior consent for amendments

Number and Heading of Working Plan Sections and Appendices


Sections, Subsections and Appendices requiring Prior Consent for Amendments

Section 1.  General Considerations
All

Section 2.  Site Engineering
All

Section 3.  Site Infrastructure
All

Section 4.  Site Operations
All

Section 5.  Pollution Control, Monitoring & Reporting
All

Section 6.  Amenity Management and Monitoring
All

Section 7.  Site Records
All

1.11.2 Supporting information which is referenced in any section of the working plan shall be deemed to be part of that section if the reference is to a specific dated version of the information, and amendments to the referenced information shall be subject to the same requirements as the specified section of the working plan under the other conditions of this licence.

1.11.3 Supporting information which is referenced in any section of the working plan shall be deemed to be separate from that section if the reference is to the title and other identifier, but not to a specific dated version and amendments to the referenced information shall be subject to the same requirement to give prior written notice to the Agency as specified in 1.12.2.

1.12 Notification of Change of Operator’s or Holder’s details

1.12.1 The following information shall be notified in writing within 5 working days to the Agency:

a any change in the Licence Holder’s trading name, registered name or registered office address; 

b any steps taken with a view to the Licence Holder going into administration, entering into a company voluntary arrangement or being wound up;

c any change in the operator’s trading name, registered name or registered office address (if different from the Licence Holder).
1.13 Notifications and Submissions to the Agency

1.13.1 Except where otherwise specified, all notifications and submissions to the Agency under the requirements of these licence conditions:

a shall be made in writing to the address specified by the Agency in writing;

b shall quote the licence reference number and the name of the Licence Holder.

2 Site engineering for pollution prevention 

2.1 Engineering surveys

2.1.1 Engineering surveys shall be carried out as follows:

a On the commencement of any permanent engineering works carried out to meet the requirements of these licence conditions, to establish the levels and co-ordinates of the base of the works for validation and recording purposes.

b On the completion of those permanent engineering works carried out to meet the requirements of these licence conditions, to establish the levels and co-ordinates of the completed works for validation and recording purposes.  

c Annually to determine the following measurements:

i Remaining air space in cubic metres

ii Total air space used since last survey in cubic metres 

iii Contours of site showing deformation and settlement since last survey, 




2.1.2 The results of any such surveys shall be submitted to the Agency in writing within one calendar month of the survey being carried out and shall be to the following standards of accuracy;.

a measured in m AOD accurate to 0.01 metre;

b surveyed on a 10m grid accurate to 0.01m on National Grid co-ordinates

2.2 Construction quality assurance plans (CQA) and method statements

2.2.1 CQAPs shall be provided which detail the quality assurance and validation process for any new developments in engineering systems at the site. The CQAP should cover all permanent elements or fixed elements of the engineering and construction.  The CQAPs shall be agreed in writing with the Agency prior to any new engineering works being undertaken.

2.2.2 The CQAPs and method statements required by conditions of this licence must be drafted by competent and suitably qualified engineer(s) who shall also prepare all technical (and, where relevant, geotechnical) reports and provide validation of the specified engineering works. The detail of the qualifications and experience of the engineer(s) shall be submitted to by the Agency in writing prior to the submission of the CQAPs.

2.2.3 CQAPs shall be supported by detailed method statements, which shall be submitted to the Agency for inspection as required throughout the development. Minor changes to the agreed method statements may be made on site during the development, providing that all such changes are detailed and justified in the validation report.  The CQAP should be agreed in writing with the Agency prior to any new engineering works being undertaken

2.3 Leachate monitoring  system

2.3.1 Full details of the leachate monitoring system shall be submitted to the Agency by the 26th August 2006. This should facilitate the representative sampling of leachates generated at the landfill, in accordance with current legislation and guidelines.  The report should meet the following criteria for content and quality: 

Operating procedures:

2.3.2 Operating procedures should be submitted to the Agency to provide details on how the leachate monitoring system will be operated and maintained.  These procedures should be submitted by 26th August 2006.
Maintenance procedures:

2.3.3 Details of how the leachate monitoring system will be maintained.  This will include a maintenance programme or schedule, giving frequencies and subjects of inspection, with procedures, responsibilities, and actions and deadlines for repair or replacement in the event of failed, defective or damaged components. References to schedules should be specific. 

2.3.4 Engineering Records:

2.3.5 The design, construction, supervision/testing/validation, operation, and maintenance and repair of the system must be fully documented and recorded.  The following information should be provided:

a Format and content of records;

b Quality assurance of records.

In addition, the report should specify where the records will be kept and the data security measures.

2.3.6 Construction of the leachate monitoring system shall be supervised by competent and suitably qualified engineers  (the QA Engineer) who shall provide a report detailing compliance with the CQAP. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing.

2.3.7 The licence holder shall submit a Construction Quality Assurance Validation Report to the Agency following the completion of each phase of the leachate management system. The report shall provide validation by the QA Engineer that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification.

2.4 Leachate Management System

2.4.1 Full details of the leachate management system shall be submitted to the Agency by the 26th August 2006.  This should detail how the system will minimise, and remediate high level leachate breakouts at the site in order to prevent pollution of the environment, harm to human health or serious detriment to amenity, in accordance with current legislation and guidelines.  
2.5 Surface water management system 

2.5.1 Within 12 months from the date of issue of this modification the landfill shall be provided with a surface water management system in order to;

a segregate surface water runoff which is uncontaminated from surface water runoff potentially contaminated by contact with waste;

b prevent uncontrolled egress of surface water from the site;

c prevent the uncontrolled ingress of water to the site; and

d prevent surface water damage to the structure or integrity of the final cap or other engineered pollution prevention works.

2.5.2 By 26th August 2006 the Licence Holder shall submit to the Agency a written report detailing the design, current extent and planned implementation of a surface water management system for the landfill to fulfill the above objectives

2.5.3 The report should meet the following criteria for content and quality:

Design

2.5.4 A technically justified design must be provided for the system, this should include drawings and/or plans to appropriate scales and should provide the design details specified under this sub-heading.

2.5.5 The design of the relevant system will use information from appropriate risk assessments to indicate the design details required.  The design will technical specifications for all materials used as well as scale drawing(s) of the proposed installations.

2.5.6 Where the licence holder proposes to fully develop the detailed design on a phased basis, an outline design for the system must be provided as a minimum, in sufficient detail to enable the design to be assessed by the Agency.

2.5.7 Detailed design drawings and specifications should be included in or specifically referenced as part of the report except where they may reasonably be expected to require ongoing development in response to operational conditions and the design is being carried out by a competent and suitably qualified engineer(s) under a detailed Construction Quality Assurance Plan (see condition 2.2 above).

Construction:

2.5.8 A construction methodology which describes how any additional works will be undertaken.

2.5.9  Detailed method statements may be generally referenced in support of, rather than as part of, the relevant section of the report, where it is reasonable to expect it to require ongoing development in response to operational conditions and the work is being carried out under the full time supervision of competent and suitably qualified engineer(s) under a detailed Construction Quality Assurance Plan (see condition 2.2 above).

Construction programme:

2.5.10 A construction programme must be provided for any additional works, which details the time frame for the works, including any proposed phased development

Operating procedures:

2.5.11 Details of how the engineering works will be operated and maintained.

Maintenance procedures:

2.5.12 Details of how the engineering works will be maintained.  This will include a maintenance programme or schedule, giving frequencies and subjects of inspection, with procedures, responsibilities, and actions and deadlines for repair or replacement in the event of failed, defective or damaged components. References to schedules should be specific.

Engineering Records:

2.5.13 The design, construction, supervision/testing/validation, operation, and maintenance and repair of the system must be fully documented and recorded.  The following information should be provided:

a Format and content of records;

b Quality assurance of records.

In addition, the report should specify where the records will be kept and the data security measures.

2.5.14 Construction of the surface water management system shall be supervised by competent and suitably qualified engineers who shall provide a report detailing compliance with the CQAP. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing..

2.5.15 The licence holder shall submit a Construction Quality Assurance Validation Report to the Agency following the completion of each phase of the surface water management system. The report shall provide validation by the QA Engineer that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification.

2.6 Landfill gas management

2.6.1 The landfill shall be provided with a gas management system in order to prevent pollution of the environment and harm to human health by emissions of landfill gas.

2.6.2 The gas management system shall include;

a 
Landfill gas collection, extraction, treatment and disposal systems  which should:

i have sufficient capacity to handle all landfill gas emissions from the landfill;

ii prevent the uncontrolled release of landfill gas from the waste mass to atmosphere;

iii prevent the migration of  landfill gas beyond the site boundary above specified trigger concentrations;

iv enable landfill gas to be collected for  treatment and/or disposal (via flaring or other controlled release or use as a supplementary fuel);

v withstand physical damage from the loading imposed by the waste, and any compaction operations working over the system;

vi be resistant to chemical attack in the landfill internal environment;

vii avoid damage to the engineered containment which may be caused through the installation or loading of the landfill gas management system;

viii be able to function effectively;

ix be capable of being inspected, tested, maintained and, where necessary, repaired or replaced.

b 
Landfill gas monitoring points which should:

i permit at any time an accurate determination of landfill gas quality at each monitoring point to be measured and recorded;

ii enable gas flow rates and differential pressure trends to be measured at each monitoring point when required;

iii enable representative samples of the landfill gas to be taken for further analysis when required from each monitoring point;

iv withstand physical damage and chemical attack in the landfill environment;

v be secure to prevent unauthorised access and vandalism, and entry of foreign matter; and


vi provide not less than 4 landfill gas monitoring points within the landfill, and not less than 2 landfill gas monitoring points per hectare of the landfill area.

2.6.3 By 31st August 2006 the Licence Holder shall submit to the Agency a written report detailing the design, current extent and planned implementation of a landfill gas management system to fulfil the obligations imposed by condition 2.6.1. The report should be prepared in accordance with LFTGN03 “Guidance on the Management of Landfill Gas” and meet the following criteria for content and quality:

Scope and Development

2.6.4 This section of the report should cover the landfill gas management system and its phasing, including:

a 
Landfill gas collection and extraction systems; i.e. engineered means by which landfill gas is collected and removed;

b Landfill gas monitoring systems; i.e. the engineered landfill gas monitoring points, for monitoring specified parameters of landfill gas within the waste mass (the monitoring programme requirements are covered by Section 5 of this licence);

c Landfill gas treatment and disposal systems; i.e. the engineered means by which landfill gas will be treated and disposed of (including landfill gas flaring and use as an energy source).

Contents:

2.6.5 This section of the report shall describe the design and of the works, including all proposed timescales, necessary engineering plans and drawings, documentation, procedures and technical standards, and supported by the risk assessment and other relevant scientific evidence and technical calculations.

a The design description should include details of the following, as appropriate:

b Landfill gas collection and extraction system; which may include:  landfill gas barriers (other than those specified in the engineered landfill containment system); landfill gas collection pipes; protection systems for landfill gas collection pipes; pumping/storage  systems;

c Landfill gas treatment/disposal systems within the licensed area; which may include: landfill gas flaring; landfill gas power units; alternative treatment and control systems, e.g. methane oxidation.

d Site engineered systems for monitoring landfill gas within the waste body:  locations and designs.

e Landfill gas treatment/disposal systems within the licensed area; e.g. landfill gas flaring systems; energy generation systems.

Operating procedures:

2.6.6 Details of how the engineering works will be operated and maintained.

Maintenance procedures:

2.6.7 Details of how the engineering works will be maintained.  This will include a maintenance programme or schedule, giving frequencies and subjects of inspection, with procedures, responsibilities, and actions and deadlines for repair or replacement in the event of failed, defective or damaged components. References to schedules should be specific.

Engineering Records:

2.6.8 The design, construction, supervision/testing/validation, operation, and maintenance and repair of the system must be fully documented and recorded.  The following information should be provided:

a Format and content of records;

b Quality assurance of records.

In addition, the report should specify where the records will be kept and the data security measures.

2.6.9 Construction of the landfill gas management system shall be supervised by competent and suitably qualified engineers. An independent third party engineer shall provide full time independent third part quality assurance of the works. and provide a report detailing compliance with the CQAP. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing. Full records shall be kept and made available on request for each element of the works.

2.6.10 The licence holder shall  submit a Construction Quality Assurance Validation Report to the Agency following the completion of each phase of the gas management system. The report shall provide validation by the QA Engineer that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification.

2.6.11 The gas management systems at the site shall be inspected daily. Any damage, mechanical malfunction, or extraneous material likely to impair its effectiveness shall be rectified immediately.

2.7 Restoration scheme

2.7.1 Once final waste levels in each phase have been reached a capping layer shall be constructed consisting of a minimum of 1m thickness of clay or other low permeability material emplaced in layers to achieve a permeability to water of not greater than 1.0 x 10ADVANCE \u3-9ADVANCE \d3 metres/second.  This cap shall be protected by covering with sub-soil and shall be topsoiled and planted during the next planting season.  Any planting shall only be permitted where the roots will not damage the integrity of the cap.

2.7.2 By 26th August 2006 the Licence Holder shall provide to the Agency a written report detailing the proposals for the installation of the engineered final cap and final landform at the site.  The report should provide the confidence that the engineered final cap is fit for purpose and will be designed, constructed and maintained to meet the following standards:

a prevent outside contact with the waste body;

b prevent uncontrolled surface water infiltration into the waste mass and prevent surface water pooling on the site;

c prevent uncontrolled emission of landfill gas to atmosphere from the waste mass;

d prevent damage from overlying materials or installations to the engineered leachate and landfill gas systems.

The report should meet the following criteria for content and quality:

Design:

2.7.3 A technically justified design must be provided for the system, this should include details of the final cap specifications, including design and dimensions, materials specifications; installation methods, maintenance provisions, and measures provided to protect the cap against damage and deterioration until completion.

2.7.4 Where the licence holder proposes to fully develop the detailed design on a phased basis, an outline design for the system must be provided as a minimum, in sufficient detail to enable the design to be assessed by the Agency.

2.7.5 Detailed design drawings and specifications should be included in or specifically referenced as part of the report except where they may reasonably be expected to require ongoing development in response to operational conditions and the design is being carried out by a competent and suitably qualified engineer(s) under a detailed Construction Quality Assurance Plan (see condition 2.2 above).

Construction:

2.7.6 A construction methodology, which describes how the works will be undertaken.

2.7.7 Detailed method statements may be generally referenced in support of, rather than as part of, the relevant section of the report, where it is reasonable to expect it to require ongoing development in response to operational conditions and the work is being carried out under the full time supervision of competent and suitably qualified engineer(s) under a detailed Construction Quality Assurance Plan (see below).

Construction programme:

2.7.8 A construction programme must be provided, which details the time frame for the works, including any proposed phased development

Construction Quality Assurance Plan (CQAP):

2.7.9 A CQAP for any new developments of the system must be provided which details the assurance and validation process for that system. The CQAP should be agreed in writing with the Agency prior to any new engineering works being undertaken.

2.7.10 The CQAP should cover all permanent elements or fixed elements of the engineering and construction.  The CQAP should be supported by detailed method statements.  

 Maintenance procedures:

2.7.11 Details of how the engineering works will be maintained.  This will include a maintenance programme or schedule, giving frequencies and subjects of inspection, with procedures, responsibilities, and actions and deadlines for repair or replacement in the event of failed, defective or damaged components. References to schedules should be specific.

Engineering Records:

2.7.12 The design, construction, supervision/testing/validation, operation, and maintenance and repair of the system must be fully documented and recorded.  The following information should be provided:

a Format and content of records;

b Quality assurance of records.

In addition, the report should specify where the records will be kept and the data security measures.

2.7.13 Construction of the cap shall be supervised by competent and suitably qualified engineers. .  An independent third party engineer shall provide full time independent third part quality assurance of all engineering works on site and provide a report detailing compliance with the CQAP. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing. Full records shall be kept and made available on request for each element of the capping works.

2.7.14 The licence holder shall submit a Construction Quality Assurance Validation Report to the Agency following the completion of each phase of the capping works. The report shall provide validation by the QA Engineer that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification.

2.7.15 The licence holder shall ensure that sufficient soils are available for the protection layer before the commencement of each phase of the capping works.

2.7.16 Unless specifically agreed in writing with the Agency, levels of contaminants within the soil utilised in the capping protection layer shall not exceed the Lower Threshold nor the Leachate Quality Threshold as they are laid out in the document ‘Interim Guidance on the Disposal of Contaminated Soils’ 2nd Edition (01/05/97) published by the Environment Agency.

2.7.17 The Agency shall be notified in advance of any instances of emplacement of the soil protection layer.   This notification shall state the proposed dates for these works.

2.7.18 On the same day and prior to the emplacement of the protective soil layer over any areas of the engineered cap, those areas of compacted clay proposed to be covered shall be inspected by an independent CQA engineer for damage.   Where the inspection reveals that deterioration of the clay has occurred appropriate measures shall be taken to remediate  the affected  area.  Any such remedial works shall be supervised by the independent CQA engineer .  The results of all inspections and remedial works shall be documented by the independent CQA engineer and forwarded to the Agency.

2.7.19 The licence holder shall ensure that surface water contaminated with suspended solids arising from any earthworks at the site is treated so as to not cause pollution of the environment. NB  Any discharge to controlled waters may require a Discharge Consent issued by the Environment Agency.

2.7.20 The integrity of the engineered cap shall be maintained during the subsistence of this licence.

2.8 Excavation or movement of previously emplaced waste

2.8.1 Prior to any excavation or movement of previously emplaced waste at the site an assessment shall be made of the potential for the disturbance of asbestos deposits and a written report of the assessment provided to the Agency. 

3 Site infrastructure

3.1 Provision of site identification  board

3.1.1 An identification board must be provided at or near the site entrance

3.1.2 The identification board shall be inspected once each working day.  In the event of damage or defect, the board shall be repaired or replaced within 3 working days.

3.1.3 The board shall be easily readable from outside the site entrance in daylight hours, and shall display the following information:

a Site name and address;

b Licence Holder name ; (Company name, not individual name unless justified as necessary)
c Operator  name ; (Company name, not individual name unless justified as necessary)
d Licence number;

e Emergency contact name and telephone number; (for security reasons, personal names and home phone numbers should not be used, except where no alternative is practicable).
f Statement that the site is licensed by the Environment Agency.
g Agency national number: 08708 506506 and 0800 807060; or as subsequently notified in writing by the Agency. 

h Days and hours site is open to receive waste.

3.2 Site security

3.2.1 Site security systems shall be provided and maintained at all times during the subsistence of this licence.  These shall be installed, operated and maintained to prevent access by humans and livestock which is not authorised either by the Licence Holder or under legal powers of entry.

3.2.2 The site security shall be fully inspected at the commencement of each working day, and recorded in the site diary.  Any defects or damage shall be made secure by the end of the working day, and shall be repaired within 10 working days of the damage being detected.  All repairs shall be recorded in the site diary.

3.2.3 The site shall be kept closed and secure at all times when unattended.

3.2.4 By 31st July 2006 the Licence Holder shall provide to the Agency an updated section for incorporation into the working plan for the site detailing the site security provisions for the landfill site. This should include; 

a Description of site security provisions at or within the licensed site boundary and at site access points, detailing:

b Type of security and timetable of provision:

c Design standards for physical security, detailing design and specification (scale plans and drawings), including access.

d Operational standards for security, including operational and out-of -hours provisions.

e Maintenance and repair schedules.

NB.  This report may rely on referenced supporting documents which the applicant may wish to keep confidential for security reasons.
4 Site operations

4.1 Control of mud and debris

4.1.1 Measures shall be taken on-site to prevent mud or debris from the site operations being lost from control and deposited on the road outside the site boundary. 

4.1.2 By 31st July 2006 the Licence Holder shall provide the Agency with an updated section of the working plan describing the procedures and equipment that will be employed to satisfy this requirement.  

4.1.3 In the event that mud or debris from the site operations is lost from control and deposited on the road outside the site boundary immediate steps shall be taken to collect and dispose of the offending material.  This shall include the use of a road sweeper where required.  

4.2 Potentially polluting leaks and spillages 

4.2.1 All vehicles used on the site, which are under the operator’s control, and all plant and all equipment used on the site in connection with waste management operations, shall be operated and maintained so as to prevent potentially polluting leaks and spillages of wastes. 

4.2.2 All spillages shall be dealt with immediately to clear or alleviate the effect of the spillage, and to prevent pollution of the environment and to ensure public safety.  Adequate quantities of sand/absorbent material shall be available at the site for this purpose.  All spillage events shall be logged in the site diary and a record kept of the actions taken.

4.2.3 All materials used to absorb any spillage and any removable contaminated material shall be collected and placed in a secure container.  This material shall be removed for disposal to a suitably licensed facility within 72 hours of the occurrence and logged accordingly in the site diary.

4.3 Fires on site

4.3.1 By 31st July 2006 the Licence Holder shall update their working plan to include site specific information describing the measures that will be taken to prevent and control fire at the site.  The information and procedures shall meet the following for content and quality; 

a The standard of fire prevention and control measures provided should meet the substantive risk posed by the site due to the waste types or permitted activities. These should be provided in accordance with the relevant requirements under Health and Safety legislation and of the local Fire Authority.

b should not include the fire prevention and control provisions made in accordance with the Health & Safety at Work, etc. Act 1974 or with the requirements of the local Fire Authority, but should reference them generally.

c detail the necessary actions to be taken to prevent or minimise pollution of the environment in the event of a fire in a Fire Action Plan, which may be specifically referenced and should include appropriate details of: 

i Fire control and elimination procedures;

ii Fire fighting equipment and materials;

iii Training;

iv Storage and disposal of residues;

v Recording and reporting/notification procedures.
4.3.2 No waste shall be burned on the site other than through a specified waste management operation authorised under the other conditions of this licence. 

5 Pollution control, monitoring & reporting 

5.1 Quality assurance of monitoring and sampling results

5.1.1 Prior to undertaking monitoring or sampling at the site the licence holder shall provide to the Agency a written monitoring and sampling quality assurance plan in respect of that monitoring or sampling.  The plan should include

a the monitoring and sampling methodologies that will be used, including documented quality assurance procedures and documentation. 

b the training and qualifications that will be provided/required for  monitoring and sampling personnel;

c the analytical methodologies that will be used, including documented quality assurance procedures and documentation;

d the identity of the laboratories performing the specified analyses, with their relevant competence/accreditation 

5.1.2 Monitoring and sampling of the site shall be undertaken in accordance with the quality assurance plan required under condition 5.1.1.

5.1.3 Any proposed changes to the details provided in Monitoring Quality Assurance Plans shall be agreed in writing with the Agency prior to the changes being implemented.

5.1.4 All equipment used for monitoring and sampling shall be properly maintained and calibrated to the manufacturers recommendations and specifications.   Copies of calibration certificates for such equipment shall be made available to Agency on request.

5.1.5 All analysis of  leachate, surface water and ground water shall be at a UKAS accredited laboratory

5.2 Monitoring & sampling programmes

5.2.1 All monitoring and sampling programmes required by conditions of this section should meet the following criteria for content and quality:

Monitoring and sampling points:

5.2.2 The locations and identities of monitoring points should be given on a plan of the site and its surroundings, drawn to an appropriate scale.  These should be cross-referenced to relevant engineering details.

Determinands that will be monitored:

5.2.3 The determinands that will be monitored by measurement at the monitoring point, and/or by sampling and analysis, should be tabulated for each monitoring/sampling point, against minimum frequencies for monitoring/sampling, specified units and accuracies, and specified trigger levels based on an appropriate risk assessment at which action will be taken.   Where the proposed determinands/frequencies differ from those recommended in Waste Management Paper Number 4, 27, or 26a the licence holder shall supply a scientific justification for his decision supported by risk assessment. 

Records of monitoring and sampling:

5.2.4 The format in which the results of the specified environmental monitoring and sampling programme will be documented and recorded  

Monitoring action plans

5.2.5 A monitoring action plan should be provided which will be designed and operated to ensure that any results of monitoring or sampling that exceed the specified trigger levels for the determinands being monitored are acted upon immediately to:

a prevent hazard to human life, property  or the environment outside the site boundary;

b control and minimise any immediate risks of pollution of the environment;

c ensure the immediate initiation of necessary investigations and management actions to identify, mitigate and remediate the causes of the exceedance.

d prevent unauthorised discharge to controlled waters

5.2.6 The action plan should be effective, and should include training and, where necessary, periodic tests.

5.3 LANDFILL GAS MONITORING 
Landfill gas risk assessment

5.3.1 By 31st August 2006 the Licence Holder shall submit to the Agency a written landfill gas risk assessment for the site. The assessment should include: 

a a detailed desk top study and preliminary identification of landfill gas hazards, pathways and targets;

b a preliminary site investigation with factual and interpretative reports;

c a main site investigation with factual and interpretative reports incorporating a qualitative and quantitative landfill gas risk assessment:

d a geological investigation should be carried out to establish the nature of the surrounding geology and in particular the presence of any permeable strata

Engineered gas monitoring 

5.3.2 The site shall be provided with engineered landfill gas monitoring systems to meet the following objectives; 

a 
permit at any time an accurate and reliable determination of landfill gas quality at each monitoring point external to the waste mass to be measured and recorded;

b enable gas flow rates and differential pressure trends to be measured at each monitoring point when required;

c enable representative samples of the landfill gas to be taken for further analysis when required from each monitoring point;

d withstand physical damage and chemical attack in the subsurface environment; and

e be secure to prevent unauthorised access and entry of foreign matter.

f enable gas migration from the waste mass to be characterised

5.3.3 By 31st August 2006 the Licence Holder shall submit to the Agency a written report detailing the current extent and where appropriate proposed extensions to the engineered systems provided at the site to satisfy the requirements of condition 5.3.2.  This report shall include for content:

a 
Design

i A technically justified design must be provided for the system, this should include drawings and/or plans to appropriate scales and should provide the design details specified under this sub-heading.

ii The design of the relevant system will use information from appropriate risk assessments to indicate the design details required.  The design shall provide technical specifications for all materials used as well as scale drawing(s) of the proposed installations.

iii Where the licence holder proposes to fully develop the detailed design on a phased basis, an outline design for the system must be provided as a minimum, in sufficient detail to enable the design to be assessed by the Agency.

iv Detailed design drawings and specifications should be included in or specifically referenced as part of the report.  The exception to this requirement is where they may reasonably be expected to require ongoing development in response to operational conditions and the design is being carried out by a competent and suitably qualified engineer(s), under a detailed Construction Quality Assurance Plan (see condition 2.2).

v The design for the monitoring system should include specifications for the locations, spacing, depths, design and construction of boreholes. 

b 
Construction:

i A construction methodology which describes how any additional works will be undertaken.

ii  Detailed method statements may be generally referenced in support of, rather than as part of, the relevant section of the report, where it is reasonable to expect it to require ongoing development in response to operational conditions and the work is being carried out under the full time supervision of competent and suitably qualified engineer(s) under a detailed Construction Quality Assurance Plan (see condition 2.2).

c 
Construction programme:

i A construction programme must be provided for any additional works

d 
Operating procedures:

i Details of how the engineering works will be operated and maintained.

e 
Maintenance procedures:

i Details of how the engineering works will be maintained.  This will include a maintenance programme or schedule, giving frequencies and subjects of inspection, with procedures, responsibilities, and actions and deadlines for repair or replacement in the event of failed, defective or damaged components. References to schedules should be specific.

f 
Engineering Records:

i The design, construction, supervision/testing/validation, operation, and maintenance and repair of the system must be fully documented and recorded.  The following information should be provided:

· Format and content of records;

· Quality assurance of records.
ii In addition, the report should specify where the records will be kept and the data security measures.
5.3.4 Construction of the gas monitoring system shall be supervised by competent and suitably qualified engineers who shall provide a report detailing compliance with the Construction Quality Assurance Plan. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing by 31st August 2006.

5.3.5 The licence holder shall submit a Construction Quality Assurance Validation Report to the Agency by 31st August 2006. The report shall provide validation by the engineer (referred to in condition 5.3.4 above) that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification. 

5.3.6 All gas monitoring boreholes shall be fitted with a suitable device to enable representative gas sampling without air dilution and secured to prevent unauthorised access.  Access to the boreholes, for the Agency shall be maintained during working hours.
5.3.7 The installation of the gas monitoring and groundwater monitoring systems shall be deemed to be engineering works and be subject to condition 2.2.
5.3.8 All site buildings shall be monitored as follows:

a Any site buildings located within 25 metres of waste shall be monitored continuously of flammable gas and not less frequently than at monthly intervals for carbon dioxide.

b Every room in all site building within the licensed area but further than 25 metres from the boundary of waste, shall be monitored for the presence of flammable gas and carbon dioxide not less frequently than at monthly intervals.

c A written record shall be made of the monitoring of buildings. 

5.3.9 Annually a minimum of 2 gas samples shall be taken for gas chromatographic analysis from points agreed with the Agency.    The results of the analysis shall be recorded.

5.3.10 All gas monitoring points situated within the waste shall be monitored for flammable gas and oxygen not less frequently than at monthly intervals.  A written record shall be made of the following parameters:

a Date and time of monitoring

b Barometric pressure and weather conditions at the time of monitoring

c The identity of the monitoring personnel

d The levels of flammable gas and oxygen.

5.3.11 Gas monitoring boreholes external to the waste mass shall be monitored at weekly intervals and a written record shall be made of the following parameters;

a Date and time of monitoring

b Barometric pressure and weather conditions at the time of monitoring

c The date and time at which excess water was last removed from the borehole

d The identity of the monitoring personnel

e The level of the top and base of the borehole referenced to ordnance datum

f Borehole datum

g The levels of flammable gas, oxygen and carbon dioxide present in each       borehole.

5.3.12 Should the concentration of flammable gas from the landfill gas in any of the monitoring points around the perimeter of the site, exceed 1% by volume in air (20% of the lower explosive limit (L.E.L.) for methane), or the concentration of carbon dioxide from the landfill gas exceed 1.5% by volume, the licence holder shall take the following steps:-

a the matter shall be reported to the Agency immediately;

b  an assessment of the immediate risks to persons and property, based on the monitoring  results shall be submitted in a report  (The Preliminary Risk Assessment), to the Agency within 7 working days;

c a further study into the nature and source of the gas shall be undertaken. This study may include analyses of gas samples by gas chromatography, investigation by spike bar, investigation by boreholes or piezometers, desk studies and/or other investigations as considered necessary. Any survey shall pay particular attention to the land between affected areas and any structures, buildings or underground services within 250 metres.  The findings of this further study shall be submitted in a report (The Detailed Risk Assessment), to the Agency; and

d a programme of works supported by the Detailed Risk Assessment shall be devised to prevent gas migration and/or alleviate the risks to persons and/or property posed by any migrating gas. 

5.3.13 If the concentration of flammable gas in any room in any building within the licensed area exceeds 2,500 parts per million the licence holder shall notify the Agency  by telephone of facsimile transmission without undue delay and in any event within 24 hours, and confirm in writing within 72 hours.  The affected building shall be monitored and ventilated until it can be demonstrated that flammable gas concentration are stable below this level.

5.3.14 In the event of a concentration of flammable gas in excess of 1% by volume or a concentration of carbon dioxide in excess of 0.5% by volume being measured in any building or temporary accommodation within the licensed area, the affected building or temporary accommodation within the licensed area, the affected building or temporary accommodation shall be evacuated.  Effective measures shall be taken to reduce the levels of flammable gas and carbon dioxide before the affected building or temporary accommodation is reopened to personnel.

Water and leachate monitoring  

Conceptual hydrological and hydrogeological model

5.3.15 By 31st July 2006 the Licence Holder shall submit to the Agency a written assessment for the sites potential impacts on the quality of controlled waters. The hydrogeological model should be prepared in accordance with Agency guidance document “Hydrogeological Risk Assessment for landfills “ (LFTGN01).  The assessment should include:

a a detailed desk top study and preliminary identification of sources, pathways and receptors;

b a conceptual hydrological and hydrogeological model of the site and its surroundings based on all available site investigations.

Groundwater monitoring system
5.3.16 Construction of the groundwater monitoring system shall be supervised by competent and suitably qualified engineers who shall provide a report detailing compliance with the Construction Quality Assurance Plan. The detail of the qualifications and experience of the engineer(s) shall be submitted to the Agency in writing.

5.3.17 The licence holder shall submit a Construction Quality Assurance Validation Report to the Agency following the completion of each phase of installation of the groundwater monitoring system. The report shall provide validation by the engineer, referred to in condition 5.3.16 that all the works subject to CQA procedures have been carried out in accordance with the method statements, design and specification.

5.3.18 Following the installation of the groundwater monitoring system, all groundwater monitoring points shall be individually monitored, sampled and analysed for the following parameters; This monitoring should be completed by 31st June 2006.
a Water level groundwater only, pH, temperature, electrical conductivity, dissolved oxygen, BOD, COD, ammoniacal nitrogen, chlorides, sulphates, total alkalinity as CaCO3 at pH 4.5, oxidised, nitrogen, TOC, Na, K, Ca, Mg, Fe, Mn, Cd, Cr, Cu, Ni, Pb, Zn.

b Half of the groundwater samples taken for routine analysis shall be randomly selected and be subject of additional testing to allow for the calculation of ionic balance.  The results of the ionic balance calculations shall be recorded. If a deficiency in the balance is found in any of the groundwater samples greater than plus or minus 5 % the results shall be subject to further investigation including resampling where necessary.
5.3.19 Following the installation of the leachate monitoring system, all leachate monitoring points shall be individually monitored, sampled and analysed for the following parameters; This monitoring should be completed by the 31st June 2006.
a pH, temperature, electrical conductivity, dissolved oxygen, BOD, COD, ammoniacal nitrogen, chlorides, sulphates, total alkalinity as CaCO3 at pH 4.5, oxidised, nitrogen, TOC, Na, K, Ca, Mg, Fe, Mn, Cd, Cr, Cu, Ni, Pb, Zn.

b Half of the leachate samples shall taken for routine analysis shall be randomly selected and be subject of additional testing to allow for the calculation of ionic balance. The results of the ionic balance calculations shall be recorded. If a deficiency in the balance is found in any of the leachate samples greater than plus or minus 15% the results shall be subject to further investigation including resampling where necessary.

c A representative number of leachate samples shall be subject to analysis for List 1 substances.  The analytical techniques to be utilised in this analysis shall be as follows;

i GCMS scan for volatiles

ii GCMS scan for semi-volatiles;
iii Derivitised GCMS scan for semi-volatiles;
iv Extraction of organotin compounds;
v Reduction of mercury compounds; and
vi Solution of cadmium compounds.
5.4 Groundwater risk assessment 

5.4.1 By 31st July 2006 the licence holder shall submit to the Agency a completed qualitative and quantitative risk assessment for the sites potential impacts on the quality of controlled waters. The assessment shall include the following:-

a a detailed desk top study and preliminary identification of source, pathways and receptors.

b a phased site investigation with factual and interpretative reports;

c a conceptual hydrological and hydrogeological model of the site and its surroundings.

d any relevant site investigation and monitoring data already available and interpretation of that data;

e an examination of the hydrogeological conditions of the area in and around the site;

f an examination of the possible purifying powers of the soil and subsoil;

g an investigation to assess the actual and potential impact of discharges from the site in respect of Regulation 15 of the Waste Management Licensing Regulations 1994 (SI 1056) and Council Directive 80/68/EEC.

h an assessment of the risk of pollution and alteration of the quality of groundwater including the risk of harm to other aquatic systems and ecosystems and the likelihood of impeding exploitation of groundwater resources from any discharge, whether direct or indirect, of list I or list II substances.

i a completed risk assessment that identifies the potential impact of the site on controlled waters and identified receptors

5.4.2 The results of the investigation to assess the actual and potential impact of discharges from the site in respect of Regulation 15 of the Waste Management Licensing Regulations 1994 (SI 1056) and Council Directive 80/68/EEC shall include:

a recommendations of the essential technical precautions which must be taken, paying particular attention to the nature and concentration of the substances present in the matter being disposed of or tipped, the characteristics of the receiving environment and the proximity of the water catchment areas, in particular those for drinking, thermal and mineral water in order to;

b In the case where groundwater is considered to be permanently unsuitable for other uses, to ensure that no substance in list I can reach other aquatic ecosystems or harm other ecosystems, to ensure that the presence of any list I substance once discharged into the groundwater will not impede exploitation of ground resources and to prevent pollution of groundwater by list II substances; and

c In the case where groundwater is not considered to be permanently unsuitable for other uses, to prevent any discharges into groundwater of substances in list I and to prevent any pollution of groundwater by substances in list II.

5.5 Groundwater monitoring and sampling programme 

5.5.1 By the 26th August 2006 the Licence Holder shall submit to the Agency a written groundwater monitoring and sampling programme for the site. The purpose of this programme shall be to enable the assessment of the impact of the site on groundwater quality.  The programme shall include proposals for the monitoring of List I and List II substances as prescribed in the EC Groundwater Directive 80/68/EEC. This report should be prepared in accordance with Agency document “Guidance on Monitoring of Landfill Leachate, Groundwater, & Surface Waters” (LFTGN02).
5.5.2 The report shall be produced and justified using the risk assessment required by condition 5.4.1 and shall take account of the advice given in Waste Management Paper Number 4 and 26a. 

5.5.3 Every six months half of the groundwater samples taken for routine analysis shall be randomly selected and be subject of additional testing to allow for the calculation of ionic balance.  The results of the ionic balance calculations shall be recorded.  If a deficiency in the balance is found in any of the samples greater than plus or minus 5 % the Agency shall be notified and the results investigated by the licence holder.

5.6 Leachate monitoring 

5.6.1 At the same time as submission of the risk assessment required by condition 5.4.1 the Licence Holder shall submit to the Agency a written report proposing a site specific leachate monitoring programme for the site.  The purpose of this monitoring programme shall be to representatively characterise leachate distribution and leachate quality within the site.  This report should be prepared in accordance with Agency document “Guidance on Monitoring of Landfill Leachate, Groundwater, & Surface Waters” (LFTGN02).
5.6.2 The programme shall be produced utilising a risk assessment approach and shall take account of the advice given in Waste Management Paper Numbers 4 and 26A. The programme shall include proposals for the monitoring of List I and List II substances as prescribed in the EC Groundwater Directive 80/68/EEC.

5.7 Maintenance arrangements for engineered monitoring systems

5.7.1 All monitoring boreholes shall be checked bi-annually for depth.  Records of this monitoring and the depths of the boreholes shall be reported to the Agency in the Annual report required by condition 5.8.2.  In the event that the checking finds that depth has become unsuitable for monitoring and obtaining samples the Agency shall be informed and measures taken within 21 days to repair or replace the effected borehole.

5.7.2 All monitoring systems shall be inspected at least weekly.   If at anytime any element of the monitoring system becomes unserviceable for sampling, then it shall be made serviceable or replaced by agreement with the Agency within 4 weeks of becoming unserviceable.  The event shall be recorded in the site diary.

5.8 Monitoring records

5.8.1 Records shall be kept of all monitoring and sampling at the site.  The records should provide the following quality assured monitoring and sampling information:

a Determinands monitored/sampled;

b Specified details of measurements/samples to support analytical and QA requirements; e.g. dates, times, locations, other relevant parameters;

c Results of measurements/sample analyses, with error limits;

d Interpretation and review of results against specified trigger levels;

e Validation of accuracy and validity of results, by designated quality assurer.

5.8.2 On the 1st June each year, the licence holder shall collate all data relating to the site monitoring during the preceding 12 months. The collated data should be interpreted by a suitably qualified person with experience of leachate management and groundwater monitoring and copies of the interpretation, together with any recommendations made shall be forwarded to the Agency within two months of the end of the annual period to which it relates. The required data interpretation and recommendations shall address the following matters;

a the effectiveness of gas and leachate control;

b the quality of ground and surface waters and the general environmental impact of the facility;

c a review of all risk assessments undertaken in compliance with conditions of this licence; 

d a review of all site monitoring programmes;

e developing trends in gas quality and quantity

f developing trends in leachate and groundwater quality

6 Amenity management and reporting

6.1 Control and reporting of dusts, fibres and particulates

6.1.1 During periods of dry weather water sprays shall be utilised on site roads and, if necessary the restoration area, to prevent any nuisance from dust.  Visual monitoring should be undertaken to ensure that measures are provided to prevent and control releases of dusts beyond the site boundary.  Runoff from this operation shall be prevented form discharging to any controlled water in order to prevent pollution. Leachate or contaminated water should not be utilised for dust suppression. These details should be included in the working plan to be submitted by the 31st July 2006.
6.2 Noise dust and odour risk assessment

6.2.1 Prior to the undertaking of any engineering works at the site a risk assessment shall be made of the effect on properties outside the site of likely emissions of noise, dust and odour from those works.  The risk assessment shall identify environmental targets or receptors, the consequences of emissions, the trigger levels at which mitigating measures will be implemented and an assessment of the probability that the trigger levels will be attained having regard to the control measures proposed.

6.2.2 Where a risk assessment identifies a significant potential impact arising from the engineering works, or where otherwise required by the Agency, a monitoring programme shall be submitted to the Agency for approval.  The monitoring programme shall include the locations, frequency, protocols, trigger levels, recording, and quality assurance of monitoring together with an action plan for implementation when trigger levels are exceeded or are likely to be exceeded (e.g. due to particular meteorological conditions).

6.2.3 The engineering works shall not commence until the risk assessment referred to in subsection a) above has been submitted to the Agency and has been approved by the Agency in writing.  Where the risk assessment identifies the need to monitor the impact of noise, dust and odour, or when required by the Agency under subsection b) above, the engineering works shall not commence until a monitoring programme has been submitted to the Agency and has been approved in writing by the Agency.

6.2.4 Noise, dust and odour monitoring shall be carried out at the site in accordance with the monitoring programme approved in writing by the Agency.

6.2.5 When monitoring identifies that any trigger level specified within a monitoring programme has been exceeded, the emergency action plan within that programme shall be implemented immediately and the Agency shall be informed immediately.

6.3 Control of pests

6.3.1 At least once a week the site shall be inspected for signs of infestation by vermin and insects. In the event infestation is discovered immediate steps shall be taken to rid the site of that infestation.  All details of inspection and actions taken shall be recorded in the site diary. 

6.4 Control of litter

6.4.1 The site and its immediate environs shall be inspected daily for windblown litter and a record made in the site diary of the results of the inspection.  In the event that litter is found immediate steps shall be taken to ensure the offending material is collected and disposed of appropriately.

7 Security And Availability Of Records

7.1 Security and availability of records

7.1.1 All records which are required to be made under the other conditions of this licence and the working plan shall be maintained and kept secure from loss, damage or deterioration, and shall be kept at the site office.

7.2 Security of storage medium and data

7.2.1 Records which are required to be made under the other conditions of this licence and the working plan shall be made available for inspection at the place where they are kept immediately when required by an authorised officer of the Agency.

7.3 Recording of wastes accepted and removed

7.3.1 A record shall be kept of all wastes for restoration received and of all materials (wastes and recovered materials) removed from the landfill. The records shall include the following for each vehicle load of waste/material:

for waste used for restoration purposes received:
a origin of waste

b date received

c quantities in tonnes received and waste type 

d nature of the waste (solid)

for waste/material removed:
e date removed

f quantities in tonnes removed and waste and/or material type 

g destination of waste and/or materials removed

h nature of the waste and/or materials (solid, liquid or sludge)

7.3.2 A summary of the information, including nil returns, required by conditions 7.3.1 shall be submitted to the Agency, in a format required by the Agency.  Summaries shall be for each quarter of the financial year and shall be submitted to the Agency within one month of the end of each quarter.

7.4 Site diary

7.4.1 A site diary shall be kept secure and shall be available for inspection at the site when required by an authorised officer of the Agency.  This shall include a record of the following events:

a Start and finish dates of all construction works including preparatory works relevant to this licence.

b Times and dates of when technically competent management or specific personnel required for the licence were not present at the site. 

c Difficulties encountered with wastes received and action taken

d Emergencies (including any fires) which may result in pollution of the environment or harm to human health

e Inspections and maintenance of infrastructure.

f Sampling, surveying or monitoring exercises

g Operator's site inspections, their findings and remedial action taken

h Dispatch of records required by the licence to the Agency

i Extreme weather conditions

j Environmental incidents which could lead to pollution of the environment, harm to human health or detriment to the amenities of the locality


k (Vandalism or unauthorised access to the site

l Complaints received resulting from site operations

m Inspections for vermin and control measures taken  

7.4.2 Each record shall be completed within 24 hours of the relevant event occurring.

7.5 Recording Asbestos Waste Deposits 

7.5.1 Within 3 months of the date of this modification the site should collate information relating to all deposits of Asbestos wastes that have been received at the site.  The final plan and overlays of these deposits should be forwarded to the Agency. 

Rights of appeal

Section 43(1) of the Environmental Protection Act 1990 provides that, where except in pursuance of a direction given by The National Assembly For Wales,

· a licence is granted subject to conditions

the applicant may appeal from the decision to The National Assembly For Wales.

Therefore if you feel aggrieved by the decision or any of the conditions to the licence as granted you may obtain the appropriate form on which to give written notice of an appeal from:

The Planning Inspectorate

Crown Buildings

Cathays Park

Cardiff

CF10 3NQ

Tel: 02920 823859

Fax 02920 825150

This notice of appeal should be accompanied by the following information:

· a statement of the grounds of appeal

· a copy of the licence

· a copy of any correspondence relevant to the appeal

· a copy of any other document relevant to the appeal including, in particular, any relevant consent, determination, notice, planning permission, established use certificate or certificate of lawful use or development

· a statement indicating whether you wish the appeal to be in the form of a hearing or on the basis of written representations.

You are also required to serve a copy of your notice of appeal together with copies of any of the above documents that have accompanied your notice of appeal, to the Environment Agency. You should appeal within 6 months of the date that this notice takes effect but The National Assembly For Wales may allow notice of appeal to be given after the expiry of this time period.

YOUR ATTENTION IS DRAWN TO THE RIGHTS OF APPEAL DETAILED AT THE END OF THIS MODIFICATION.








Asiantaeth yr Amgylchedd Cymru

Maes Newydd, Llandarsi, Castell-Nedd Port Talbot, SA10 6JQ

Llinell gwasanaethau cwsmeriaid: 08708 506 506

Environment Agency Wales
Maes Newydd, Llandarcy, Neath Port Talbot, SA10 6JQ

Customer services line: 08708 506 506
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