


Permit Number: 	EPR/YP3937SH			Operator: 		Mekatek Limited

Facility:		Amex Park				Form Number: 	Water1 / 01/12/26
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty [4]

	W1
	Total suspended solids (TSS)
	60 mg/l
	24 hour flow-proportional composite sample
	
	BS EN 872 
	
	

	
	Total ammonium as N 
	20 mg/l (winter period) [5]
	24 hour flow-proportional composite sample
	
	Various BS EN Standards i.e. BS 6068-2.7, ISO 5664, BS 6068-2.10, ISO 6778
	
	

	
	
	15 mg/l (summer period) [6]
	
	
	
	
	

	
	Biochemical oxygen demand (5 day)
	75 mg/l (winter period) [5]
	24 hour flow-proportional composite sample
	
	BS EN ISO 5815-1
	
	

	
	
	40 mg/l (summer period) [6]
	
	
	
	
	

	
	Oils and grease
	No visible release
	Visual inspection
	
	-
	
	

	
	Temperature
	≤24ºC
	Three readings per day reported as a daily average
	
	Standard temperature sensor
	
	

	
	pH
	6 to 8.5 
	Daily average
	
	BS ISO 10523
	
	

	
	Flow
	39 l/second
	Continuous
	
	MCERTS - self monitoring of effluent flow scheme
	
	

	
	
	2500 m³/day
	
	
	
	
	

	
	Cadmium and its compounds as Cd
	0.05 mg/l
	24 hour flow-proportional composite sample
	
	Various BS EN standards available (i.e. BS EN ISO 11885, BS EN ISO 17294-2, BS EN ISO 15586)
	
	

	
	Chromium and its compounds as Cr
	0.15 mg/l
	
	
	
	
	

	
	Copper and its compounds as Cu
	0.5 mg/l
	
	
	
	
	

	
	Lead and its compounds as Pb
	0.1 mg/l
	
	
	
	
	

	
	Nickel and its compounds as Ni
	0.5 mg/l
	
	
	
	
	

	
	Zinc and its compounds as Zn
	1 mg/l
	
	
	
	
	

	
	Mercury and its compounds as Hg
	5 ug/l
	
	
	Various BS EN standards available (i.e. BS EN ISO 17852, BS EN ISO 12846)
	
	

	
	Free cyanide (CN-)
	0.1 mg/l
	
	
	Various BS EN standards available (e.g. BS EN ISO 14403-1 and -2)
	
	

	
	
	
	
	
	
	
	

	
	PFOA
	No Limit
	24 hour flow-proportional composite sample
	
	BS ISO 25101
	
	

	
	PFOS
	No Limit
	
	
	
	
	

	
	Phenol index
	0.3 mg/l
	24 hour flow-proportional composite sample
	
	BS EN ISO 14402
	
	

	
	Total nitrogen (Total N)
	25 mg/l
	24 hour flow-proportional composite sample
	
	BS EN 20236,  BS EN ISO 11905-1
	
	

	
	Total organic carbon (TOC)
	60 mg/l
	24 hour flow-proportional composite sample
	
	BS EN 1484
	
	

	
	Total phosphorus (Total P)
	2 mg/l
	24 hour flow-proportional composite sample
	
	Various BS EN standards available (i.e. BS EN ISO 15681-1 and -2, BS EN ISO 6878, BS EN ISO 11885)
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Winter period is defined as 01 October to 31 March.
[6] summer period is defined as 01 April to 30 September


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

