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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2016
___________________________________________

Resources Management U.K. Limited 
Withyhedge Landfill Site 
Bowling Farm 
Rudbaxton 
Haverfordwest 
Pembrokeshire 
SA62 4DB 

Variation application number
EPR/MP3330WP/V004
Permit number
EPR/MP3330WP













Withyhedge Landfill site 
Permit number EPR/MP3330WP
Introductory note 
This introductory note does not form a part of the notice.
[bookmark: _Hlk203381689]The main features of the permit are as follows.
Withyhedge Landfill is located approximately 5.5 km north of Haverfordwest in Pembrokeshire, Wales, at Bowling Farm, Rudbaxton (National Grid Reference: SM 970 217). The site, which covers around 53 hectares, is permitted as a non-hazardous landfill and has been operational since the mid-1980s.
The landfill has been developed in three phases:
· Phase 1 is now closed and restored. Constructed before modern landfill standards, cell construction varies – from no engineered lining in the earliest cells, to informal liners using site-won clay, and later to formal engineered liners as standards and regulations improved.

· Phase 2 consists of 11 engineered cells, all built with formal basal liners. The majority of this phase is now closed and restored.

· Phase 3 is currently being developed and filled, with each cell constructed to meet current engineering and environmental standards. Historically, this area was considered part of Phase 2, but the Operator has now chosen to designate it as a separate phase. Phase 3 will continue to be regulated under the same framework and agreements that apply to Phase 2. 
Leachate is collected and stored in tanks before being disposed of off-site. Landfill gas is actively extracted from the waste and used to generate electricity, or flared if generation is not possible.
Surface water runoff from capped surfaces of the landfill is directed to settlement ponds for attenuation and solids settlement, before being discharged to the Rudbaxton Water.
Restoration of Phases 1 and 2 has mainly used site-won subsoils and existing topsoil stockpiles. A permitted waste recovery activity enables the import of qualifying waste soils for use as engineering fill during cell construction and as restoration subsoil (with topsoil remaining site-won). These activities are managed through a Waste Recovery Plan and Construction Quality Assurance (CQA) plans as the site is developed.
The status log sets out the permitting history, including any changes to the permit reference number.
	Status log of the permit

	Description
	Date
	Comments

	Permit determined EPR/BP3131SG
	08/09/06
	

	Variation determined EPR/BP3131SG/V002
	17/12/07
	

	Variation determined EPR/BP3131SG/V003
	14/11/08
	

	Variation determined EPR/BP3131SG/V004
	05/03/10
	

	Variation determined EPR/BP3131SG/V005
Consolidated permit number EPR/GP3630HT
	16/09/10
	Consolidation of permits 
EPR/HP3498FS and 
EPR/BP3131SG

	Transfer determined EPR/GP3630HT/T001
	18/02/11
	

	Variation determined EPR/GP3630HT/V002
	18/05/11
	

	Variation determined EPR/GP3630HT/V003
	08/05/12
	

	Variation determined EPR/GP3630HT/V004
	12/06/13
	

	Variation determined EPR/GP3630HT/V005
	03/02/14
	

	Application EPR/MP3330WP/T001 (full transfer of permit EPR/GP3630HT)
	Duly made 
28/07/14
	Application to transfer the permit in full to Resources Management UK Limited

	Transfer determined EPR/MP3330WP
	29/09/14
	Full transfer of permit complete

	Regulator-initiated variation EPR/MP3330WP/V002
	21/08/2019
	Permit varied by Natural Resources Wales, Variation issued

	Variation Application 
EPR/MP3330WP/V004
(PAN-025929)
	Duly made
24/04/2025
	Application to vary the permitted pre-settlement contours, vary the management and monitoring program, add a Waste Recovery Activity and consolidate and modernise the permit. 

	Regulator-initiated variation EPR/MP3330WP/V003
(PAN-027481)
	13/05/2025
	Permit varied by Natural Resources Wales to update Financial Provision

	Additional information received in response to Schedule 5 Notice sent on 18/06/2025
	09/07/2025
	Waste Recovery Plan 

	Additional information received in response to Schedule 5 Notice sent on 28/08/2025
	09/09/2025
	Information relating to groundwater trigger levels for Nickel

	Additional information received in response to Schedule 5 Notice sent on 07/10/2025
	05/11/2025
	Updated monitoring plans, Hydrogeological Risk Assessment Review and Supporting Information 

	
	18/12/2025
	

	
	16/01/2026
	

	Variation determined  
EPR/MP3330WP/V004
	01/10/2026
	Variation issued as a result of operator led variation application (PAN-027481) and Natural Resources Wales initiated review.



End of introductory note.


Permit



The Environmental Permitting (England and Wales) Regulations 2016

Permit number
EPR/MP3330WP
This is the consolidated permit referred to in the variation and consolidation notice for application EPR/MP3330WP/V004 authorising
Resources Management U.K. Limited (“the operator”),
whose registered office is
Atlantic Eco Park
Newton Road
Rumney
Cardiff 
Wales 
CF3 2EJ
company registration number 02046398 
to operate an installation at:
Withyhedge Landfill Site 
Bowling Farm 
Rudbaxton 
Haverfordwest 
Pembrokeshire 
SA62 4DB 

to the extent authorised by and subject to the conditions of this permit.

Signed									         Date
	Holly Noble
	01/10/2026


Authorised on behalf of Natural Resources Wales








Management
[bookmark: _Ref373938749]General management
[bookmark: _Ref373938830]The operator shall manage and operate the activities:
in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints; and
using sufficient competent persons and resources.
Records demonstrating compliance with condition 1.1.1 shall be maintained. 
Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.
The operator shall comply with the requirements of an approved competence scheme.
Finance
The financial provision for meeting the obligations under this permit set out in the agreement made between the operator and Natural Resources Wales  dated 13/05/2025, or other financial provision as subsequently agreed in writing with Natural Resources Wales, shall be maintained by the operator throughout the subsistence of this permit and the operator shall produce evidence of such provision whenever required by Natural Resources Wales.
The operator shall ensure that the charges it makes for the disposal of waste in the landfill cover all of the following:
the costs of setting up and operating the landfill;
the costs of the financial provision required by condition 1.2.1; and
the estimated costs for the closure and aftercare of the landfill.
Energy efficiency
The operator shall:
take appropriate measures to ensure that energy is used efficiently in the activities;
Review and record at least every four years whether there are suitable opportunities to improve the energy efficiency of the activities; and 
Implement any appropriate measures identified by a review.
Efficient use of raw materials
The operator shall:
take appropriate measures to ensure that raw materials and water are used efficiently in the activities; 
maintain records of raw materials and water used in the activities;
review and record at least every four years whether there are suitable alternative materials that could reduce environmental impact or opportunities to improve the efficiency of raw material and water use; and
take any further appropriate measures identified by a review.
Avoidance, recovery and disposal of wastes produced by the activities
The operator shall:
take appropriate measures to ensure that waste produced by the activities is avoided or reduced, or where waste is produced it is recovered wherever practicable or otherwise disposed of in a manner which minimises its impact on the environment;
review and record at least every four years whether changes to those measures should be made; and 
take any further appropriate measures identified by a review.
Operations
Permitted activities
The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”).
The site 
The activities shall not extend beyond the site, being the land shown edged in red on the site plan at schedule 7 to this permit.
Operating techniques
The activities shall, subject to the conditions of this permit, be operated using the techniques and in the manner described in the documentation specified in schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.
If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan, and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
Improvement programme
The operator shall complete the improvements specified in schedule 1 table S1.3 by the date specified in that table unless otherwise agreed in writing by Natural Resources Wales.
Except in the case of an improvement which consists only of a submission to Natural Resources Wales, the operator shall notify Natural Resources Wales within 14 days of completion of each improvement.

Pre-operational conditions
The activities shall not be brought into operation until the measures specified in schedule 1 table S1.4a have been completed. 
The operations specified in schedule 1 table S1.4b shall not commence until the measures specified in that table have been completed.
Landfill Engineering
No construction of any new cell of the landfill shall commence until the operator has submitted construction proposals and Natural Resources Wales has confirmed that it is satisfied with the construction proposals.
Where the operator proposes to construct any new cell other than the first cell, but proposes no change from the design of the most recently approved cell which could have any impact on the performance of any element of the design, no construction of the new cell shall commence until the operator has submitted a cell layout drawing and Natural Resources Wales has confirmed that it is satisfied with the cell layout drawing.
The construction of a new cell shall take place only in accordance with the approved construction proposals unless:
any change to the approved construction proposals would have no impact on the performance of any element of the design; or 
a change has otherwise been agreed in writing by Natural Resources Wales.
No disposal of waste shall take place in a new cell until the operator has submitted a CQA Validation Report and Natural Resources Wales has confirmed that it is satisfied with the CQA Validation Report. 
No construction of landfill infrastructure shall commence until the operator has submitted relevant construction proposals or a written request to use previous construction proposals and Natural Resources Wales has confirmed that it is satisfied with the construction proposals. 
The construction of the landfill infrastructure shall take place only in accordance with the approved construction proposals unless:
any change to the approved construction proposals would have no impact on the performance of any element of the design; or 
a change has otherwise been agreed in writing by Natural Resources Wales.
The operator shall submit a CQA Validation Report within four weeks of the completion of the construction of the relevant landfill infrastructure, or other time period agreed in writing with Natural Resources Wales. 
Where pollution controls are immediately necessary to prevent an incident or accident, then conditions 2.6.5 and 2.6.6 do not apply and the relevant landfill infrastructure may be constructed, provided that the construction proposals are submitted to Natural Resources Wales as soon as practicable.
For the purposes of conditions 2.6.1, 2.6.2, 2.6.4 and 2.6.5, Natural Resources Wales shall be deemed to be satisfied where it has not, within the period of four weeks from the date of receipt of the relevant construction proposals or CQA Validation Report, either:
confirmed whether or not it is satisfied; or
informed the operator that it requires further information.
Where Natural Resources Wales has required further information under condition 2.6.9(b), Natural Resources Wales shall be deemed to be satisfied where it has not, within the period of four weeks from the date of receipt of the further information, either:
confirmed whether or not it is satisfied; or
informed the operator that it requires further information.
Waste acceptance
Wastes shall only be accepted for disposal if: 
they are listed in schedule 2, table S2.1 or S2.3;
they are non- hazardous waste or asbestos and construction materials containing asbestos;
they are not whole used tyres (other than bicycle tyres and tyres with an outside diameter of more than 1400mm); 
they are not shredded used tyres; 
they are not liquid waste (including waste waters but excluding sludge); 
they are not chemical substances from research and development or teaching activities, for example laboratory residues, which are unidentified and/or which are new and whose effects on man and/or the environment are unknown; 
they are not wastes that are textiles and foam from waste upholstered domestic seating that contain persistent organic pollutants; 
they are not wastes that would be explosive, corrosive, oxidising, flammable or highly flammable in the landfill; 
they are not wastes separately collected for preparing for re-use and recycling, and
they are not waste woods;
all the relevant waste acceptance procedures have been completed; 
they fulfil the relevant waste acceptance criteria; 
they have not been diluted or mixed solely to meet the relevant waste acceptance criteria;
they are wastes which have been treated, except for: inert wastes for which treatment is not technically feasible; or it is waste other than inert waste and treatment would not reduce its quantity or the hazards which it poses to human health or the environment; and
they are wastes with a code beginning with 07 05 and 16 03, they shall exclude waste medicinal products and pharmaceutically active waste materials arising from their manufacture.
Wastes shall only be accepted for restoration where:
they are listed in schedule 2, table S2.2; and
they are accepted in accordance with a restoration plan approved in writing by Natural Resources Wales.
Asbestos containing wastes and construction materials containing asbestos shall only be disposed of with other suitable wastes and not in cells containing biodegradable non-hazardous waste. Asbestos waste and construction material containing asbestos must meet the relevant waste acceptance criteria and must be covered daily and before each compaction operation with appropriate material. 
The operator shall: 
visually inspect without unloading it, waste that is not in an enclosed container or enclosed vehicle on arrival at the landfill and waste at the point of deposit; and
be satisfied that the waste conforms to the requirements of condition 2.7.1. 
Where the operator has taken samples to establish that the waste is in conformity with the documentation submitted by the holder then the samples taken shall be retained for at least one month and results of any analysis for at least two years.
The operator on accepting each delivery of waste shall provide a receipt to the person delivering it.
The total quantity of waste that shall be deposited in the landfill shall be limited by the pre-settlement levels shown on drawing ‘Proposed Pre-Settlement Landform and Landscaping Details’ (drawing reference 2365/4) dated 05/2024.
The quantity of waste that is deposited in the landfill in any year shall not exceed the limits in schedule 1 table S1.5.
The operator shall maintain and implement a system which ensures that a record is made of the quantity, characteristics, date of delivery and, where practicable, origin of any waste that is received for disposal or recovery and of the identity of the producer, or in the case of municipal waste and multiple collection vehicles, of the collector of such waste. Any information regarded by the operator as commercially confidential shall be clearly identified in the record.
Leachate levels
The limits for the level of leachate listed in schedule 3 table S3.1 shall not be exceeded. 
Closure and aftercare
The operator shall maintain a closure and aftercare management plan.
Landfill gas management
The operator shall take appropriate measures, including, but not limited to, those specified in any approved landfill gas management plan, to:
collect landfill gas; and
control the migration of landfill gas.
The operator shall use the collected landfill gas to produce energy. If the collected landfill gas cannot be used to produce energy, the operator shall use appropriate measures to flare or treat the gas in accordance with an approved landfill gas management plan.
The operator shall:
if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a revised landfill gas management plan; and
implement the revised landfill gas management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
Emissions and monitoring
Emissions to water, air or land
The limits in Schedule 3 shall not be exceeded.
There shall be no point source emissions to water, air or land except from the sources and emission points listed in schedule 3 tables S3.2 and S3.3.
The limits given in table S3.2 shall not be exceeded, save that compliance with an emission limit in that table shall include incorporation of the uncertainty allowance stated in Environment Agency guidance LFTGN 05 and LFTGN 08.
The operator shall prevent the input of any hazardous substances from the activities into groundwater. 
There shall be no emission from the activities into groundwater of any non-hazardous pollutants so as to cause pollution
The operator shall submit to Natural Resources Wales a review of the Hydrogeological Risk Assessment:
between nine and six months prior to the fourth anniversary of the granting of the permit; and 
between nine and six months prior to every subsequent six years after the fourth anniversary of the granting of the permit.
Emissions of substances not controlled by emission limits
[bookmark: _Toc318726318]Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
[bookmark: _Toc318726319]The operator shall:
if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits; and
implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
[bookmark: _Toc318726320]All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.


Odour
Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
The operator shall:
if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to odour, submit to Natural Resources Wales for approval within the period specified, an odour management plan which identifies and minimises the risks of pollution from odour; and
implement the revised odour management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
Noise and vibration
Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
The operator shall:
if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration; and
implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
Monitoring 
The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring and any other actions specified in the following tables in schedule 3 to this permit:
Leachate specified in tables S3.1 and S3.10;
Point source emissions specified in tables S3.2 and S3.3;
Groundwater specified in tables S3.4 and S3.8;
Landfill gas specified in tables S3.5, S3.7 and S3.9;
Surface water specified in table S3.11; and
Particulate matter specified in table S3.12.
The operator shall maintain records of all monitoring required by this permit including records of the taking and analysis of samples, instrument measurements (periodic and continual), calibrations, examinations, tests and surveys and any assessment or evaluation made on the basis of such data.
A topographical survey of the site referenced to ordnance datum shall be carried out and shall be used to produce a plan of a scale adequate to show the surveyed features of the site:
annually;
prior to the disposal of waste in any new cell or new development area of the landfill; and
following closure of the landfill or part of the landfill.
Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1, S3.2, S3.3, S3.4, S3.5 and 3.8, 3.10 unless otherwise agreed in writing by Natural Resources Wales.
Pests
The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  
The operator shall:	
if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution hazard or annoyance from pests; and
implement the pests management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
Information
Records
[bookmark: _Toc318726339]All records required to be made by this permit shall:
[bookmark: _Toc318726340]be legible;
[bookmark: _Toc318726341]be made as soon as reasonably practicable;
[bookmark: _Toc318726342]if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
[bookmark: _Toc318726343]be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
the results of groundwater monitoring; 
sub-surface landfill gas monitoring; 
leachate levels, quality and quantities;
landfill gas generation and collection;
waste types and quantities; and
the specification and as built drawings of the basal, sidewall and capping engineering systems.
The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales.
Reporting
The operator shall send reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
A report or reports on the performance of the activities over the previous year (‘the annual report’) shall be submitted to Natural Resources Wales by 31 January each year or such other date as may be agreed in writing by Natural Resources Wales, with the exception of 4.2.2(c) that must be provided by the end of February each year. The report(s) shall include as a minimum:
a review of the results of the monitoring and assessment carried out in accordance with this permit against the relevant assumptions, parameters and results in the risk assessments submitted in relation to this installation and any agreed amendments thereto. The review will include written descriptions of the improvements made to operational performance during the year, action plans developed and planned improvements for the coming year;
the energy consumed at the site, reported in the format set out in schedule 4 table S4.3;
the annual production/treatment set out in schedule 4 table S4.2;
the topographical surveys required by condition 3.5.3 other than those submitted as part of a CQA validation report;
the volumetric difference (reported in cubic metres) between the most recent topographical survey and the previous annual topographical survey i.e. the additional volume of the landfill void that is occupied by waste;
an assessment of the settlement behaviour of the landfill body based on the difference between the most recent topographical survey and previous annual topographical survey for the areas of the landfill which did not receive waste between the surveys;
a calculation of the remaining capacity (reported in cubic metres) derived from the pre-settlement contours and the most recent topographical survey; 
a plan(s) (‘the monitoring and extraction point plan – MEPP’) showing the locations of existing and any new leachate and landfill gas extraction and monitoring points; and
a summary of the results of any waste validation (level 3) testing you have carried out.
Within 28 days of the end of the reporting period the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
in respect of the parameters and emission points specified in schedule 4 table S4.1;
using the forms specified in schedule 4 table S4.4 or other reporting format as agreed in writing with Natural Resources Wales; and
giving the information from such results and assessments as may be required by the forms specified in those tables.
Within one month of the end of each quarter, the operator shall submit to Natural Resources Wales using the form made available for the purpose, the information specified on the form relating to the site and the waste accepted and removed from it during the previous quarter.
The operator shall, unless notice under this condition has been served within the preceding four years, submit to Natural Resources Wales, within six months of receipt of a written notice, a report assessing whether there are other appropriate measures that could be taken to prevent, or where that is not practicable, to minimise pollution.
Notifications
(a)	In the event that the operation of the activities gives rise to an incident or accident which significantly affects or may significantly affect the environment, the operator must immediately—
inform Natural Resources Wales; 
take the measures necessary to limit the environmental consequences of such an incident or accident; and
take the measures necessary to prevent further possible incidents or accidents.
in the event of a breach of any permit condition the operator must immediately—
inform Natural Resources Wales; and
take the measures necessary to ensure that compliance is restored within the shortest possible time;
in the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment, the operator must immediately suspend the operation of the activities or the relevant part of it until compliance with the permit conditions has been restored.
Any information provided under condition 4.3.1 shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales, when the relevant monitoring is to take place. The operator shall provide this information to Natural Resources Wales, at least 14 days before the date the monitoring is to be undertaken.
Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules:
Where the operator is a registered company:
any change in the operator’s trading name, registered name or registered office address; and
any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
 any change in the operator’s name or address; and
any steps taken with a view to the dissolution of the operator;
In any other case: 
the death of any of the named operators (where the operator consists of more than one named individual);
any change in the operator’s name(s) or address(es); and
any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership.
[bookmark: _Toc318726381]Interpretation
[bookmark: _Toc318726382]In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
[bookmark: _Toc318726383]In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “immediately”, in which case it may be provided by telephone. 
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Schedule 1 – Operations
	Table S1.1 Activities

	Activity reference 
	WFD Annex I and II operations (where applicable)
	Activity listed in Schedule 1 of the EP Regulations 
	Description of specified activity
	Limits of specified activity 

	A1
	D1 – Deposit into or onto land e.g. landfill 

D5 –Specially engineered landfill 


	[bookmark: _Hlk193290024]Section 5.2 Part A(1) (a), the disposal of waste in a landfill
	Landfill for non-hazardous waste
	Receipt, handling and disposal of wastes, consisting of the types specified in Table S2.1 as an integral part of landfilling.

The receipt, handling, and disposal of asbestos waste shall be limited to the types specified in Table S2.3. Disposal of asbestos waste shall be restricted to a single hazardous waste cell and shall not commence until NRW has provided written confirmation that pre-operational measure 6 for future development, as specified in Table S1.4A, has been completed.

Quantities restricted to those specified in Table S1.5. 

Disposal of waste limited to ‘Phase 2’ and ‘Phase 3’ as shown on the Site Plan in Schedule 7 (document titled “Withyhedge Landfill Permit Variation 2023 Site Plan” document reference 2365/1r1, dated 03/2025). 

No further disposal of waste shall occur in capped areas of the landfill where pre-settlement levels (in accordance with condition 2.7.7.) have been achieved, unless otherwise agreed in writing with Natural Resources Wales.


	Directly Associated Activities

	A2
	R1 – use principally as a fuel to generate energy
	Landfill Gas Management
	Combustion of landfill gas for the purpose of electricity generation. 


	Treatment and utilisation of landfill gas arising from the landfill.

	A3
	N/A
	
	Flaring of landfill gas.
	Landfill gas arising from the permitted landfill.

	A4
	D15 – Storage pending any of the disposal operations

R – Storage of waste pending any of the recovery operations

	Leachate Management
	Collection and storage of leachate prior to removal from site for disposal. 
	Leachate arising from the landfill. Storage pending removal by road tanker. 



	A5
	D6 – release to waterbody except seas/oceans  
	Surface Water Management
	Discharge of site drainage from the landfill. 
	From surface water management system to point of entry to controlled waters. 

	A6
	N/A
	N/A
	Fuel storage 
	Storage of fuel in a fuel tank/ bowser for operation of plant and equipment. 

	A7
	R5 – Recycling/reclamation of other inorganic materials 
	N/A
	Deposit of waste for recovery 
	Annual quantities restricted to those specified in Table S1.5. 
 
In any event the total quantity of waste used shall not exceed the amount needed to complete the recovery operation to the final levels in the approved waste recovery plan received 09/07/2025 or any subsequent waste recovery plan agreed in writing with Natural Resources Wales Note 1.

Only the waste types specified in table S2.2 shall be accepted for restoration. Such wastes shall only be used as specified in the approved waste recovery plan   No waste shall be deposited into a water body or sub-water table.


Note 1: The waste recovery plan shall be reviewed every 5 years and approved in writing by Natural Resources Wales 

	[bookmark: _Hlk210035044]Table S1.2 Operating techniques 

	Description
	Parts
	Date Received

	  Operating techniques 
	Operating techniques agreed prior to the issuing of permit variation EPR/MP3330W/V004 have been consolidated in a separate document referenced ‘Table S1.2 Withyhedge Landfill Operating Techniques’
	-

	Review of Waste Inputs and Waste Acceptance Procedure for Cell 9
	Report number 2481r1v1d1024
	04/11/2024

	Variation Application 
EPR/MP3330WP/V004 – not duly made response

	Drawing reference ‘Proposed Pre-Settlement Landform and Landscaping Details’, drawing number 2365/4, dated 05/2024
	21/03/2025

	
	Drawing reference ‘Surface Water Management system, drawing number   2365/16, dated 03/25’
	21/03/2025

	Variation Application 
EPR/MP3330WP/V004
(PAN-025929) - response to Schedule 5 Notice dated 18/06/2025
	 Waste Recovery Plan (document reference ‘Waste Recovery Plan for use of soils in restoration and engineering, report number 2528r1v1d0325, dated March 2025)
	09/07/2025

	
	 Waste Acceptance Procedure for Soils for Restoration (document reference ‘Waste Acceptance Procedure for Soils for Restoration v1.1, dated 30/07/2025’)
	30/07/2025

	Variation Application 
EPR/MP3330WP/V004
(PAN-025929) - response to  informal information request sent on 18/08/2025
	 Phase 2 Surface Water Management System (document reference Withyhedge Landfill Phase 2 Surface Water Management System, Design and Construction Validation Report, report number 2548r1v1d0425, dated April 2025)
	20/08/2025

	Waste Acceptance Procedures
	RML - Waste Acceptance (NSSL ARL Only) – v2.0
	02/09/2025

	Waste Phasing Plan for Cell 10

	10Cell 10 Infilling Plan. 
Report Number 2590r1v1d0925
	09/2025

	Variation Application 
EPR/MP3330WP/V004
(PAN-025929) - response to Schedule 5 Notice dated 07/10/2025
	 Hydrogeological Risk Assessment Review (document reference ‘Hydrogeological Risk Assessment Review, report number 2365r2v2d1025, dated October 2025), specifically: 
section 10.3 ‘Surface Water’
section 10 ‘Requisite Surveillance’
section 11 ‘New Triggers and Controls’ 
	16/01/2026

	
	Supporting Information (document reference ‘Withyhedge Landfill Permit Variation EPR MP330WP Supporting Information, report number 2365r2vd1025, dated October 2025), specifically: 
section 5.5 Perimeter Ground Gas Monitoring 
 ‘Proposed Restoration Surface Gradient’, drawing number 2365/5, dated 04/2023
	16/01/2026

	Waste Acceptance Procedures
	RML - Waste Acceptance (NSSL ARL Only) – v2.0
	02/09/2025

	Response to Improvement Condition 20
	All updated Management Plans approved by Natural Resources Wales in accordance with Improvement Condition 20
	-



	[bookmark: _Hlk210051438]Table S1.3 Improvement programme requirements

	Reference
	Requirement
	Date

	1 - 19
	Improvement conditions stipulated prior to the issuing of permit variation EPR/MP3330W/V004 have been consolidated in a separate document referenced ‘Table S1.3 Withyhedge Landfill Improvement Conditions’. These are considered completed (or superseded). 
	-

	20
	The operator shall review and update its Environmental Management System (EMS) to reflect all the changes introduced by the variation. This includes, but is not limited to, an updated: 
· Landfill Gas Management Plan 
· Leachate Management Plan 
· Odour Management Plan

 The updated EMS shall take into account all relevant guidance and:
· detail any revised operational procedures and controls
· update roles and responsibilities where applicable
· include any new monitoring, reporting, or record-keeping requirements and;
· include evidence of staff training or awareness related to the changes.

The operator shall submit the updated EMS to Natural Resources Wales for approval by the date specified.
	Within 6 months of EPR/MP3330WP/V004
permit issue or as otherwise agreed in writing with Natural Resources Wales.

	21
	The operator shall produce an interim review of the Hydrological Risk Assessment (HRA) for the site.

The HRA shall take into consideration data gathered following implementation of the new monitoring programme, outlined in ‘Hydrogeological Risk Assessment Review (report number 2365r2v2d1025, dated October 2025)

The operator should submit the review to Natural Resources Wales for approval. 
	31st December 2027 



	Table S1.4 Pre-operational measures 

	 Reference
	Pre-operational Measures

	1-4
	Pre-operational measures stipulated prior to the issuing of permit variation EPR/MP3330W/V004 have been consolidated in a separate document referenced ‘Table S1.4 and S1.4A Withyhedge Landfill Pre-operational Measures’. These are considered completed (or superseded).



	Table S1.4 Pre-operational measures for Future Development

	 Reference
	Pre-operational Measures

	1-5, 7, 8
	Pre-operational measures for future development stipulated prior to the issuing of permit variation EPR/MP3330W/V004 have been consolidated in a separate document referenced ‘Table S1.4 and S1.4A Withyhedge Landfill Pre-operational Measures’. These are considered completed (or superseded).

	6
	Prior to the construction of a new cell for the deposit of asbestos wastes in Phase’s 2 or 3 of the landfill.
Detailed construction design proposals shall be submitted for approval and shall include consideration of impact of design upon existing leachate management infrastructure , access to asbestos cell – if across closed cells a review of assumptions made in Stability Risk assessments for closed cells, asbestos waste acceptance and placement methodology and an asbestos monitoring procedure.

	9a
	Prior to the construction of a new cell for the deposit of asbestos wastes in Phase’s 2 or 3 of the landfill.
The operator shall review the particulate risk assessment in light of the increased rate of waste deposit and future construction activities and shall submit a written proposal, for approval, for 12 months dust deposition and particulate monitoring along the site boundary to assess impacts from dust with a view to establishing the need for permanent monitoring and particulate emission limits. 
The proposed plan shall be prepared in accordance with the relevant standards contained within Environment Agency guidance documents:
• Monitoring emissions to air, land and water (MCERTS): Monitoring guides for air 

	9b
	On completion of 9a, the Operator shall submit the particulates risk assessment for approval prior to the commencement of construction of a new cell for asbestos wastes in Phase’s 2 or 3 of the landfill.

Upon completion of 12 months monitoring data the operator shall review and submit the Agency the particulates risk assessment. The review shall include:
• Quantification of emissions from the site;
• Identification of off site receptors and impacts
• An assessment of the effectiveness of control measures including a detailed appraisal of alternative control measures;
Recommendations, and timetable for implementation, for the establishment of alternative control measures and ongoing monitoring of dust and particulates emissions at the installation where identified as necessary.

	10
	Prior to the construction of any new landfill cells within Phase 3, the Operator shall undertake a review of groundwater monitoring data to assess if any control measures are required to ensure an unsaturated zone of 1.0m is maintained beneath the base of the engineered lining of the cell. 

The findings of the review, including the monitoring data and justification for any control measures (or no control measures) shall be documented and submitted within the CQA Plan for the cell. The CQA Plan must be approved by Natural Resources Wales prior to the cell being constructed. 


	11
	Prior to the construction of any new landfill cells within Phase 3 (including any enabling works such as soil stripping), the Operator  shall construct a surface water management system capable of effectively managing surface run-off from the whole development area C. 
A CQA Plan for the surface water management system and its construction should be submitted to Natural Resources Wales. The CQA Plan must be approved by Natural Resources Wales, and the surface water system fully operational prior to the cell being constructed. 

Alternatively, the Operator should submit evidence to prove that the existing surface water management system for Phase 3 is capable of effectively managing the additional surface run-off. 







	Table S1.5 Annual waste input limits

	Category
	Limit Tonnes/ Year

	Non-hazardous waste
	250,000

	Inert waste
	

	Asbestos wastes Note 1
	5,000

	Waste for restoration
	50,000

	Total
	305,000


Note 1: Asbestos wastes only permitted once pre-operational measures for future development references 6, 9a and 9b have been satisfied and agreed in writing with Natural Resources Wales

Schedule 2 – List of permitted wastes
	Table S2.1 Permitted waste types for disposal at a landfill for non-hazardous waste

	Waste code
	Description

	Exclusions
	Wastes having any of the following characteristics shall not be accepted: 
· wastes separately collected for preparing for re-use and recycling
· waste woods

	01
	Wastes resulting from exploration, mining, quarrying, and physical and chemical treatment of minerals

	01 01
	wastes from mineral excavation

	01 01 01
	wastes from mineral metalliferous excavation

	01 01 02
	wastes from mineral non-metalliferous excavation

	01 03
	wastes from physical and chemical processing of metalliferous minerals

	01 03 06
	tailings other than those mentioned in 01 03 04 and 01 03 05

	01 03 08
	dusty and powdery wastes other than those mentioned in 01 03 07

	01 03 09
	red mud from alumina production other than the wastes mentioned in 01 03 10

	01 04
	wastes from physical and chemical processing of non-metalliferous minerals

	01 04 08
	waste gravel and crushed rocks other than those mentioned in 01 04 07

	01 04 09
	waste sand and clays

	01 04 10
	dusty and powdery wastes other than those mentioned in 01 04 07

	01 04 11
	wastes from potash and rock salt processing other than those mentioned in 01 04 07

	01 04 12
	tailings and other wastes from washing and cleaning of minerals other than those mentioned in 01 04 07 and 01 04 11

	01 04 13
	wastes from stone cutting and sawing other than those mentioned in 01 04 07

	01 05
	drilling muds and other drilling wastes

	01 05 04
	freshwater drilling muds and wastes

	01 05 07
	barite-containing drilling muds and wastes other than those mentioned in 01 05 05 and 01 05 06

	01 05 08
	chloride-containing drilling muds and wastes other than those mentioned in 01 05 05 and 01 05 06

	02
	Wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing, food preparation and processing

	02 01
	wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing

	02 01 01
	sludges from washing and cleaning

	02 01 02
	animal-tissue waste

	02 01 03
	plant-tissue waste

	02 01 04
	waste plastics (except packaging)

	02 01 06
	animal faeces, urine and manure (including spoiled straw), effluent, collected separately and treated off-site

	02 01 07
	wastes from forestry

	02 01 09
	agrochemical waste other than those mentioned in 02 01 08

	02 01 10
	waste metal

	02 02
	wastes from the preparation and processing of meat, fish and other foods of animal origin

	02 02 01
	sludges from washing and cleaning

	02 02 02
	animal-tissue waste

	02 02 03
	materials unsuitable for consumption or processing

	02 02 04
	sludges from on-site effluent treatment

	02 03
	wastes from fruit, vegetables, cereals, edible oils, cocoa, coffee, tea and tobacco preparation and processing; conserve production; yeast and yeast extract production, molasses preparation and fermentation

	02 03 01
	sludges from washing, cleaning, peeling, centrifuging and separation

	02 03 02
	wastes from preserving agents

	02 03 03
	wastes from solvent extraction

	02 03 04
	materials unsuitable for consumption or processing

	02 03 05
	sludges from on-site effluent treatment

	02 04
	wastes from sugar processing

	02 04 01
	soil from cleaning and washing beet

	02 04 02
	off-specification calcium carbonate

	02 04 03
	sludges from on-site effluent treatment

	02 05
	wastes from the dairy products industry

	02 05 01
	materials unsuitable for consumption or processing

	02 05 02
	sludges from on-site effluent treatment

	02 06
	wastes from the baking and confectionery industry

	02 06 01
	materials unsuitable for consumption or processing

	02 06 02
	wastes from preserving agents

	02 06 03
	sludges from on-site effluent treatment

	02 07
	wastes from the production of alcoholic and non-alcoholic beverages (except coffee, tea and cocoa)

	02 07 01
	wastes from washing, cleaning and mechanical reduction of raw materials

	02 07 02
	wastes from spirits distillation

	02 07 03
	wastes from chemical treatment

	02 07 04
	materials unsuitable for consumption or processing

	02 07 05
	sludges from on-site effluent treatment

	03
	Wastes from wood processing and the production of panels and furniture, pulp, paper and cardboard

	03 01
	wastes from wood processing and the production of panels and furniture

	03 01 01
	waste bark and cork

	03 01 05
	sawdust, shavings, cuttings, wood, particle board and veneer other than those mentioned in 03 01 04

	03 03
	wastes from pulp, paper and cardboard production and processing

	03 03 01
	  waste bark and wood

	03 03 02
	green liquor sludge (from recovery of cooking liquor)

	03 03 05
	de-inking sludges from paper recycling

	03 03 07
	mechanically separated rejects from pulping of waste paper and cardboard

	03 03 08
	wastes from sorting of paper and cardboard destined for recycling

	03 03 09
	lime mud waste

	03 03 10
	fibre rejects, fibre-, filler- and coating-sludges from mechanical separation

	03 03 11
	sludges from on-site effluent treatment other than those mentioned in 03 03 10

	04
	Wastes from the leather, fur and textile industries

	04 01
	wastes from the leather and fur industry

	04 01 01
	fleshings and lime split wastes

	04 01 02
	liming waste

	04 01 06
	sludges, in particular from on-site effluent treatment containing chromium

	04 01 07
	sludges, in particular from on-site effluent treatment free of chromium

	04 01 08
	waste tanned leather (blue sheetings, shavings, cuttings, buffing dust) containing chromium

	04 01 09
	wastes from dressing and finishing

	04 02
	wastes from the textile industry

	04 02 09
	wastes from composite materials (impregnated textile, elastomer, plastomer)

	04 02 10
	organic matter from natural products (for example grease, wax)

	04 02 15
	wastes from finishing other than those mentioned in 04 02 14

	04 02 17
	dyestuffs and pigments other than those mentioned in 04 02 16

	04 02 20
	sludges from on-site effluent treatment other than those mentioned in 04 02 19

	04 02 21
	wastes from unprocessed textile fibres

	04 02 22
	wastes from processed textile fibres

	05
	Wastes from petroleum refining, natural gas purification and pyrolytic treatment of coal

	05 01
	wastes from petroleum refining

	05 01 10
	sludges from on-site effluent treatment other than those mentioned in 05 01 09

	05 01 13
	boiler feedwater sludges

	05 01 14
	wastes from cooling columns

	05 01 17
	bitumen

	05 06
	wastes from the pyrolytic treatment of coal

	05 06 04
	waste from cooling columns

	06
	Wastes from inorganic chemical processes

	06 03
	wastes from the MFSU of salts and their solutions and metallic oxides

	06 03 14
	solid salts and solutions other than those mentioned in 06 03 11 and 06 03 13

	06 03 16
	metallic oxides other than those mentioned in 06 03 15

	06 05 03
	sludges from on-site effluent treatment other than those mentioned in 06 05 02

	06 09
	wastes from the MSFU of phosphorous chemicals and phosphorous chemical processes

	06 09 02
	phosphorous slag

	06 11
	wastes from the manufacture of inorganic pigments and opacificiers

	06 11 01
	calcium-based reaction wastes from titanium dioxide production

	06 13
	wastes from inorganic chemical processes not otherwise specified

	06 13 03
	carbon black

	07
	Wastes from organic chemical processes

	07 01
	wastes from the manufacture, formulation, supply and use (MFSU) of basic organic chemicals

	07 01 12
	sludges from on-site effluent treatment other than those mentioned in 07 01 11

	07 02
	wastes from the MFSU of plastics, synthetic rubber and man-made fibres

	07 02 12
	sludges from on-site effluent treatment other than those mentioned in 07 02 11

	07 02 13
	waste plastic

	07 02 15
	wastes from additives other than those mentioned in 07 02 14

	07 02 17
	waste containing silicones other than those mentioned in 07 02 16

	07 03
	wastes from the MFSU of organic dyes and pigments (except 06 11)

	07 03 12
	sludges from on-site effluent treatment other than those mentioned in 07 03 11

	07 04
	wastes from the MFSU of organic plant protection products (except 02 01 08 and 02 01 09), wood preserving agents (except 03 02) and other biocides

	07 04 12
	sludges from on-site effluent treatment other than those mentioned in 07 04 11

	07 05
	wastes from the MFSU of pharmaceuticals

	07 05 14
	solid wastes other than those mentioned in 07 05 13

	07 06
	wastes from the MFSU of fats, grease, soaps, detergents, disinfectants and cosmetics

	07 06 12
	sludges from on-site effluent treatment other than those mentioned in 07 06 11

	07 07
	wastes from the MFSU of fine chemicals and chemical products not otherwise specified

	07 07 12
	sludges from on-site effluent treatment other than those mentioned in 07 07 11

	08
	Wastes from the manufacture, formulation, supply and use (MFSU) of coatings (paints, varnishes and vitreous enamels), adhesives, sealants and printing inks

	08 01
	wastes from MFSU and removal of paint and varnish

	08 01 12
	waste paint and varnish other than those mentioned in 08 01 11

	08 01 14
	sludges from paint or varnish other than those mentioned in 08 01 13

	08 01 16
	aqueous sludges containing paint or varnish other than those mentioned in 08 01 15

	08 01 18
	wastes from paint or varnish removal other than those mentioned in 08 01 17

	08 02
	wastes from MFSU of other coatings (including ceramic materials)

	08 02 01
	waste coating powders

	08 02 02
	aqueous sludges containing ceramic materials

	08 03
	wastes from MFSU of printing inks

	08 03 07
	aqueous sludges containing ink

	08 03 13
	waste ink other than those mentioned in 08 03 12

	08 03 15
	ink sludges other than those mentioned in 08 03 14

	08 03 18
	waste printing toner other than those mentioned in 08 03 17

	08 04
	wastes from MFSU of adhesives and sealants (including water proofing products)

	08 04 10
	waste adhesives and sealants other than those mentioned in 08 04 09

	08 04 12
	adhesive and sealant sludges other than those mentioned in 08 04 11

	08 04 14
	aqueous sludges containing adhesives or sealants other than those mentioned in 08 04 13

	09
	Wastes from the photographic industry

	09 01
	wastes from the photographic industry

	09 01 07
	photographic film and paper containing silver or silver compounds

	09 01 08
	photographic film and paper free of silver or silver compounds

	09 01 10
	single-use cameras without batteries

	09 01 12
	single-use cameras containing batteries other than those mentioned in 09 01 11

	10
	Wastes from thermal processes

	10 01
	wastes from power stations and other combustion plants (except 19)

	10 01 01
	bottom ash, slag and boiler dust (excluding boiler dust mentioned in 10 01 04)

	10 01 02
	coal fly ash

	10 01 03
	fly ash from peat and untreated wood

	10 01 05
	calcium-based reaction wastes from flue-gas desulphurisation in solid form

	10 01 07
	calcium-based reaction wastes from flue-gas desulphurisation in sludge form

	10 01 15
	bottom ash, slag and boiler dust from co-incineration other than those mentioned in 10 01 14

	10 01 17
	fly ash from co-incineration other than those mentioned in 10 01 16

	10 01 19
	wastes from gas cleaning other than those mentioned in 10 01 05, 10 01 07 and 10 01 18

	10 01 21
	sludges from on-site effluent treatment other than those mentioned in 10 01 20

	10 01 23
	aqueous sludges from boiler cleansing other than those mentioned in 10 01 22

	10 01 24
	sands from fluidised beds

	10 01 25
	wastes from fuel storage and preparation of coal-fired power plants

	10 01 26
	wastes from cooling-water treatment

	10 02
	wastes from the iron and steel industry

	10 02 01
	wastes from the processing of slag

	10 02 02
	unprocessed slag

	10 02 08
	solid wastes from gas treatment other than those mentioned in 10 02 07

	10 02 10
	mill scales

	10 02 12
	wastes from cooling-water treatment other than those mentioned in 10 02 11

	10 02 14
	sludges and filter cakes from gas treatment other than those mentioned in 10 02 13

	10 02 15
	other sludges and filter cakes

	10 03
	wastes from aluminium thermal metallurgy

	10 03 02
	anode scraps

	10 03 05
	waste alumina

	10 03 16
	skimmings other than those mentioned in 10 03 15

	10 03 18
	carbon-containing wastes from anode manufacture other than those mentioned in 10 03 17

	10 03 20
	flue-gas dust other than those mentioned in 10 03 19

	10 03 22
	other particulates and dust (including ball-mill dust) other than those mentioned in 10 03 21

	10 03 24
	solid wastes from gas treatment other than those mentioned in 10 03 23

	10 03 26
	sludges and filter cakes from gas treatment other than those mentioned in 10 03 25

	10 03 28
	wastes from cooling-water treatment other than those mentioned in 10 03 27

	10 03 30
	wastes from treatment of salt slags and black drosses other than those mentioned in 10 03 29

	10 04
	wastes from lead thermal metallurgy

	10 04 10
	wastes from cooling-water treatment other than those mentioned in 10 04 09

	10 05
	wastes from zinc thermal metallurgy

	10 05 01
	slags from primary and secondary production

	10 05 04
	other particulates and dust

	10 05 09
	wastes from cooling-water treatment other than those mentioned in 10 05 08

	10 05 11
	dross and skimmings other than those mentioned in 10 05 10

	10 06
	wastes from copper thermal metallurgy

	10 06 01
	slags from primary and secondary production

	10 06 02
	dross and skimmings from primary and secondary production

	10 06 04
	other particulates and dust

	10 06 10
	wastes from cooling-water treatment other than those mentioned in 10 06 09

	10 07
	wastes from silver, gold and platinum thermal metallurgy

	10 07 01
	slags from primary and secondary production

	10 07 02
	dross and skimmings from primary and secondary production

	10 07 03
	solid wastes from gas treatment

	10 07 04
	other particulates and dust

	10 07 05
	sludges and filter cakes from gas treatment

	10 07 08
	wastes from cooling-water treatment other than those mentioned in 10 07 07

	10 08
	wastes from other non-ferrous thermal metallurgy

	10 08 04
	particulates and dust

	10 08 09
	other slags

	10 08 11
	dross and skimmings other than those mentioned in 10 08 10

	10 08 13
	carbon-containing wastes from anode manufacture other than those mentioned in 10 08 12

	10 08 14
	anode scrap

	10 08 16
	flue-gas dust other than those mentioned in 10 08 15

	10 08 18
	sludges and filter cakes from flue-gas treatment other than those mentioned in 10 08 17

	10 08 20
	wastes from cooling-water treatment other than those mentioned in 10 08 19

	10 09
	wastes from casting of ferrous pieces

	10 09 03
	furnace slag

	10 09 06
	casting cores and moulds which have not undergone pouring other than those mentioned in 10 09 05

	10 09 08
	casting cores and moulds which have undergone pouring other than those mentioned in 10 09 07

	10 09 10
	flue-gas dust other than those mentioned in 10 09 09

	10 09 12
	other particulates other than those mentioned in 10 09 11

	10 09 14
	waste binders other than those mentioned in 10 09 13

	10 09 16
	waste crack-indicating agent other than those mentioned in 10 09 15

	10 10
	wastes from casting of non-ferrous pieces

	10 10 03
	furnace slag

	10 10 06
	casting cores and moulds which have not undergone pouring, other than those mentioned in 10 10 05

	10 10 08
	casting cores and moulds which have undergone pouring, other than those mentioned in 10 10 07

	10 10 10
	flue-gas dust other than those mentioned in 10 10 09

	10 10 12
	other particulates other than those mentioned in 10 10 11

	10 10 14
	waste binders other than those mentioned in 10 10 13

	10 10 16
	waste crack-indicating agent other than those mentioned in 10 10 15

	10 11
	wastes from manufacture of glass and glass products

	10 11 03
	waste glass-based fibrous materials

	10 11 05
	particulates and dust

	10 11 10
	waste preparation mixture before thermal processing, other than those mentioned in 10 11 09

	10 11 12
	waste glass other than those mentioned in 10 11 11

	10 11 14
	glass-polishing and -grinding sludge other than those mentioned in 10 11 13

	10 11 16
	solid wastes from flue-gas treatment other than those mentioned in 10 11 15

	10 11 18
	sludges and filter cakes from flue-gas treatment other than those mentioned in 10 11 17

	10 11 20
	solid wastes from on-site effluent treatment other than those mentioned in 10 11 19

	10 12
	wastes from manufacture of ceramic goods, bricks, tiles and construction products

	10 12 01
	waste preparation mixture before thermal processing

	10 12 03
	particulates and dust

	10 12 05
	sludges and filter cakes from gas treatment

	10 12 06
	discarded moulds

	10 12 08
	waste ceramics, bricks, tiles and construction products (after thermal processing)

	10 12 10
	solid wastes from gas treatment other than those mentioned in 10 12 09

	10 12 12
	wastes from glazing other than those mentioned in 10 12 11

	10 12 13
	sludge from on-site effluent treatment

	10 13
	wastes from manufacture of cement, lime and plaster and articles and products made from them

	10 13 01
	waste preparation mixture before thermal processing

	10 13 04
	wastes from calcination and hydration of lime

	10 13 06
	particulates and dust (except 10 13 12 and 10 13 13)

	10 13 07
	sludges and filter cakes from gas treatment

	10 13 13
	solid wastes from gas treatment other than those mentioned in 10 13 12

	10 13 14
	waste concrete and concrete sludge

	11
	Wastes from chemical surface treatment and coating of metals and other materials; non-ferrous hydro-metallurgy

	11 01
	wastes from chemical surface treatment and coating of metals and other materials (for example galvanic processes, zinc coating processes, pickling processes, etching, phosphating, alkaline degreasing, anodising)

	11 01 10
	sludges and filter cakes other than those mentioned in 11 01 09

	11 01 14
	degreasing wastes other than those mentioned in 11 01 13

	11 02
	wastes from non-ferrous hydrometallurgical processes

	11 02 03
	wastes from the production of anodes for aqueous electrolytical processes

	11 02 06
	wastes from copper hydrometallurgical processes other than those mentioned in 11 02 05

	11 05
	wastes from hot galvanising processes

	11 05 01
	hard zinc

	11 05 02
	zinc ash

	12
	Wastes from shaping and physical and mechanical surface treatment of metals and plastics

	12 01
	wastes from shaping and physical and mechanical surface treatment of metals and plastics

	12 01 01
	ferrous metal filings and turnings

	12 01 02
	ferrous metal dust and particles

	12 01 03
	non-ferrous metal filings and turnings

	12 01 04
	non-ferrous metal dust and particles

	12 01 05
	plastics shavings and turnings

	12 01 13
	welding wastes

	12 01 15
	machining sludges other than those mentioned in 12 01 14

	12 01 17
	waste blasting material other than those mentioned in 12 01 16

	12 01 21
	spent grinding bodies and grinding materials other than those mentioned in 12 01 20

	15
	Waste packaging, absorbents, wiping cloths, filter materials and protective clothing not otherwise specified

	15 01
	packaging (including separately collected municipal packaging waste)

	15 01 01
	paper and cardboard packaging

	15 01 02
	plastic packaging

	15 01 03
	wooden packaging

	15 01 04
	metallic packaging

	15 01 05
	composite packaging

	15 01 06
	mixed packaging

	15 01 07
	glass packaging

	15 01 09
	textile packaging

	15 02
	absorbents, filter materials, wiping cloths and protective clothing

	15 02 03
	absorbents, filter materials, wiping cloths and protective clothing other than those mentioned in 15 02 02

	16
	Wastes not otherwise specified in the list

	16 01
	end-of-life vehicles from different means of transport (including off-road machinery) and wastes from dismantling of end-of-life vehicles and vehicle maintenance (except 13, 14, 16 06 and 16 08)

	16 01 03
	end-of-life tyres

	16 01 12
	brake pads other than those mentioned in 16 01 11

	16 01 17
	ferrous metal

	16 01 18
	non-ferrous metal

	16 01 19
	plastic

	16 01 20
	glass

	16 02
	wastes from electrical and electronic equipment

	16 02 14
	discarded equipment other than those mentioned in 16 02 09 to 16 02 13

	16 02 16
	components removed from discarded equipment other than those mentioned in 16 02 15

	16 03
	off-specification batches and unused products

	16 03 04
	inorganic wastes other than those mentioned in 16 03 03

	16 03 06
	organic wastes other than those mentioned in 16 03 05

	16 08
	spent catalysts

	16 08 01
	spent catalysts containing gold, silver, rhenium, rhodium, palladium, iridium or platinum (except 16 08 07)

	16 08 03
	spent catalysts containing transition metals or transition metal compounds not otherwise specified

	16 11
	waste linings and refractories

	16 11 02
	carbon-based linings and refractories from metallurgical processes others than those mentioned in 16 11 01

	16 11 04
	other linings and refractories from metallurgical processes other than those mentioned in 16 11 03

	16 11 06
	linings and refractories from non-metallurgical processes others than those mentioned in 16 11 05

	17
	Construction and demolition wastes (including excavated soil from contaminated sites)

	17 01
	concrete, bricks, tiles and ceramics

	17 01 01
	concrete

	17 01 02
	bricks

	17 01 03
	tiles and ceramics

	17 01 07
	mixtures of concrete, bricks, tiles and ceramics other than those mentioned in 17 01 06

	17 02
	wood, glass and plastic

	17 02 01
	wood

	17 02 02
	glass

	17 02 03
	plastic

	17 03
	bituminous mixtures, coal tar and tarred products

	17 03 02
	bituminous mixtures other than those mentioned in 17 03 01

	17 04
	metals (including their alloys)

	17 04 01
	copper, bronze, brass

	17 04 02
	aluminium

	17 04 03
	lead

	17 04 04
	zinc

	17 04 05
	iron and steel

	17 04 06
	tin

	17 04 07
	mixed metals

	17 04 11
	cables other than those mentioned in 17 04 10

	17 05
	soil (including excavated soil from contaminated sites), stones and dredging spoil

	17 05 04
	soil and stones other than those mentioned in 17 05 03

	17 05 06
	dredging spoil other than those mentioned in 17 05 05

	17 05 08
	track ballast other than those mentioned in 17 05 07

	17 09
	other construction and demolition wastes

	17 09 04
	mixed construction and demolition wastes other than those mentioned in 17 09 01, 17 09 02 and 17 09 03

	18
	Wastes from human or animal health care and/or related research (except kitchen and restaurant wastes not arising from immediate health care)

	18 01
	wastes from natal care, diagnosis, treatment or prevention of disease in humans

	18 01 04
	wastes whose collection and disposal is not subject to special requirements in order to prevent infection (for example dressings, plaster casts, linen, disposable clothing, diapers)

	18 02
	wastes from research, diagnosis, treatment or prevention of disease involving animals

	18 02 03
	wastes whose collection and disposal is not subject to special requirements in order to prevent infection

	18 02 06
	chemicals other than those mentioned in 18 02 05

	19
	Wastes from waste management facilities, off-site waste water treatment plants and the preparation of water intended for human consumption and water for industrial use

	19 01
	wastes from incineration or pyrolysis of waste

	19 01 02
	ferrous materials removed from bottom ash

	19 01 12
	bottom ash and slag other than those mentioned in 19 01 11

	19 01 14
	fly ash other than those mentioned in 19 01 13

	19 01 16
	boiler dust other than those mentioned in 19 01 15

	19 01 18
	pyrolysis wastes other than those mentioned in 19 01 17

	19 01 19
	sands from fluidised beds

	19 02
	wastes from physico/chemical treatments of waste (including dechromatation, decyanidation, neutralisation)

	19 02 03
	premixed wastes composed only of non-hazardous wastes

	19 02 06
	sludges from physico/chemical treatment other than those mentioned in 19 02 05

	19 03
	stabilised/solidified wastes

	19 03 05
	stabilised wastes other than those mentioned in 19 03 04

	19 03 07
	solidified wastes other than those mentioned in 19 03 06

	19 04
	vitrified waste and wastes from vitrification

	19 04 01
	vitrified waste

	19 05
	wastes from aerobic treatment of solid wastes

	19 05 01
	non-composted fraction of municipal and similar wastes

	19 05 02
	non-composted fraction of animal and vegetable waste

	19 05 03
	off-specification compost

	19 06
	wastes from anaerobic treatment of waste

	19 06 04
	digestate from anaerobic treatment of municipal waste

	19 06 06
	digestate from anaerobic treatment of animal and vegetable waste

	19 08
	wastes from waste water treatment plants not otherwise specified

	19 08 01
	screenings

	19 08 02
	waste from desanding

	19 08 05
	sludges from treatment of urban waste water

	19 08 09
	grease and oil mixture from oil/water separation containing only edible oil and fats

	19 08 12
	sludges from biological treatment of industrial waste water other than those mentioned in 19 08 11

	19 08 14
	sludges from other treatment of industrial waste water other than those mentioned in 19 08 13

	19 09
	wastes from the preparation of water intended for human consumption or water for industrial use

	19 09 01
	solid waste from primary filtration and screenings

	19 09 02
	sludges from water clarification

	19 09 03
	sludges from decarbonation

	19 09 04
	spent activated carbon

	19 09 05
	saturated or spent ion exchange resins

	19 09 06
	solutions and sludges from regeneration of ion exchangers

	19 10
	wastes from shredding of metal-containing wastes

	19 10 01
	iron and steel waste

	19 10 02
	non-ferrous waste

	19 10 04
	fluff-light fraction and dust other than those mentioned in 19 10 03

	19 10 06
	other fractions other than those mentioned in 19 10 05

	19 11
	wastes from oil regeneration

	19 11 06
	sludges from on-site effluent treatment other than those mentioned in 19 11 05

	19 12
	wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified

	19 12 01
	paper and cardboard

	19 12 02
	ferrous metal

	19 12 03
	non-ferrous metal

	19 12 04
	plastic and rubber

	19 12 05
	glass

	19 12 07
	wood other than that mentioned in 19 12 06

	19 12 08
	textiles

	19 12 09
	minerals (for example sand, stones)

	19 12 10
	combustible waste (refuse derived fuel)

	19 12 12
	other wastes (including mixtures of materials) from mechanical treatment of wastes other than those mentioned in 19 12 11

	19 13
	wastes from soil and groundwater remediation

	19 13 02
	solid wastes from soil remediation other than those mentioned in 19 13 01

	19 13 04
	sludges from soil remediation other than those mentioned in 19 13 03

	19 13 06
	sludges from groundwater remediation other than those mentioned in 19 13 05

	20
	Municipal wastes (household waste and similar commercial, industrial and institutional wastes) including separately collected fractions

	20 01
	separately collected fractions (except 15 01)

	20 01 01
	paper and cardboard

	20 01 02
	glass

	20 01 08
	biodegradable kitchen and canteen waste

	20 01 10
	clothes

	20 01 11
	textiles

	20 01 25
	edible oil and fat

	20 01 28
	paint, inks, adhesives and resins other than those mentioned in 20 01 27

	20 01 30
	detergents other than those mentioned in 20 01 29

	20 01 36
	discarded electrical and electronic equipment other than those mentioned in 20 01 21, 20 01 23 and 20 01 35

	20 01 38
	wood other than that mentioned in 20 01 37

	20 01 39
	plastics

	20 01 40
	metals

	20 01 41
	wastes from chimney sweeping

	20 02
	garden and park wastes (including cemetery waste)

	20 02 01
	biodegradable waste

	20 02 02
	soil and stones

	20 02 03
	other non-biodegradable wastes

	20 03
	other municipal wastes

	20 03 01
	mixed municipal waste

	20 03 02
	waste from markets

	20 03 03
	street-cleaning residues

	20 03 04
	septic tank sludge

	20 03 06
	waste from sewage cleaning

	20 03 07
	bulky waste



	Table S2.1A Waste types previously permitted for disposal – Phase 1

	 Description

	Contaminated land 

	Sewage sludge

	Filter cake

	Asbestos

	Slag (including boiler or flue cleaning)

	Mineral processing wastes

	Silt and dredgings

	Contaminated water

	Scrap rubber (including tyres)

	Fats, waxes and greases

	Contaminated rubbish

	Empty used containers

	Industrial effluent treatment sludges

	Interceptor pit wastes

	Paint waste

	Tannery and fellmongers waste

	Waste treated timber

	Soap and detergents

	Animal processing wastes

	Food processing wastes 

	Glue wastes



	Table S2.2 Permitted waste types for waste recovery

	Waste code
	Description 

	01
	Wastes resulting from exploration, mining, quarrying, and physical and chemical treatment of minerals

	01 01 
	wastes from mineral excavation

	01 01 02
	Wastes from non metalliferous excavation

	01 04
	wastes from physical and chemical processing of non-metalliferous minerals

	01 04 08 
	waste gravel and crushed rocks other than those containing dangerous substances

	01 04 09
	waste sand and clays

	02
	Wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing, food preparation and processing 

	02 04
	Wastes from sugar processing

	02 04 01
	soil from cleaning and washing beet

	10
	Wastes from thermal processes

	 10 12
	wastes from manufacture of ceramic goods, bricks, tiles and construction products

	 10 12 08 
	Waste ceramics, bricks, tiles and construction products (after thermal processing)

	17
	Construction and demolition wastes

	17 01
	concrete, bricks, tiles and ceramics

	17 01 01
	concrete

	17 01 02
	bricks

	17 01 03
	  tiles and ceramics 

	17 01 07
	mixtures of concrete, bricks, tiles and ceramics

	17 03
	bituminous mixtures, coal tar and tarred products

	17 03 02
	Road base and road planings other than those containing coal tar

	17 05 
	soil (including excavated soil from contaminated sites), stones and dredging spoil

	17 05 04
	Soil and stones (topsoil, peat, subsoil and stones)

	17 05 08
	Track ballast, soil and stones other than those containing dangerous substances

	19
	Wastes from waste management facilities, off-site waste water treatment plants and the preparation of water intended for human consumption and water for industrial use

	19 12
	wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified

	  19 12 09
	Minerals (such as sand and stones) from the treatment of waste aggregates that are otherwise naturally occurring minerals. This excludes fines from treatment of any non-hazardous waste or gypsum from recovered plasterboard or residual fines from mechanical treatment of mixed waste at transfer stations

	  19 12 12
	Crushed bricks, tiles, concrete and ceramics, including mixtures of materials. This excludes metal from reinforced concrete and fines from treatment of any non-hazardous waste or gypsum from recovered plasterboard or residual fines from mechanical treatment of mixed waste at transfer stations



	Table S2.3 Permitted waste types for disposal in the asbestos cell Note 1

	Waste code
	Description

	16
	Wastes not otherwise specified in the list

	16 01
	end-of-life vehicles from different means of transport (including off-road machinery) and wastes from dismantling of end-of-life vehicles and vehicle maintenance (except 13, 14, 16 06 and 16 08)

	16 01 11*
	Brake pads containing asbestos 

	17
	Construction and demolition wastes (including excavated soil from contaminated sites)

	17 06
	insulation materials and asbestos-containing construction materials

	17 06 01*
	insulation materials containing asbestos

	17 06 05*
	construction materials containing asbestos


Note 1: Asbestos wastes only permitted once pre-operational measures for future development references 6, 9a and 9b have been satisfied and agreed in writing with Natural Resources Wales
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Schedule 3 – Emissions and monitoring
	[bookmark: _Hlk220763729]Table S3.1  Leachate level limits and monitoring requirements

	Monitoring point reference/ Description
	Limit 
	Monitoring frequency
	Monitoring standard and method

	LE1, LE2, LE3, LE4, LE5, LE6, LW1, LW2, LW4, LD3, Cell 11 Sump E, Cell 11 Sump W, , Cell 13 Sump 1, Cell 13 Sump 2, Cell 14 Sump, Cell 15 Sump 
LMV1, LMV2, LM1, LM2, LM3(S), LM3(N), LM4, LM5, L4, L5, C4NLM1, C4NLM2, C5SLM1, C5NLM1, C5NLM2, C4/5SLM1, C4/5SLM2, C6LM1, C7LM1 and C8LM1

as shown on drawing titled “Leachate Monitoring Wells” (drawing number 2365/11, dated 10/2025) or any updated drawing as agreed in writing with Natural Resources Wales.

	1m above the cell basal liner

	Monthly

Must revert to Weekly if any  section of the cap is temporarily removed. 


 
	As specified in Monitoring of landfill leachate, groundwater and surface water: LFTGN 02 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.  

Or as otherwise agreed with Natural Resources Wales as part of a leachate monitoring plan.


	C9ALM1, C9BLM1, C9CLM1, C10ALM1 and C10BLM1 
	1m above the cell basal liner
	Weekly reducing to Monthly following capping of the entire cell. 

Must revert to Weekly if any  section of the cap is temporarily removed
	

	All subsequent new leachate monitoring points within cells constructed in Phase 3 and any additional monitoring points agreed in writing with Natural Resources Wales.


	1m above the cell basal liner
	Weekly reducing to Monthly following capping of the entire cell. 

Must revert to Weekly if any  section of the cap is temporarily removed
	



	Table S3.2  Point source emissions to air – emission limits and monitoring requirements

	Emission point Ref. & Location
	Parameter  
	Source
	Limit (including unit) 
	Reference Period
	Monitoring Frequency
	Monitoring Standard or Method

	Engine Exhaust 1 and Engine Exhaust 2 ( locations as outlined in RML letter (dated 2nd Oct 2007) and identified on Drawing reference: SN103/AB/004 (dated September 2007
	Oxides of Nitrogen (NOx)
	Gas Utilisation Plant
	500 mg/m3 
	Hourly mean
	Annually
	In accordance with Monitoring landfill gas engine emissions: LFTGN 08 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales

	
	Carbon Monoxide (CO)
	
	1400 mg/m3
	
	
	

	
	Total VOCs
	
	1000 mg/m3
	
	
	

	
	Oxides of Nitrogen (NOx)
	
	No limit 
	-
	QuarterlyNote1
	Portable combustion gas analyser 

In accordance with Environment Agency document LFTGN 08 Monitoring landfill gas engine emissions: LFTGN 08 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales

	
	Carbon Monoxide (CO)
	
	No limit 
	-
	
	

	Flare Stack as identified on Drawing reference: SN103/AB/004 (dated September 2007)
	Oxides of Nitrogen
	Landfill Gas Flare
	150 mg/m3
	Hourly mean
	Annually
	In accordance with Environment Agency document LFTGN 08 Monitoring landfill gas engine emissions: LFTGN 08 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales

Monitoring is unnecessary where the flare is active for <10% of the year.


	
	Carbon Monoxide (CO)
	
	50 mg/m3
	
	
	

	
	Total VOCs
	
	10 mg/m3
	
	
	


All emissions are reported under the following conditions. Temperature 0ºC (273K), pressure 101.3 kPa and oxygen 5% dry gas.
Note 1: frequency may be increased depending on concentrations of the inlet gases and the individual engine drift rate. Testing frequency to be reviewed annually by the operator and reported to Natural Resources Wales in accordance with condition 4.2.2

	Table S3.3  Point source emissions to water (other than sewer) – emission limits and monitoring requirements

	Emission point Ref. & Location
	Parameter  
	Source
	Limit (incl unit)
	Reference Period
	Monitoring Frequency
	Monitoring Standard or Method

	D1, D2 and D3 Note 1
as shown on plan named ‘Surface Water Monitoring Points’, drawing number 2365/9r2, dated 10/2025 or any updated plan as agreed in writing with Natural Resources Wales

	pH
	
	6 to 9 (pH units)
	Spot Sample
	Monthly
	In accordance with Environment Agency document LFTGN02 ‘Guidance on Monitoring of Landfill Leachate, Groundwater and Surface Water’ (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.

	
	Total Suspended solids
	
	30 (mg/l)
	
	
	

	
	Ammoniacal Nitrogen
	
	0.5 (mg/l)
	
	
	

	
	Biological Oxygen Demand
	
	17 (mg/l)
	
	
	

	
	Chemical Oxygen Demand
	
	150(mg/l)
	
	
	

	
	Chloride
	
	250 (mg/l)
	
	
	


Note 1: The limits and monitoring requirements for emission point D3 do not apply until Phase 3 is operational and pre-operational measure for future development 11 is approved by Natural Resources Wales.

	Table S3.4  Groundwater – emission limits and monitoring requirements

	Monitoring point reference
	Parameter
	Limit (including unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	BH1, BH2, BH3, BH4, BH5, BH6, BH8, BH12, BH29, BH30, BH33, TP9, TP11, TP12 and BH104

as shown on drawing titled “Groundwater Monitoring Wells” (document reference 2365/10r2, dated 10/2025) or any updated plan as agreed in writing with Natural Resources Wales 
	Ammoniacal Nitrogen
	12.0 mg/l
	Spot Sample
	Monthly 
	As specified in Environment Agency Guidance Monitoring of landfill leachate, groundwater and surface water: LFTGN 02 - GOV.UK  or such other subsequent guidance as may be agreed in writing with Natural Resources Wales



	
	Chloride
	500.0 mg/l
	
	
	

	
	Nickel 
	0.05 mg/l Note 1
	
	Quarterly
	

	
	Phenol
	0.15 mg/l Note 1
	
	
	

	
	Cadmium
	0.0095 mg/l Note 1
	
	
	

	
	Mecoprop
	0.018 mg/l
	
	
	

	
	Naphthalene
	0.002 mg/l
	
	
	

	
	Electrical Conductivity
	No limit
	
	
	


Note 1: Or other limit(s) as agreed in writing with Natural Resources Wales following the approval of Improvement Condition 23
	Table S3.5  Landfill gas in external monitoring boreholes – limits and monitoring requirements

	Monitoring point Ref. /description
	Parameter
	Limit 
(including units) 
	Monitoring frequency
	Monitoring standard or method

	BH24G, BH25G, BH26G, GW1G, BH27G, BH28G, TP10G, TP9G, TP11G, TP12G, BH104G, BH10G,    BH33G, BH11G, BH12G, BH13G, BH14G, BH15G, BH16G, BH17G, BH19AG, BH1G, BH2G, BH3G, BH4G, BH5G, BH6G, BH30G
as shown on drawing titled “Perimeter Gas Wells” (document reference 2365/12, dated 10/2025) or any updated plan as agreed in writing with Natural Resources Wales
	Methane
	1.2% v/v
	Monthly
	As specified in Environment Agency Guidance Management of landfill gas: LFTGN 03 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.

Record whether the ground is:
· waterlogged
· frozen 
· snow covered


	
	Oxygen
	No limit
	
	

	
	Carbon Dioxide 
	No limit
	
	

	
	Hydrogen Sulphide
	No limit
	
	

	
	Atmospheric pressure
	No limit 
	
	

	
	Differential Pressure
	No limit 
	
	

	
	Groundwater levels 
	No limit
	
	







	Table S3.6 Point source emissions to sewer, effluent treatment plant or by tankering or other transfer off-site – emission limits and monitoring requirements

	Emission point Ref. & Location
	Parameter  
	Source
	Limit (including unit)
	Reference Period
	Monitoring Frequency
	Monitoring Standard or Method

	Leachate storage tanks as identified on drawing reference: Wth-SPMP-0608, dated: 2008

	Volume transferred off-site
	Leachate from the permitted landfill
	No limit
	Spot sample
	Volume of each load shall be recorded
	-



	Table S3.7 Landfill gas emissions from capped surfaces for cells that have accepted non hazardous biodegradable waste – monitoring requirements 

	Monitoring point Ref. /description
	Parameter
	Monitoring frequency
	Monitoring Standard or method
	Other specification

	Permanently capped zone
	Average methane flux and total methane emission 
	Every 12 months Note 1 
	Flame ionisation detector walkover, flux  box or as otherwise agreed in writing with  Natural Resources Wales.

As specified in Environment Agency Guidance Monitoring landfill gas surface emissions: LFTGN 07 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.
	Where the average zone emission rate of 0.001 mg/m2 /second is exceeded appropriate measures must be taken to reduce the rate.

	Temporarily capped zone
	
	
	
	Where the average zone emission rate of 0.1 mg/m2 /second is exceeded appropriate measures must be taken to reduce the rate.


Note 1: If a cap has previously been shown compliant and there have been no significant physical changes in the gas management during the year, a detailed walkover survey can be used to demonstrate that the surface emissions are under control. If this survey shows no change in the pattern of methane emission, it may be used as the annual survey and the values for average methane flux and total methane emissions measured in the previous year may be reported. A quantitative survey is not necessary. If the zone remains stable, the results of a detailed walkover survey will be acceptable for the annual report for a period of four years before a further quantitative survey is required.

	Table S3.8 Groundwater – other monitoring requirements

	Monitoring Point Ref.
/Description
	Parameter
	Monitoring frequency
	Monitoring standard or method

	BH17, BH18, BH19A, BH24A, BH25, BH26 GW1, BH27, BH28, BH34, TP10, TP9, TP11, TP12, BH104, BH14, BH15, BH16, BH33, BH10, BH11, BH12, BH13, BH29, BH1, BH2, BH3, BH4, BH5, BH6, BH7, BH8, BH9, BH30, BH38


as shown on drawing titled “Groundwater Monitoring Wells” (document reference 2365/10, dated 10/2025) or any updated plans agreed in writing with Natural Resources Wales 

	Water level
	Monthly, Quarterly, Annually 
	As specified in Monitoring of landfill leachate, groundwater and surface water: LFTGN 02 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.  Or as otherwise agreed with Natural Resources Wales as part of a groundwater monitoring plan.


	
	pH
	
	

	
	Electrical conductivity 
	
	

	
	Ammoniacal Nitrogen 
	
	

	
	Chloride 
	
	

	
	Temperature
	Quarterly, Annually 
	

	
	Dissolved Oxygen
	
	

	
	Nickel (filtered) 
	
	

	
	Cadmium (filtered)
	
	

	
	Mecoprop
	
	

	
	Naphthalene
	
	

	
	Phenol
	
	

	
	Phenols (total)
	
	

	
	Copper (filtered)
	
	

	
	Calcium
	
	

	
	Magnesium 
	
	

	
	Sodium 
	
	

	
	Potassium 
	
	

	
	Total Alkalinity 
	
	

	
	Sulphates 
	
	

	
	Cyanide 
	
	

	
	Iron (filtered)
	
	

	
	Manganese (filtered)
	
	

	
	Mercury (filtered)
	
	

	
	Chromium (filtered)
	
	

	
	Lead (filtered)
	
	

	
	Zinc (filtered)
	
	

	
	Nitrate 
	
	

	
	Nitrite
	
	

	
	Hazardous Substances
	Annually 
	

	
	Base of monitoring point (mAoD)
	
	



	Table S3.9  Landfill gas – other monitoring requirements

	Monitoring Point Ref.
/Description
	Parameter
	Monitoring frequency
	Monitoring standard or method
	Other specifications

	All gas collection wells and any other (in-waste) gas monitoring points.
	Methane
	Fortnightly unless otherwise agreed in writing with Natural Resources Wales








	v/v ± 0.1% 
	Calibrated handheld monitoring instrument

	
	Carbon Dioxide
	
	v/v ± 0.1%* 
	

	
	Oxygen
	
	v/v ± 0.1%* 
	

	
	Carbon Monoxide
	
	ppm 
	

	
	Hydrogen Sulphide
	
	v/v ± 0.1%* 
	

	
	Atmospheric Pressure
	
	± 1mb* 
	

	
	Differential Pressure
	
	± 1mb* 
	

	
	% Balance Gas Note 1
	
	v/v ± 0.1%*
	

	
	Valve Settings
	
	Operational check
	Open, partially open or closed

	
	Meteorological Data
	
	As specified in Environment Agency Guidance Management of landfill gas: LFTGN 03 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.
	-

	A sample of the source gas at the inlet to the Gas Utilisation Compound

	Methane
	Fortnightly unless otherwise agreed in writing with Natural Resources Wales
	v/v ± 0.1% 
	Calibrated handheld monitoring instrument

	
	Carbon Dioxide
	
	v/v ± 0.1%* 
	

	
	Oxygen
	
	v/v ± 0.1%* 
	

	
	Carbon Monoxide
	
	ppm 
	

	
	Hydrogen sulphide
	
	v/v ± 0.1%* 
	

	
	Atmospheric pressure
	
	± 1mb* 
	

	
	Differential pressure
	
	± 1mb* 
	

	
	% Balance Gas Note 1
	
	v/v ± 0.1%*
	

	
	Gas Flow
	
	± 1m3/hr
	

	
	Meteorological Data
	
	As specified in Environment Agency Guidance Management of landfill gas: LFTGN 03 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.
	-

	
	Trace Gas 
	Annually 
	Trace gas analysis in accordance with Monitoring trace components in landfill gas: LFTGN 04 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales [or a trace gas characterisation method agreed with Natural Resources Wales].
	The concentration of trace gas components shall be assessed against the assumptions made in the Landfill gas risk assessment and dispersion modelling.

	Flare Stack as identified on Drawing reference: SN103/AB/004 (dated September 2007)
	Temperature
	Daily 
(when operational)
	Spot Reading

	As specified in Monitoring enclosed landfill gas flares: LFTGN 05  (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.


Note 1: Calculated as the difference between the sum of measured gases and 100%






	Table S3.10 Leachate – other monitoring requirements

	Monitoring point reference or description
	Parameter
	Monitoring frequency
	Monitoring standard or method

	All leachate monitoring wells and sumps.
	Depth to base(mAoD)
	Annually 
	

	LW1, LW2, LW4, LE1, LE6, LD3, Cell 11 Sump W, Cell11 Sump E, Cell 13 Sump 1, Cell 13 Sump 2, Cell 14 Sump, Cell 15 Sump.

as shown on drawing titled “Leachate Monitoring Wells” (drawing number 2365/11, dated 10/2025) or any updated drawing as agreed in writing with Natural Resources Wales.

	pH
	 
 Annually 
	As specified in Monitoring of landfill leachate, groundwater and surface water: LFTGN 02 - GOV.UK (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.  Or as otherwise agreed with Natural Resources Wales as part of a leachate monitoring plan.


	
	Electrical Conductivity
	
	

	
	Temperature
	
	

	
	Dissolved Oxygen
	
	

	
	Ammoniacal Nitrogen
	
	

	
	Chloride
	
	

	
	Nickel (filtered) 
	
	

	
	Cadmium (filtered)
	
	

	
	Mecoprop
	
	

	
	Naphthalene
	
	

	
	Phenol
	
	

	
	Phenols (total)
	
	

	
	Copper (filtered)
	
	

	
	Calcium
	
	

	
	Magnesium 
	
	

	
	Sodium 
	
	

	
	Potassium 
	
	

	
	Total Alkalinity 
	
	

	
	Sulphates 
	
	

	
	Cyanide 
	
	

	
	Iron (filtered)
	
	

	
	Manganese (filtered)
	
	

	
	Mercury (filtered)
	
	

	
	Chromium (filtered)
	
	

	
	Lead (filtered)
	
	

	
	Zinc (filtered)
	
	

	
	Nitrate 
	
	

	
	Nitrite
	
	

	
	Hazardous substances
	Once every 2 years
	

	LV1, LV2, LV3, LV4, L1, L2, L3, C4NL1, C5NL1, C5NL2, C6L1, C7L1, C8L1, C9AL1, C9BL1, C9CL1 and C10AL1, C10BL1

as shown on drawing titled “Leachate Monitoring Wells” (drawing number 2365/11, dated 10/2025) or any updated drawing as agreed in writing with Natural Resources Wales.

All subsequent new leachate sumps within cells constructed in Phase 3. 









	Leachate level
	Quarterly
	

	
	pH
	Once every 6 months

	

	
	Electrical Conductivity
	
	

	
	Temperature
	
	

	
	Dissolved Oxygen
	
	

	
	Ammoniacal Nitrogen
	
	

	
	Chloride
	
	

	
	Nickel (filtered) 
	
	

	
	Cadmium (filtered)
	
	

	
	Mecoprop
	
	

	
	Naphthalene
	
	

	
	Phenol
	
	

	
	Phenols (total)
	
	

	
	Copper (filtered)
	
	

	
	Calcium
	
	

	
	Magnesium 
	
	

	
	Sodium 
	
	

	
	Potassium 
	
	

	
	Total Alkalinity 
	
	

	
	Sulphates 
	
	

	
	Cyanide 
	
	

	
	Iron (filtered)
	
	

	
	Manganese (filtered)
	
	

	
	Mercury (filtered)
	
	

	
	Chromium (filtered)
	
	

	
	Lead (filtered)
	
	

	
	Zinc (filtered)
	
	

	
	Nitrate 
	
	

	
	Nitrite
	
	

	
	Hazardous substances
	Once every 2 years
	


	
	Table S3.11 Surface water – other monitoring requirements

	Monitoring Point Ref.
/Description
	Parameter
	Monitoring frequency
	Monitoring standard or method
	Other specifications

	SP1, SP3, SP5, SP7, SP9, 

as shown on drawing titled “Surface Water Monitoring Points” (document reference 2365/19, dated 10/2025) or any updated drawing as agreed in writing with Natural Resources Wales


	pH 
	Monthly
	Spot sample
	As specified in Environment Agency Guidance TGN02 ‘Monitoring of Landfill Leachate, Groundwater and Surface Water’ (June 2014) or such other subsequent guidance as may be agreed in writing with Natural Resources Wales.

	
	Electrical Conductivity
	
	
	

	
	Temperature
	
	
	

	
	Dissolved Oxygen  
	
	
	

	
	Ammoniacal Nitrogen
	
	
	

	
	Chloride
	
	
	

	
	Nickel (filtered) 
	
	
	

	
	Cadmium (filtered)
	
	
	

	
	Mecoprop
	
	
	

	
	Naphthalene
	
	
	

	
	Phenol
	
	
	

	
	Phenols (total)
	
	
	

	
	Biological Oxygen Demand
	
	
	

	
	Chemical Oxygen Demand 
	
	
	

	
	Phosphate
	
	
	

	
	Total Suspended Solids 
	
	
	

	
	Mercury (filtered)  
	
	
	

	D1, D2 and D3 Note 1

as shown on drawing titled “Surface Water Monitoring Points” (document reference 2365/19, dated 10/2025) or any updated drawing as agreed in writing with Natural Resources Wales

	Electrical Conductivity
	
	
	

	
	Temperature
	
	
	

	
	Dissolved Oxygen  
	
	
	

	
	Nickel (filtered) 
	
	
	

	
	Cadmium (filtered)
	
	
	

	
	Mecoprop
	
	
	

	
	Naphthalene
	
	
	

	
	Phenol
	
	
	

	
	Phenols (total)
	
	
	

	
	Phosphate
	
	
	

	
	Mercury (filtered)  
	
	
	


Note 1: The limits and monitoring requirements for emission point D3 do not apply until Phase 3 is operational and pre-operational measure for future development 11 is approved by Natural Resources Wales
	Table S3.12 Particulate matter in ambient air - monitoring requirements Note 1

	Monitoring Point Ref.
/Description
	Parameter
	Limit
	Reference Period
	Monitoring Frequency
	Monitoring Standard or Method

	20m downwind of asbestos disposal cell

	Asbestos Fibres
	Where total fibre concentration exceeds 0.01 fibres/ ml in any sample, that sample must be submitted for electron microscopy to confirm the concentration of asbestos fibres present

	2 hours
	Twice per year or every 5000 tonnes asbestos deposited, whichever is greater 
	While asbestos is being deposited.
Pumped sampling
1m above ground level
Flow rate = 4 litres/ minute
Minimum  sample volume = 480 litres
Filter pore size = 1.2µm
Asbestos fibre limit of detection = 0.001 fibres/ ml

	50m upwind of asbestos disposal cell

	Asbestos Fibres
	
	2 hours
	During all downwind monitoring  
	

	Site boundary downwind of asbestos disposal cell
	Asbestos Fibres
	
	2 hours
	Minimum twice per year  
	


Note 1: Monitoring only required when site is depositing asbestos wastes 
Schedule 4 – Reporting
	Table S4.1 Reporting of monitoring data 

	Parameter
	Reporting period
	Period ends

	Leachate level
As specified by schedule 3, table S3.1
	Every 3 months
	31 March, 30 June, 30 September, 31 December

	Point source emission to air
As specified by schedule 3, table S3.2
	Every 12 months
	31 December

	Point source emission to water (other than sewer)
As specified by schedule 3, table S3.3
	Every 3 months


	31 March, 30 June, 30 September, 31 December

	Emission to groundwater
As specified by schedule 3, table S3.4
	Every 3 months
	31 March, 30 June, 30 September, 31 December

	Landfill gas in external monitoring boreholes
As specified by schedule 3, table S3.5
	Every 3 months
	31 March, 30 June, 30 September, 31 December

	Emissions to sewer, effluent treatment plant or by tankering or other transfer off-site 
As specified by schedule 3, table S3.6
	Every 3 months 
	31 March, 30 June, 30 September, 31 December

	Emission of landfill gas from capped surfaces 
As specified by schedule 3, table S3.7
	Every 12 months

	31 December

	Other groundwater monitoring
As specified by schedule 3, table S3.8
	Every 3 months
	31 March, 30 June, 30 September, 31 December

	Other Landfill gas monitoring
As specified by schedule 3, table S3.9

	Every 3 months


	31 March, 30 June, 30 September, 31 December

	Trace gas monitoring
	Every 12 months
	31 December

	Other leachate monitoring
As specified by schedule 3, table S3.10
	Every 12 months


	31 December


	Other surface water monitoring
As specified by schedule 3, table S3.11
	Every 12 months

	31 December

	Particulate matter in ambient air
As required by schedule 3, table S3.12
	Every 6 months Note 1

	30 June, 31 December

	Meteorological data
Landfill Directive, annex III, section 2
	Every 12 months
	31 December


* - where the reporting period is 12 months, you may submit this information as part of the ‘annual report’ required by condition 4.2.2. 
Note 1: Monitoring only required when site is depositing asbestos wastes 

	Table S4.2: Annual production/treatment

	Leachate:
Disposed of off site;
	Cubic metres/year

	Landfill gas: 
combustion in flares; 
combustion in gas engines; 
Other methods of gas utilisation.
	Normalised cubic metres/year






	Table S4.3 Performance Parameters

	Parameter
	Frequency of assessment
	Annual total
	Unit

	Energy used (including for leachate treatment)
	Annually
	
	MWh of electricity or natural gas



	Table S4.4 Reporting Forms

	Media/parameter
	Reporting Format
	

	Leachate
	Reporting format as agreed in writing with Natural Resources Wales
	

	Air
	
	

	Controlled water
	
	

	Groundwater
	
	

	Landfill gas
	
	

	Performance
	
	

	Particulate matter Note 1
	
	

	Waste Return
	E-waste Return Form
	

	Landfill topographical surveys and interpretation 

	Reporting format to be agreed in writing with Natural Resources Wales
	


Note 1: Monitoring only required when site is depositing asbestos wastes 


Schedule 5 – Notification
This page outlines the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	To be notified within 24 hours of detection

	Date and Time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a permit condition

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	



	(c) Notification requirements in the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator


Schedule 6 – Interpretation
“accident” means an accident that may result in pollution.
“annually” means once every year.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“Background concentration” means such concentration of that substance as is present in: 
For emissions to surface water, the surface water quality up-gradient of the site; or 
For emissions to sewer, the surface water quality up-gradient of the sewage treatment works discharge; or
For emissions of landfill gas, the ground or air outside the site and not attributable to the site.
(a) “Cell layout drawing” means: A drawing or drawings of the proposed new cell that illustrate(s) in sufficient detail:
the location of the new cell on the site;
the proposed level (Above Ordnance Datum) of the base of the excavation;
the proposed finished levels of all containment and leachate drainage layers;
the positions of leachate management infrastructure; and
the positions of landfill gas infrastructure (if appropriate).
A detailed written explanation of any minor design changes from the most recently approved cell that result from the new cell layout.  This would include, for example:
0. changes to slope length and gradient within the cell;
new leachate or landfill gas infrastructure construction design;
slope stability issues such as new basal excavation level; and/or
depth of waste.
“Construction Proposals” means written information, at a level of detail appropriate to the complexity and pollution risk, on the design, specifications of materials selected, stability assessment (where relevant) and the construction quality assurance (CQA) programme in relation to the New Cell or Landfill Infrastructure.
“CQA Validation Report” means the final “as built” construction and engineering details of the New Cell or of the Landfill Infrastructure.  It must provide a comprehensive record of the construction and must include, where relevant: 
The results of all testing required by the CQA programme - this must include the records of any failed tests with a written explanation, details of the remedial action taken, referenced to the appropriate secondary testing; 
Plans showing the location of all tests; 
“As-built” plans and sections of the works; 
Copies of the site engineer’s daily records; 
Records of any problems or non-compliances and the solution applied; 
Any other site specific information considered relevant to proving the integrity of the New Cell or Landfill Infrastructure; 
Validation by a qualified person that all of the construction has been carried out in accordance with the Construction Proposals.
“emissions to land” includes emissions to groundwater.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations 2010, SI 2010 No.675. Words and expressions used in this permit which are also used in those Regulations have the same meanings as in those Regulations.
[bookmark: _Toc318726385]“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission or background concentration limit.
“exceeded” means that a value is above a permitted limit, or where a range of values or a minimum value is set as a permitted limit it means a value outside that range or below the minimum value, whichever is applicable.
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
 “Hazardous substances” as defined by the Environmental Permitting (England and Wales) Regulations 2010, SI 2010 No.675, schedule 22 and listed in our Hydrogeological risk assessment guidance, annex J to our H1 risk assessment guidance.  
 “Landfill Infrastructure” means any specified element of the:
permanent capping; 
temporary capping (i.e. engineered temporary caps not cover materials); 
leachate abstraction systems; 
leachate transfer, treatment and storage systems; 
surface water drainage systems; 
leachate monitoring wells; 
groundwater monitoring boreholes; 
landfill gas monitoring boreholes; 
landfill gas management systems;
lining within the installation. 
within the site.
“Liquids” means any liquid other than leachate within the engineered landfill containment system.
“List of Wastes” means the list of wastes established by Commission Decision 2000/532/EC replacing Decision 94/3/EC establishing a list of wastes pursuant to Article 1(a) of Council Directive 75/442/EEC on waste and Council Decision 94/904/EC establishing a list of hazardous waste pursuant to Article 1(4) of Council Directive 91/689/EEC on hazardous waste, as amended from time to time.
"inert waste" means waste that does not undergo any significant physical, chemical or biological transformations. Inert waste will not dissolve, burn or otherwise physically or chemically react, biodegrade or adversely affect other matter with which it comes into contact in a way likely to give rise to environmental pollution or harm human health. The total leachability and pollutant content of the waste and the ecotoxicity of the leachate must be insignificant, and in particular not endanger the quality of surface water and/or groundwater
“Medicinal product” means any medicine licensed by the Medicines and Healthcare products Regulatory Agency (MHRA) or their predecessors under the Medicines Act 1968, section 130.
“M2” means Environment Agency Guidance Monitoring of stack emissions to air.
“New Cell” means any new cell, part of a cell or other similar new area of the site where waste deposit is to commence after issue of this permit and can comprise:
groundwater under-drainage system; 
permanent geophysical leak location system; 
leak detection layer; 
sub-grade; 
Geological barriers; 
Geosynthetic liners; 
leachate collection system; 
leachate abstraction system; 
separation bund/layer; 
cell or area surface water drainage system;
side wall subgrade and containment systems; 
for the New Cell.
[bookmark: _Toc318726386]“MEPP” Monitoring and extraction point plan, required by condition 4.2.2(h) to specify extraction points and routine monitoring locations.
“MCERTS” means Natural Resources Wales’s Monitoring Certification Scheme.
“No impact” means that the change made to the construction process will not affect the agreed design criteria, specification or performance in a way that has a negative effect.
“Pests” means Birds, Vermin and Insects.
“Pollution” means any emission as a result of human activity which may—
(a)be harmful to human health or the quality of the environment,
(b)cause offence to a human sense,
(c)result in damage to material property, or
(d)impair or interfere with amenities or other legitimate uses of the environment;
“Previous year” means the 12 month period preceding the month the annual report is submitted in.
[bookmark: _Toc318726387]“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.
“Relevant waste acceptance procedures” means the procedure for the acceptance of waste at landfills and the associated sampling and test methods specified in the Council Decision Annex (2003/33/EC, European Council of 19 December 2002).
“Relevant waste acceptance criteria” means the waste acceptance criteria and the associated sampling and test methods specified in the Council Decision Annex (2003/33/EC, European Council of 19 December 2002).
“Review of the Hydrogeological Risk Assessment” means a written review of the hydrogeological risk assessment included in the Application, together with any other parts of the Application that addressed the requirements of the EP Regulations.  The review shall assess whether the activities of disposal or tipping for the purpose of disposal of waste authorised by the permit continue to meet the requirements of the EP Regulations.
“Sustainably extracted” means where suction can be applied to the extraction wells such that a flow rate of landfill gas, with a methane content capable of either being combusted, or treated by bio-oxidation, can be extracted without increasing the risk of air ingress to the waste or inducing aerobic degradation within the waste. 
“Waste code” - See ‘List of Wastes’. 

“wastes separately collected for preparing for re-use and recycling” means any waste paper, card, cartons, metal, plastic, glass, food, small electrical and electronic equipment or textiles for landfill if that waste has been separately collected for the purposes of preparing for re-use or recycling as defined in The Prohibition on the Incineration, or the Deposit in Landfill, of Specified Waste (Wales) Regulations 2023
 
“waste wood” means any waste wood (whether or not separately collected) as per The Prohibition on the Incineration, or the Deposit in Landfill, of Specified Waste (Wales) Regulations 2023 

“WFD” means Directive 2008/98/EC of the European Parliament and of the Council of 19 November 2008 on waste [and repealing certain Directives] – the Waste Framework Directive.
Unless otherwise stated, any references in this permit to concentrations of substances in emissions into air means the standards included in Environment Agency Guidance for Monitoring Enclosed Landfill Gas Flares LFTGN 05 or Guidance for Monitoring Landfill Gas Engine Emissions LFTGN 08.
Where the following terms appear in the waste code list in Tables S2.1, S2.2. or S2.3, they have the meaning given below:

“hazardous substance” means a substance classified as hazardous as a consequence of fulfilling the criteria laid down in parts 2 to 5 of Annex I to Regulation (EC) No 1272/2008;

“heavy metal” means any compound of antimony, arsenic, cadmium, chromium (VI), copper, lead, mercury, nickel, selenium, tellurium, thallium and tin, as well as these materials in metallic form, as far as these are classified as hazardous substances;

“polychlorinated biphenyls and polychlorinated terphenyls” (“PCBs”) means PCBs as defined in Article 2(a) of Council Directive 96/59/EC’. 
Article 2(a) says that ‘PCBs’ means:
· polychlorinated biphenyls
· polychlorinated terphenyls
· monomethyl-tetrachlorodiphenyl methane, Monomethyl-dichloro-diphenyl methane, Monomethyldibromo-diphenyl methane
· any mixture containing any of the above mentioned substances in a total of more than 0,005 % by weight;

“transition metals” means any of the following metals: any compound of scandium, vanadium, manganese, cobalt, copper, yttrium, niobium, hafnium, tungsten, titanium, chromium, iron, nickel, zinc, zirconium, molybdenum and tantalum, as well as these materials in metallic form, as far as these are classified as hazardous substances;

“stabilisation” means processes which change the hazardousness of the constituents in the waste and transform hazardous waste into non-hazardous waste;

“solidification” means processes which only change the physical state of the waste by using additives without changing the chemical properties of the waste;

“year” means calendar year ending 31 December
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