Schedule 5 - Notification                            TIR0323 14/07/2026

Part A 
	Permit Number
	VP3935AT

	Name of Operator
	Enovert South Ltd

	Location of Installation
	Tir John Landfill, Wern Terrace, Off Fabian Way, Swansea, SA1 8PA

	Time and date of the detection 
	June 2026

	(b) Notification requirements for the breach of a limit (within 24 hours unless otherwise agreed)

	Emission point reference/ source
	Phase 2 LEW Leachate Wells
Leachate Head above Cell Base
>1m
See Table 1 Below


	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	Leachate remains contained within the engineered containment system, so no emission from the site is occurring.


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Leachate removal to sewer is ongoing. 
A Leachate Action Plan was submitted to NRW on 30th August 2025 which provides a wealth of detail about our investigations and planned further actions. An update was submitted on 8th May 2026 which demonstrates a general improvement and downward trend of leachate heads across the site.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Landfill capping works are now fully completed across the site, which reduce rainfall infiltration and leachate generation rates.
We may experience new fluctuations across leachate levels as the site settles. It is unlikely that all the dipped levels are representative of the actual leachate levels in the waste mass. It is likely that as the waste ages and compresses, the pore spaces are reduced, and liquid is effectively squeezed out into the wells.
Pumping, capping and drainage methods have impacted average leachate heads across the site, which appear to be following an overall continuous downward trend year on year.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The blocked or elevated levels recorded in wells LEW09b and 15a are due to well or pump clogging issues, due to the presence of the solidifying jelly-like substance. Having commissioned Ayesa to undertake some work on the jelly it is clear that a single method is not going to resolve the issue for the widespread impact however we have subsequently installed a macerator pump down LEW14 which is currently proving successful in clearing the liquid below in that well. Unfortunately, the size limits its use in some of the other affected wells and alternative pumps are being reviewed. LAP update has been submitted.  

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	See previous notifications.


	Name*
	Michelle Preston

	Post
	Environmental Data Analyst

	Date
	14/07/2026


[bookmark: _Int_iiKeGdxg]* authorised to sign on behalf of Enovert South Ltd

	Sample Point
	Date
	Leachate Head (m)
	Comment

	LEW07
	30/06/2026
	1.04
	

	LEW12a
	30/06/2026
	3.03
	

	LEW15A
	30/06/2026
	13.02
	Site investigating

	LEW20
	30/06/2026
	1.31
	

	LEW21
	30/06/2026
	1.07
	

	LEW23
	30/06/2026
	3.39
	

	LEW24
	30/06/2026
	2.57
	

	LEW25
	30/06/2026
	1.36
	

	LEW26
	30/06/2026
	1.42
	

	LEW28
	30/06/2026
	1.98
	

	LEW29
	30/06/2026
	1.09
	

	LEW31
	30/06/2026
	1.72
	

	LEW32
	30/06/2026
	3.06
	

	LEW33
	30/06/2026
	8.69
	Site investigating

	LEW34
	30/06/2026
	4.34
	Site investigating


Table 1: Breach of Compliance Limit for Leachate Boreholes Phase 2 area - June 2026



