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Notice of variation and consolidation with introductory note
The Environmental Permitting (England & Wales) Regulations 2016	

Dŵr Cymru Cyfyngedig

Llanfaethlu Wastewater Treatment Works
Llanfaethlu
Holyhead
Anglesey
LL65 4NW 

Variation number
PAN-033432
Permit number
CG0110201


Llanfaethlu Wastewater Treatment Works
Permit Number CG0110201
Introductory note
This introductory note does not form a part of the permit

The following notice gives notice of the variation and consolidation of an environmental permit.

The permit has been varied to include the addition iron limits. 

The schedules specify the changes made to the permit.

The status log of the permit sets out the permitting history, including any changes to the permit reference number. It is not backdated before 6th April 2010.

	Status log of the permit

	Description
	Date
	Comments

	Application PAN-002302
	Duly made 
30/01/2018
	Application to increase the DWF 
from 21 to 80m3/day, add a storm 
tank for flows over 3 DWF to pass to 
a new reed bed, plus remove the 
grass plot.

	Variation determined  
CG0110201/V002
	25/05/2018
	Varied and consolidated permit 
issued in modern condition format.

	Application received
PAN-033432
	Duly made 
07/08/2026
	Operator initiated variation to include iron limits

	Variation Issued
CG0110201
	04/11/2026
	Varied permit issued to Dŵr Cymru Cyfyngedig.


End of Introductory Note.
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Notice of variation and consolidation 


The Environmental Permitting (England and Wales) Regulations 2016

[bookmark: _Hlt13295849]The Natural Resources Body for Wales (“Natural Resources Wales”) in exercise of its powers under regulation 20 of the Environmental Permitting (England and Wales) Regulations 2016 varies and consolidates

Permit number
CG0110201

[bookmark: _Hlk13917238]Issued to
Dŵr Cymru Cyfyngedig (“the operator”)

[bookmark: InstallationAddress21]whose registered office is
Linea 
Fortran Road 
St Mellons 
Cardiff 
CF3 0LT

company registration number 02366777

to operate a water discharge activity at
Llanfaethlu Wastewater Treatment Works
Llanfaethlu
Holyhead
Anglesey
LL65 4NW 

to the extent set out in the schedules.

The notice shall take effect from 04/11/2026
	Name
	Date

	Joanne Fitton 
	04/11/2026


Authorised on behalf of Natural Resources Wales.

Schedule 1
The following conditions were varied as a result of the application made by the operator:
Condition 3.1.4 DWF definition has changed.
Schedule 3 - Total iron limits added to table S3.1.
Schedule 4 - Total iron as Fe added in tables S4.1 and S4.2.


Schedule 2 – consolidated permit
Consolidated permit issued as a separate document. 
Variation and consolidation
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Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number
CG0110201

This is the consolidated permit referred to in the variation and consolidation notice for variation PAN-033432 authorising 

Dŵr Cymru Cyfyngedig (“the operator”)

whose registered office is
Linea 
Fortran Road 
St Mellons 
Cardiff 
CF3 0LT

company registration number 02366777

to operate a water discharge activity at
Llanfaethlu Wastewater Treatment Works
Llanfaethlu
Holyhead
Anglesey
LL65 4NW 

to the extent authorised by and subject to the conditions of this permit.

The permit variation and consolidation shall take effect from 04/11/2026

	Name
	Date

	Joanne Fitton
	04/11/2026


Authorised on behalf of Natural Resources Wales.


Conditions
Management
0. [bookmark: _Ref373938749]General management
[bookmark: _Ref373938830]The operator shall manage and operate the activity:
in accordance with a written management system that identifies and minimises risks of pollution so far as is reasonably practicable, including those risks arising from operations, maintenance, accidents, incidents, non-conformances and those drawn to the attention of the operator as a result of complaints; and
using sufficient competent persons and resources.
Records demonstrating compliance with condition 1.1.1 shall be maintained. 
Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of the permit.
Operations
Permitted activities
The only activity authorised by the permit is the activity specified in schedule 1 table S1.1.
The site 
The discharge activity shall take place at the discharge point marked on the site plan at schedule 7 to this permit, and as listed in table S3.2; and, the operating techniques that are the subject of conditions prefixed by 2.3 shall be applied at the locations shown, or otherwise described, in schedule 7.
Operating techniques
For the activity referenced in schedule 1, table S1.1 The operator shall comply with the relevant requirements of the Urban Waste Water Treatment (England and Wales) Regulations 1994.

Emissions and monitoring
[bookmark: _Hlk70518089]Emissions to water
The limits given in schedule 3 table S3.1 shall not be exceeded.
The limits in schedule 3 table S3.1 to which this condition applies may be exceeded where: in any series of samples of the discharge taken at regular but randomised intervals in any period of twelve consecutive months as listed in column 1 of schedule 3A, no more than the relevant number of samples, as listed in column 2 of schedule 3A, exceed the applicable limit for that relevant parameter.

For the emission limits in schedule 3 table S3.1 to which this condition applies, no sample of the discharge taken at a time when unusual weather conditions are adversely affecting the operation of the waste water treatment works, shall be taken into account in deciding whether or not the emission limit has been complied with.
On any occasion where unusual weather conditions adversely affect the operation of the waste water treatment works, the operator shall use its best endeavours to mitigate that adverse effect.
For any sample of the discharge taken to be considered for the purposes of (a) above, the operator shall notify Natural Resources Wales in writing within 14 days of becoming aware that an emission limit has been exceeded. That notification shall include a full description of the unusual weather conditions and their impact on the operation of the works.
0. The permitted Dry Weather Flow limit in schedule 3 table S3.1 is set at the operator’s planned annual 80% exceeded daily volume discharged. 
1. For compliance purposes an exceedance shall be recorded for a calendar year only when the limit in effect on 31 December of that calendar year is exceeded by 90% or more of the ‘good’ recorded Total Daily Volumes in that calendar year. 
1. Until 1 January 2026 
2. If an exceedance of the Dry Weather Flow limit is recorded in a calendar year then the operator shall, as soon as is practicable, investigate the reasons for the exceedance. 
2. The operator shall report the reasons for the exceedance to Natural Resources Wales and the steps that it proposes to take to restore compliance. 
2. An exceedance of the Dry Weather Flow limit shall not be recorded as a failure of the Dry Weather Flow limit in that calendar year if the operator takes appropriate steps to restore compliance. 
1. From 1 January 2026 
The limit has been complied with in an assessment calendar year unless; 
(i) the limit was exceeded in the compliance assessment calendar year and, 
(ii) two or more exceedances have occurred in the preceding 4 calendar years. 
Only exceedances from a calendar year after 31 December 2026 shall be used.
Emissions of substances not controlled by emission limits
The operator shall take appropriate measures to minimise so far as reasonably practicable the polluting effects of the emissions of substances in the discharge not controlled by emission limits (excluding odour).
Monitoring 
The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
point source emissions specified in tables S3.1 and S3.4.
inlet quality specified in tables S3.1 and S3.4.
The operator shall maintain records of all monitoring required by this permit.
Monitoring equipment, techniques, personnel and organisations employed for the emissions monitoring programme specified in condition 3.3.1 shall have either MCERTS certification or MCERTS accreditation (as appropriate), where available, unless otherwise agreed in writing by Natural Resources Wales.
Accessible monitoring points shall be provided and maintained to enable the emissions monitoring programme to be carried out at the monitoring points specified in table S3.4 of schedule 3 and shown marked on the site plan in schedule 7. 
The monitoring programme for the parameters subject to schedule 3B shall be: 
pre-scheduled to cover a calendar year and the programme recorded before the start of a calendar year sample period; and 
spot samples collected at approximately equal intervals during the year, including samples from different days of the week and different times. Approximately 10% of samples should be outside the normal sampling window which is 9am-3pm, Monday to Friday. 
After becoming aware, or following a notification that a sample has not been taken on the schedule 3B Monitoring Programme pre-scheduled date, or is lost, or a result for that sample cannot be reported, the operator shall record the details and reschedule the sample.
0. 
(a) Total Daily Volumes shall be calculated from the average of the available ‘good’ 15-minute flow readings taken from midnight to midnight where; 
Total Daily Volume (m3) = {Sum of ‘good’ readings (l/s) / number of ‘good’ readings} x {86,400 (s) /1000}. 
Where there are 87 or more ‘good’ 15-minute flow readings the Total Daily Volume shall be reported as ‘good’, where there are 1 – 86 ‘good’ readings it shall be reported as ‘suspect’ and where there are no ‘good’ readings as ‘missing’. 
(b) The operator shall record all failures of the flow measurement system and any other breaks in the flow record and the reasons for all issues, failures and breaks that lead to missing or suspect Total Daily Volume records and all steps taken to prevent a re-occurrence. 
(c) There shall be no more than 37 days and/or no more than 14 consecutive days with ‘suspect’ or ‘missing’ Total Daily Volumes in a calendar year, unless otherwise agreed in writing by Natural Resources Wales. 
(d) All 15-minute flow readings shall be flagged as ‘good’, ‘suspect’ or ‘missing’ using an appropriate methodology set out in the operator`s flow monitoring quality management system.
Information
Records
All records required to be made by schedule 3, 4 and 5 to this permit shall:
be legible;
be made as soon as reasonably practicable;
if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 10 years from the date when the records were made. 
The operator shall maintain convenient access, in either electronic or hard copy, to the records, plan and management system required to be maintained by this permit. 
Reporting
The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
Within the time period after the end of the reporting period specified in schedule 4 table S4.1 the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
in respect of the parameters and monitoring points specified in schedule 4 table S4.1;
for the reporting periods specified in schedule 4 table S4.1 and using the forms specified in schedule 4 table S4.2; and
giving the information from such results and assessments as may be required by the forms specified in those tables.
Notifications
Natural Resources Wales shall be notified as soon as reasonably practicable following detection, within the site of the regulated facility of: 
(a) any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution; and 
(b) any breach of a limit specified in schedule 3 table S3.1 (including individual exceedances of limits which are covered by condition 3.1.2).
Any other significant adverse environmental effects, which may have been caused by the activity, shall also be notified to Natural Resources Wales as soon as reasonably practicable following detection.
The information provided under condition 4.3.1 shall be supported by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling specified in schedule 3B, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules:
Where the operator is a registered company:
any change in the operator’s trading name, registered name or registered office address; and
any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
any steps taken with a view to the dissolution of the operator.
Where the operator proposes to make a change in the nature of the activity by increasing the concentration of, or the addition of, or allowing the introduction of, a substance to the activity to an extent that the operator considers could have a significant adverse environmental effect on the receiving waters, and the change is not permitted by emission limits specified within schedule 3 table S3.1 or the subject of an application for approval under the EP Regulations or under the terms of this permit:
Natural Resources Wales shall be notified in writing at least 14 days before the increase or addition or allowing the introduction; and
the notification shall contain a description of the proposed change. 
The operator shall inform Natural Resources Wales in writing of any change, or proposed change, to the population equivalent such as would make a material change to the application of the Regulations and shall, on request, inform the Natural Resources Wales in writing of the actual population equivalent.
Interpretation
In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “as soon as reasonably practicable”, in which case it may be provided by telephone.


Schedule 1 – Operations 
	Table S1.1 Activities

	Description of activity
	Limits of specified activity

	Discharge of secondary treated sewage effluent via Final Effluent Discharge Point

	Only flows in excess of 2.25 l/s will pass to the storm tank. Any overflow of the storm tank will combine with the treated final effluent which will then pass via a reed bed before being discharged at Llanfaethlu WwTW sewage effluent discharge.



	Table S1.2 Operating techniques

	Table S1.2 not in use




Schedule 2 – Waste types, raw materials and fuels
Schedule 2 not in use.


Schedule 3 – Emissions and monitoring
	Table S3.1 Point Source emissions to water (other than sewer) – emission limits and monitoring requirements

	Effluent and discharge point
	Parameter  
	Limit (including unit)
	Reference Period
	Limit of effective range
	Monitoring frequency
	Compliance Statistic

	Secondary treated sewage effluent via Final Effluent Discharge Point
	Dry weather flow
	80 m3/day

	Total daily volume 

	N/A


	Continuous
	Conditions 3.1.4 and 3.3.7 apply



	
	15-minute instantaneous or averaged flow
	No limit set. Record as l/s
	15 minute
	N/A
	Continuous
	N/A

	
	ATU-BOD as O2
	14.5 mg/l
	Instantaneous (spot sample)
	N/A
	As specified in schedule 3B
	Look up table (Conditions 3.1.2 and 3.1.3 apply)

	
	Ammoniacal nitrogen (expressed as N)
	9.5 mg/l
	Instantaneous (spot sample)
	N/A
	As specified in schedule 3B
	Look up table (Conditions 3.1.2 and 3.1.3 apply)

	
	Suspended solids (measured after drying at 105oC)
	21.5 mg/l
	Instantaneous (spot sample)
	N/A
	As specified in schedule 3B
	Look up table (Conditions 3.1.2 and 3.1.3 apply)

	
	Total iron as Fe
	4000 µg/l
	Instantaneous (spot sample)
	N/A
	As specified in schedule 3B
	Look up table (Conditions 3.1.2 and 3.1.3 apply

	
	Total iron as Fe
	8000 µg/l
	Instantaneous (spot sample)
	N/A
	As specified in schedule 3B
	Maximum (Condition 3.1.3 applies)

	
	Visible oil or grease
	No significant trace present so far as is reasonably practicable
	Instantaneous (visual examination)
	N/A
	N/A
	No significant trace (Condition 3.1.3 applies)




	Table S3.2 Discharge points

	Effluent Name
	Discharge Point
	Discharge point NGR
	Receiving water/Environment

	Secondary treated sewage effluent
	Final Effluent Discharge Point
	SH 32058 86998
	Tributary of Afon Alaw



	Table S3.3 Storm sewage discharge settings
	

	Table S3.3 not in use.



	Table S3.4 Monitoring points

	Effluent and discharge point
	Monitoring type
	Monitoring point NGR
	Monitoring point reference

	Secondary treated sewage effluent via Final Effluent Discharge Point
	Final Effluent sampling 
	SH 31802 87128
	Final Effluent Sample Point 

	
	MCERTS continuous flow monitoring
	SH 31802 87128
	MCERTS Flow Monitoring 
Point 














































Schedule 3A - Look up table
	Look up table

	[bookmark: _Hlt511551491]Number of samples taken in any period of 12 months
	Maximum number of samples permitted to exceed limit for given parameter

	4–7  
	 1

	8–16
	 2

	17–28 
	 3

	29–40 
	 4

	41–53  
	 5

	54–67  
	 6

	68–81  
	 7

	82–95 
	 8

	96–110 
	 9

	111–125  
	 10

	126–140  
	 11

	141–155  
	 12

	156–171  
	 13

	172–187 
	 14

	188–203  
	 15

	204–219  
	 16

	220–235  
	 17

	236–251 
	 18

	252–268 
	 19

	269–284  
	 20

	285–300  
	 21

	301–317 
	 22

	318–334  
	 23

	335–350 
	 24

	351–365 
	 25









Schedule 3B - OSM tier 3 sampling frequency
	Parameter
	‘Normal frequency’ of samples per year
	Reduced Sampling frequency after 12 consecutive months of numeric permit compliance, samples per year or pro rata over the remainder of a year
	On numeric limit failure return to normal frequency as soon as reasonably practicable, samples per 12 months
	Out of hours samples

	Sanitary

	24
	12
	24
	For 24 samples 2 out of hours samples per annum

	Non sanitary

	12
	12
	12
	For 12 samples 1 out of hours sample per annum




Schedule 4 – Reporting
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.
	Table S4.1 Reporting of monitoring data

	Parameter
	Monitoring point reference
	Reporting period
	Period begins

	Dry Weather Flow (daily flows total)
	MCERTS Flow Monitoring Point 
	Annually
Report to be submitted within 2 months of the end of the calendar year
	1st January

	15-minute flow
	MCERTS Flow Monitoring Point 
	Reports to be provided to Natural Resources Wales upon request 
Report to be submitted within 28 days unless otherwise specified in writing by Natural Resources Wales
	Upon request by Natural Resources Wales

	Operator Self Monitoring - ATU-BOD as O2, ammoniacal nitrogen (expressed as N), suspended solids (measured after drying at 105oC), total iron as Fe
	Final Effluent Sample Point
	Quarterly
Report to be submitted within 28 days
	1st of month

	Operator Self Monitoring
	Final Effluent Sample Point
	Annually
Report to be submitted within 2 months of the end of the calendar year
	1 January



	Table S4.2 Reporting forms

	Parameter
	Reporting format

	Dry Weather Flow (daily flows total)
	WISKI electronic format specified by Natural Resources Wales 

	15-minute flow
	WISKI electronic format specified by Natural Resources Wales

	OSM - ATU-BOD as O2, ammoniacal 
nitrogen (expressed as N), suspended 
solids (measured after drying at 
105oC), total iron as Fe
	Quarterly - Electronic format specified by Natural Resources 
Wales

	Operator Self Monitoring summary 
report
	Annually - Summary report of compliance with the monitoring 
programme specified in Table 3.1 and schedule 3B in a format 
specified by Natural Resources Wales




Schedule 5 – Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A
	Permit Number
	CG0110201

	Name of operator
	Dŵr Cymru Cyfyngedig

	Location of Facility
	Llanfaethlu Wastewater Treatment Works, Llanfaethlu, Holyhead, Anglesey, LL65 4NW 

	Time and date of the detection 
	



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution.

	To be notified within 24 hours of detection unless otherwise agreed in writing by Natural Resources Wales.

	Date and time of the event.
	

	Reference or description of the location of the event.
	

	Description of where any release into the environment took place.
	

	Substances(s) potentially released/type or nature of sewage released.
	

	Best estimate of the quantity or rate of release of substances and/or duration of discharge.
	

	Best estimate of the environmental impact of the discharge.
	

	Measures taken, or intended to be taken, to stop any emission.
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit specified in schedule 3 table S3.1 (including individual exceedances of limits which are covered by condition 3.1.2).


	The information specified below is to be notified to Natural Resources Wales as soon as reasonably practicable following detection.

	Monitoring point reference/ source
	

	Self-monitoring regime (where relevant)
	e.g. OSM

	Type of failure 
	e.g. LUT failure/LUT exceedance/upper tier/other

	Date of sample/event
	

	Parameter
	

	Result and units
	

	Limit and units
	




Part B – to be submitted as soon as reasonably practicable unless otherwise agreed in writing by Natural Resources Wales
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident/breach/exceedance.
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator


Schedule 6 – Interpretation 
“accident” means an accident that may result in pollution.
"annually" means once every year.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“Appropriate measures” for the purposes of the emission of substances not controlled by emission limits condition (condition 3.2.1) do not require the operator to undertake treatment to a level beyond that specified in schedule 1 table S1.1, or to carry out routine monitoring for substances not controlled by emission limits.
“ATU-BOD as O2” means the biochemical oxygen demand (measured after 5 days at 20°C with nitrification suppressed by the addition of allylthiourea).
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the permitted activities, which are not controlled by an emission limit.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“MCERTS” means the Environment Agency’s Monitoring Certification Scheme.
“minimum screen capacity flow” means the minimum flow passed through the screens to the outfall when the screen bypass operates. 
“Natural Resources Wales” means the Natural Resources Body for Wales established by article 3 of the Natural Resources Body for Wales (Establishment) Order 2012. The Natural Resources Body for Wales (Functions) Order 2013 transferred the relevant functions of the Countryside Council for Wales, and functions of the Environment Agency and the Forestry Commission in Wales to the Natural Resources Body for Wales.
“overflow event” any individual operation, of any duration, of the event recorder or any recorded discharge of sewage from the outfall.
“overflow setting” means the minimum flow passed forward to the continuation sewer when the overflow operates.
"quarter" means a calendar year quarter commencing on 1st January, 1st April, 1st July or 1st October.
“significant pollution” means a high level impact incident as indicated by NRW incident classification system.
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]“significant spill” any spill that has not been demonstrated to have been, or measured as being, less than 50 m3 in volume.
“unusual weather conditions” includes, but is not limited to:
· low ambient temperatures, or the freezing of mechanical equipment in the works;
· significant snow deposits;
· tidal or fluvial flooding;
· weather conditions causing unforeseen loss of power supply to the sewage treatment that could not be ameliorated by the reasonable provision and operation of standby generation facilities.
“Urban Waste Water Treatment (England and Wales) Regulations 1994 (UWWTR)” means Urban Waste Water Treatment (England and Wales) Regulations 1994 SI 2841and the words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“year” means calendar year ending 31st December.


Schedule 7 – Site plan
[image: ]
© Crown Copyright and database right 2026. Ordnance Survey licence number 100019741.
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