Permit Number: 
JP3239ST



Operator: 

The County Council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Feb 19-C…
Reporting of ……Ground Water…… monitoring for the period for … February 2019
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Feb 19
	0.07
	25
	19/02/19
	10.6



	C1


	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C1


	Nickel


	0.22 ug/l


	Feb 19
	2.0
	34
	19/02/19
	8.82



	C1


	Chloride
	TBA


	Feb 19
	31.5
	25
	19/02/19
	21.5



	C1


	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C1


	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Feb 19
	0.73
	25
	19/02/19
	10.6



	C2
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C2
	Nickel


	0.22 ug/l


	Feb 19
	1.6
	34
	19/02/19
	8.82



	C2
	Chloride


	TBA


	Feb 19
	31.2
	25
	19/02/19
	21.5



	C2
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C2
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Feb 19
	6.5
	25
	19/02/19
	10.6



	C3
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C3
	Nickel


	0.22 ug/l


	Feb 19
	2.9
	34
	19/02/19
	8.82



	C3
	Chloride


	TBA


	Feb 19
	14.00
	25
	19/02/19
	21.5



	C3
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C3
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	10.6



	C4
	Cadmium


	1 ug/l 
	Feb 19
	NO SAMPLE
	34
	19/02/19
	7.83



	C4
	Nickel


	0.22 ug/l


	Feb 19
	NO SAMPLE
	34
	19/02/19
	8.82



	C4
	Chloride


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	21.5



	C4
	MP Xylene


	1 ug/l 
	Feb 19
	NO SAMPLE
	54
	19/02/19
	

	C4
	Mecoprop


	0.1 ug/l 
	Feb 19
	NO SAMPLE
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Feb 19
	0.94
	25
	19/02/19
	10.6



	C5
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C5
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C5
	Chloride


	TBA


	Feb 19
	8.0
	25
	19/02/19
	21.5



	C5
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C5
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Feb 19
	0.55
	25
	19/02/19
	10.6



	C6
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C6
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C6
	Chloride


	TBA


	Feb 19
	3.8
	25
	19/02/19
	21.5



	C6
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C6
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Feb 19
	0.43
	25
	19/02/19
	10.6



	C8
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C8
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C8
	Chloride


	TBA


	Feb 19
	3.6
	25
	19/02/19
	21.5



	C8
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C8
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	10.6



	C10
	Cadmium


	1 ug/l 
	Feb 19
	NO SAMPLE
	34
	19/02/19
	7.83



	C10
	Nickel


	0.22 ug/l


	Feb 19
	NO SAMPLE
	34
	19/02/19
	8.82



	C10
	Chloride


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	21.5



	C10
	MP Xylene


	1 ug/l 
	Feb 19
	NO SAMPLE
	54
	19/02/19
	

	C10
	Mecoprop


	0.1 ug/l 
	Feb 19
	NO SAMPLE
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Feb 19
	11.7
	25
	19/02/19
	10.6



	C12
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C12
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C12
	Chloride


	TBA


	Feb 19
	3.2
	25
	19/02/19
	21.5



	C12
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C12
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C13
	Am Nitrogen


	TBA


	Feb 19
	9.1
	25
	19/02/19
	10.6



	C13
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C13
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C13
	Chloride


	TBA


	Feb 19
	6.1
	25
	19/02/19
	21.5



	C13
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C13
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Feb 19
	1.3
	25
	19/02/19
	10.6



	C16
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C16
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C16
	Chloride


	TBA


	Feb 19
	4.1
	25
	19/02/19
	21.5



	C16
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C16
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	10.6



	C17
	Cadmium


	1 ug/l 
	Feb 19
	NO SAMPLE
	34
	19/02/19
	7.83



	C17
	Nickel


	0.22 ug/l


	Feb 19
	NO SAMPLE
	34
	19/02/19
	8.82



	C17
	Chloride


	TBA


	Feb 19
	NO SAMPLE
	25
	19/02/19
	21.5



	C17
	MP Xylene


	1 ug/l 
	Feb 19
	NO SAMPLE
	54
	19/02/19
	

	C17
	Mecoprop


	0.1 ug/l 
	Feb 19
	NO SAMPLE
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Feb 19
	0.04
	25
	19/02/19
	10.6



	C18
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C18
	Nickel


	0.22 ug/l


	Feb 19
	1.5
	34
	19/02/19
	8.82



	C18
	Chloride


	TBA


	Feb 19
	31.5
	25
	19/02/19
	21.5



	C18
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C18
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Feb 19
	0.04
	25
	19/02/19
	10.6



	C19
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C19
	Nickel


	0.22 ug/l


	Feb 19
	1.5
	34
	19/02/19
	8.82



	C19
	Chloride


	TBA


	Feb 19
	28.8
	25
	19/02/19
	21.5



	C19
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C19
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Feb 19
	0.29
	25
	19/02/19
	10.6



	C20
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C20
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C20
	Chloride


	TBA


	Feb 19
	10.1
	25
	19/02/19
	21.5



	C20
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C20
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Feb 19
	<0.01
	25
	19/02/19
	10.6



	C21
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C21
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C21
	Chloride


	TBA


	Feb 19
	2.7
	25
	19/02/19
	21.5



	C21
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C21
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Feb 19
	<0.01
	25
	19/02/19
	10.6



	C22
	Cadmium


	1 ug/l 
	Feb 19
	<0.080
	34
	19/02/19
	7.83



	C22
	Nickel


	0.22 ug/l


	Feb 19
	<1.5
	34
	19/02/19
	8.82



	C22
	Chloride


	TBA


	Feb 19
	32.6
	25
	19/02/19
	21.5



	C22
	MP Xylene


	1 ug/l 
	Feb 19
	<1.0
	54
	19/02/19
	

	C22
	Mecoprop


	0.1 ug/l 
	Feb 19
	<0.1
	1214
	19/02/19
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………9/12/19…………..     

(Authorised to sign as representative of Operator)
