Permit Number: 
JP3239ST



Operator: 

The County Council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Jun19-C…
Reporting of ……Ground Water…… monitoring for the period for … June 2019…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Jun 19
	0.88
	25
	27/06/19
	10.6



	C1


	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C1


	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C1


	Chloride
	TBA


	Jun 19
	410
	25
	27/06/19
	21.5



	C1


	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C1


	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Jun 19
	0.70
	25
	27/06/19
	10.6



	C2
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C2
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C2
	Chloride


	TBA


	Jun 19
	37.3
	25
	27/06/19
	21.5



	C2
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C2
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Jun 19
	3.0
	25
	27/06/19
	10.6



	C3
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C3
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C3
	Chloride


	TBA


	Jun 19
	1,230
	25
	27/06/19
	21.5



	C3
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C3
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Jun 19
	NO SAMPLE
	25
	
	10.6



	C4
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	
	7.83



	C4
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	
	8.82



	C4
	Chloride


	TBA


	Jun 19
	NO SAMPLE
	25
	
	21.5



	C4
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	
	

	C4
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Jun 19
	7.5
	25
	27/06/19
	10.6



	C5
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C5
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C5
	Chloride


	TBA


	Jun 19
	2,040
	25
	27/06/19
	21.5



	C5
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C5
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Jun 19
	1.2
	25
	27/06/19
	10.6



	C6
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C6
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C6
	Chloride


	TBA


	Jun 19
	2,720
	25
	27/06/19
	21.5



	C6
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C6
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Jun 19
	2.4
	25
	27/06/19
	10.6



	C8
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C8
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C8
	Chloride


	TBA


	Jun 19
	2,950
	25
	27/06/19
	21.5



	C8
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C8
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Jun 19
	NO SAMPLE
	25
	27/06/19
	10.6



	C10
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C10
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C10
	Chloride


	TBA


	Jun 19
	NO SAMPLE
	25
	27/06/19
	21.5



	C10
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C10
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Jun 19
	24.3
	25
	27/06/19
	10.6



	C12
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C12
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C12
	Chloride


	TBA


	Jun 19
	3,030
	25
	27/06/19
	21.5



	C12
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C12
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C13
	Am Nitrogen


	TBA


	Jun 19
	8.5
	25
	27/06/19
	10.6



	C13
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C13
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C13
	Chloride


	TBA


	Jun 19
	2,448
	25
	27/06/19
	21.5



	C13
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C13
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Jun 19
	1.6
	25
	27/06/19
	10.6



	C16
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C16
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C16
	Chloride


	TBA


	Jun 19
	3,170
	25
	27/06/19
	21.5



	C16
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C16
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Jun 19
	No Sample
	25
	27/06/19
	10.6



	C17
	Cadmium


	1 ug/l 
	Jun 19
	No Sample
	34
	27/06/19
	7.83



	C17
	Nickel


	0.22 ug/l


	Jun 19
	No Sample
	34
	27/06/19
	8.82



	C17
	Chloride


	TBA


	Jun 19
	No Sample
	25
	27/06/19
	21.5



	C17
	MP Xylene


	1 ug/l 
	Jun 19
	No Sample
	54
	27/06/19
	

	C17
	Mecoprop


	0.1 ug/l 
	Jun 19
	No Sample
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Jun 19
	0.04
	25
	27/06/19
	10.6



	C18
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C18
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C18
	Chloride


	TBA


	Jun 19
	1,130
	25
	27/06/19
	21.5



	C18
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C18
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Jun 19
	0.04
	25
	27/06/19
	10.6



	C19
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C19
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C19
	Chloride


	TBA


	Jun 19
	904
	25
	27/06/19
	21.5



	C19
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C19
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Jun 19
	2.6
	25
	27/06/19
	10.6



	C20
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C20
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C20
	Chloride


	TBA


	Jun 19
	3,210
	25
	27/06/19
	21.5



	C20
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C20
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Jun 19
	0.24
	25
	27/06/19
	10.6



	C21
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C21
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C21
	Chloride


	TBA


	Jun 19
	2,670
	25
	27/06/19
	21.5



	C21
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C21
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Jun 19
	3.4
	25
	27/06/19
	10.6



	C22
	Cadmium


	1 ug/l 
	Jun 19
	
	34
	27/06/19
	7.83



	C22
	Nickel


	0.22 ug/l


	Jun 19
	
	34
	27/06/19
	8.82



	C22
	Chloride


	TBA


	Jun 19
	3,100
	25
	27/06/19
	21.5



	C22
	MP Xylene


	1 ug/l 
	Jun 19
	
	54
	27/06/19
	

	C22
	Mecoprop


	0.1 ug/l 
	Jun 19
	
	1214
	27/06/19
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date:  27/06/19

(Authorised to sign as representative of Operator)
