Permit Number: 
JP3239ST



Operator: 

The County Council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…May19-SL…
Reporting of ……LEACHATE…… monitoring for the period for …May 2019
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1


	Am Nitrogen


	1370


	May 2019
	NO SAMPLE
	678
	30/05/19
	10.6



	SL1


	Cadmium


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	7.83



	SL1


	Nickel


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	8.82



	SL1


	Chloride
	13713


	May 2019
	NO SAMPLE
	678
	30/05/19
	21.5



	SL1


	MP Xylene


	0.029


	May 2019
	NO SAMPLE
	54
	30/05/19
	

	SL1


	Mecoprop


	0.032


	May 2019
	NO SAMPLE
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen


	1370


	May 2019
	NO SAMPLE
	678
	30/05/19
	10.6



	SL2
	Cadmium


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	7.83



	SL2
	Nickel


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	8.82



	SL2
	Chloride


	13713


	May 2019
	NO SAMPLE
	678
	30/05/19
	21.5



	SL2
	MP Xylene


	0.029


	May 2019
	NO SAMPLE
	54
	30/05/19
	

	SL2
	Mecoprop


	0.032


	May 2019
	NO SAMPLE
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen


	1370


	May 2019
	NO SAMPLE
	678
	30/05/19
	10.6



	SL3
	Cadmium


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	7.83



	SL3
	Nickel


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	8.82



	SL3
	Chloride


	13713


	May 2019
	NO SAMPLE
	678
	30/05/19
	21.5



	SL3
	MP Xylene


	0.029


	May 2019
	NO SAMPLE
	54
	30/05/19
	

	SL3
	Mecoprop


	0.032


	May 2019
	NO SAMPLE
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen


	1370


	May 2019
	156
	678
	30/05/19
	10.6



	SL4
	Cadmium


	0.1


	May 2019
	<0.080
	34
	30/05/19
	7.83



	SL4
	Nickel


	0.1


	May 2019
	4.6
	34
	30/05/19
	8.82



	SL4
	Chloride


	13713


	May 2019
	936
	678
	30/05/19
	21.5



	SL4
	MP Xylene


	0.029


	May 2019
	<1.0
	54
	30/05/19
	

	SL4
	Mecoprop


	0.032


	May 2019
	12.5
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen


	1370


	May 2019
	128
	678
	30/05/19
	10.6



	SL5
	Cadmium


	0.1


	May 2019
	<0.080
	34
	30/05/19
	7.83



	SL5
	Nickel


	0.1


	May 2019
	2.5
	34
	30/05/19
	8.82



	SL5
	Chloride


	13713


	May 2019
	538
	678
	30/05/19
	21.5



	SL5
	MP Xylene


	0.029


	May 2019
	<1.0
	54
	30/05/19
	

	SL5
	Mecoprop


	0.032


	May 2019
	3.5
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen


	1370


	May 2019
	249
	678
	30/05/19
	10.6



	SL6
	Cadmium


	0.1


	May 2019
	<0.080
	34
	30/05/19
	7.83



	SL6
	Nickel


	0.1


	May 2019
	16.1
	34
	30/05/19
	8.82



	SL6
	Chloride


	13713


	May 2019
	382
	678
	30/05/19
	21.5



	SL6
	MP Xylene


	0.029


	May 2019
	<1.0
	54
	30/05/19
	

	SL6
	Mecoprop


	0.032


	May 2019
	3.9
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen


	1370


	May 2019
	864
	678
	30/05/19
	10.6



	SL7
	Cadmium


	0.1


	May 2019
	<0.080
	34
	30/05/19
	7.83



	SL7
	Nickel


	0.1


	May 2019
	18.7
	34
	30/05/19
	8.82



	SL7
	Chloride


	13713


	May 2019
	3,170
	678
	30/05/19
	21.5



	SL7
	MP Xylene


	0.029


	May 2019
	48.8
	54
	30/05/19
	

	SL7
	Mecoprop


	0.032


	May 2019
	11.6
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen


	1370


	May 2019
	1,220
	678
	30/05/19
	10.6



	SL8
	Cadmium


	0.1


	May 2019
	<0.080
	34
	30/05/19
	7.83



	SL8
	Nickel


	0.1


	May 2019
	83.7
	34
	30/05/19
	8.82



	SL8
	Chloride


	13713


	May 2019
	1,520
	678
	30/05/19
	21.5



	SL8
	MP Xylene


	0.029


	May 2019
	33.0
	54
	30/05/19
	

	SL8
	Mecoprop


	0.032


	May 2019
	12.2
	1214
	30/05/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen


	1370


	May 2019
	NO SAMPLE
	678
	30/05/19
	10.6



	SL9
	Cadmium


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	7.83



	SL9
	Nickel


	0.1


	May 2019
	NO SAMPLE
	34
	30/05/19
	8.82



	SL9
	Chloride


	13713


	May 2019
	NO SAMPLE
	678
	30/05/19
	21.5



	SL9
	MP Xylene


	0.029


	May 2019
	NO SAMPLE
	54
	30/05/19
	

	SL9
	Mecoprop


	0.032


	May 2019
	NO SAMPLE
	1214
	30/05/19
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date:  ……..06/12/19………

(Authorised to sign as representative of Operator)

