Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Sep19 SL…
Reporting of ……LEACHATE…… monitoring for the period for …September 19…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1


	Am Nitrogen


	1370


	Sep 19

	NO SAMPLE
	678
	25 Sep 19
	10.6



	SL1


	Cadmium


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	7.83



	SL1


	Nickel


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	8.82



	SL1


	Chloride
	13713


	Sep 19
	NO SAMPLE
	678
	25 Sep 19
	21.5



	SL1


	MP Xylene


	0.029


	Sep 19
	NO SAMPLE
	54
	25 Sep 19
	

	SL1


	Mecoprop


	0.032


	Sep 19

	NO SAMPLE
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen


	1370


	Sep 19

	NO SAMPLE
	678
	25 Sep 19
	10.6



	SL2
	Cadmium


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	7.83



	SL2
	Nickel


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	8.82



	SL2
	Chloride


	13713


	Sep 19
	NO SAMPLE
	678
	25 Sep 19
	21.5



	SL2
	MP Xylene


	0.029


	Sep 19
	NO SAMPLE
	54
	25 Sep 19
	

	SL2
	Mecoprop


	0.032


	Sep 19

	NO SAMPLE
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen


	1370


	Sep 19

	NO SAMPLE
	678
	25 Sep 19
	10.6



	SL3
	Cadmium


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	7.83



	SL3
	Nickel


	0.1


	Sep 19
	NO SAMPLE
	34
	25 Sep 19
	8.82



	SL3
	Chloride


	13713


	Sep 19
	NO SAMPLE
	678
	25 Sep 19
	21.5



	SL3
	MP Xylene


	0.029


	Sep 19
	NO SAMPLE
	54
	25 Sep 19
	

	SL3
	Mecoprop


	0.032


	Sep 19

	NO SAMPLE
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen


	1370


	Sep 19

	187
	678
	25 Sep 19
	10.6



	SL4
	Cadmium


	0.1


	Sep 19
	<1.00
	34
	25 Sep 19
	7.83



	SL4
	Nickel


	0.1


	Sep 19
	13.4
	34
	25 Sep 19
	8.82



	SL4
	Chloride


	13713


	Sep 19
	435
	678
	25 Sep 19
	21.5



	SL4
	MP Xylene


	0.029


	Sep 19
	<0.100
	54
	25 Sep 19
	

	SL4
	Mecoprop


	0.032


	Sep 19

	7.00
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen


	1370


	Sep 19

	146
	678
	25 Sep 19
	10.6



	SL5
	Cadmium


	0.1


	Sep 19
	<1.00
	34
	25 Sep 19
	7.83



	SL5
	Nickel


	0.1


	Sep 19
	21.9
	34
	25 Sep 19
	8.82



	SL5
	Chloride


	13713


	Sep 19
	516
	678
	25 Sep 19
	21.5



	SL5
	MP Xylene


	0.029


	Sep 19
	<0.100
	54
	25 Sep 19
	

	SL5
	Mecoprop


	0.032


	Sep 19

	8.30
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen


	1370


	Sep 19

	91.4
	678
	25 Sep 19
	10.6



	SL6
	Cadmium


	0.1


	Sep 19
	<1.00
	34
	25 Sep 19
	7.83



	SL6
	Nickel


	0.1


	Sep 19
	8.85
	34
	25 Sep 19
	8.82



	SL6
	Chloride


	13713


	Sep 19
	116
	678
	25 Sep 19
	21.5



	SL6
	MP Xylene


	0.029


	Sep 19
	0.729
	54
	25 Sep 19
	

	SL6
	Mecoprop


	0.032


	Sep 19

	4.75
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen


	1370


	Sep 19

	1240
	678
	25 Sep 19
	10.6



	SL7
	Cadmium


	0.1


	Sep 19
	<1.00
	34
	25 Sep 19
	7.83



	SL7
	Nickel


	0.1


	Sep 19
	270
	34
	25 Sep 19
	8.82



	SL7
	Chloride


	13713


	Sep 19
	1700
	678
	25 Sep 19
	21.5



	SL7
	MP Xylene


	0.029


	Sep 19
	2.89
	54
	25 Sep 19
	

	SL7
	Mecoprop


	0.032


	Sep 19

	21.4
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen


	1370


	Sep 19

	1230
	678
	25 Sep 19
	10.6



	SL8
	Cadmium


	0.1


	Sep 19
	1.05
	34
	25 Sep 19
	7.83



	SL8
	Nickel


	0.1


	Sep 19
	282
	34
	25 Sep 19
	8.82



	SL8
	Chloride


	13713


	Sep 19
	1710
	678
	25 Sep 19
	21.5



	SL8
	MP Xylene


	0.029


	Sep 19
	2.67
	54
	25 Sep 19
	

	SL8
	Mecoprop


	0.032


	Sep 19

	22.4
	1214
	25 Sep 19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen


	1370


	Sep 19

	877
	678
	25 Sep 19
	10.6



	SL9
	Cadmium


	0.1


	Sep 19
	<1.00
	34
	25 Sep 19
	7.83



	SL9
	Nickel


	0.1


	Sep 19
	132
	34
	25 Sep 19
	8.82



	SL9
	Chloride


	13713


	Sep 19
	1460
	678
	25 Sep 19
	21.5



	SL9
	MP Xylene


	0.029


	Sep 19
	0.812
	54
	25 Sep 19
	

	SL9
	Mecoprop


	0.032


	Sep 19

	18.4
	1214
	25 Sep 19
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………12/1/19…………..     



(Authorised to sign as representative of Operator)

