Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Sep19-C…
Reporting of ……Ground Water…… monitoring for the period for … September 2019…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Sep 19

	0.0570
	25
	25th Sep 2019
	10.6



	C1


	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C1


	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C1


	Chloride
	TBA


	Sep 19


	153
	25
	25th Sep 2019
	21.5



	C1


	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C1


	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Sep 19


	<0.0300
	25
	25th Sep 2019
	10.6



	C2
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C2
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C2
	Chloride


	TBA


	Sep 19


	43.3
	25
	25th Sep 2019
	21.5



	C2
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C2
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Sep 19


	<0.0300
	25
	25th Sep 2019
	10.6



	C3
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C3
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C3
	Chloride


	TBA


	Sep 19


	35.3
	25
	25th Sep 2019
	21.5



	C3
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C3
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Sep 19


	<0.0300
	25
	25th Sep 2019
	10.6



	C4
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C4
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C4
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C4
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C4
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Sep 19


	0.0380
	25
	25th Sep 2019
	10.6



	C5
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C5
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C5
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C5
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C5
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Sep 19


	7.73
	25
	25th Sep 2019
	10.6



	C6
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C6
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C6
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C6
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C6
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Sep 19


	8.03
	25
	25th Sep 2019
	10.6



	C8
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C8
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C8
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C8
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C8
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Sep 19


	13.2
	25
	25th Sep 2019
	10.6



	C10
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C10
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C10
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C10
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C10
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Sep 19


	23.7
	25
	25th Sep 2019
	10.6



	C12
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C12
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C12
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C12
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C12
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Sep 19


	17.1
	25
	25th Sep 2019
	10.6



	C14
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C14
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C14
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C14
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C14
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Sep 19


	1.49
	25
	25th Sep 2019
	10.6



	C16
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C16
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C16
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C16
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C16
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Sep 19


	No Sample
	25
	25th Sep 2019
	10.6



	C17
	Cadmium


	1 ug/l 
	Sep 19


	No Sample
	34
	25th Sep 2019
	7.83



	C17
	Nickel


	0.22 ug/l


	Sep 19


	No Sample
	34
	25th Sep 2019
	8.82



	C17
	Chloride


	TBA


	Sep 19


	No Sample
	25
	25th Sep 2019
	21.5



	C17
	MP Xylene


	1 ug/l 
	Sep 19


	No Sample
	54
	25th Sep 2019
	

	C17
	Mecoprop


	0.1 ug/l 
	Sep 19


	No Sample
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Sep 19


	0.0340
	25
	25th Sep 2019
	10.6



	C18
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C18
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C18
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C18
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C18
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Sep 19


	0.113
	25
	25th Sep 2019
	10.6



	C19
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C19
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C19
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C19
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C19
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Sep 19


	<0.0300
	25
	25th Sep 2019
	10.6



	C20
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C20
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C20
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C20
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C20
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Sep 19


	7.62
	25
	25th Sep 2019
	10.6



	C21
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C21
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C21
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C21
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C21
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Sep 19


	<0.0300
	25
	25th Sep 2019
	10.6



	C22
	Cadmium


	1 ug/l 
	Sep 19


	
	34
	25th Sep 2019
	7.83



	C22
	Nickel


	0.22 ug/l


	Sep 19


	
	34
	25th Sep 2019
	8.82



	C22
	Chloride


	TBA


	Sep 19


	
	25
	25th Sep 2019
	21.5



	C22
	MP Xylene


	1 ug/l 
	Sep 19


	
	54
	25th Sep 2019
	

	C22
	Mecoprop


	0.1 ug/l 
	Sep 19


	
	1214
	25th Sep 2019
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………12/1/20…………..     



(Authorised to sign as representative of Operator)
