[bookmark: _GoBack]Permit Reference Number: SP3531SK						Operator: Tradebe Ltd

Installation: Gwent Waste Management Centre					Form Number: S1

Reporting of Emissions to Sewer for the period from …………01/010/2019…………….to………31/12/2019……………

	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty
[5]

	S1
	Ammonia un-ionised as N [6]
	N/a
	4.269
	mg/L
	2:550 using Aquachem 600
	01 Oct 19      14:45hrs
	UKAS
	+/- 3%

	S1
	Cyanide

	N/a
	0.177
	mg/L
	2:412 using SEAL AA3
	24 Oct 19      14:30hrs
	UKAS
	+/- 3%

	S1
	Suspended solids

	N/a
	331
	mg/L
	2:724 using gravimetry
	30 Oct 19      14:00hrs
	UKAS
	+/- 1%

	S1
	Flow

	N/a
	26.3
	M3/hr
	Mag Flow
	01 Oct 19      08:45hrs
	MCERTS
	+/- 2%

	S1
	Lead & its compounds (Total Pb)
	N/a
	0.2
	mg/L
	2:311 using ICP-MS
	24 Oct 19      14:30hrs
	UKAS
	+/- 5%

	S1
	Nickel & its compounds (Total Ni)
	N/a
	0.9
	mg/L
	2:311 using ICP-MS
	21 Oct 19      14:15hrs
	UKAS
	+/- 5%

	S1
	Zinc & its compounds (Total Zn)
	N/a
	1.3
	mg/L
	2:311 using ICP-MS
	09 Dec 19      14:15hrs
	UKAS
	+/- 5%

	S1
	Chromium & its compounds (Total Cr)
	N/a
	0.1
	mg/L
	2:311 using ICP-MS
	09 Dec 19      14:15hrs
	UKAS
	+/- 5%

	S1
	Copper & its compounds (Total Cu)
	N/a
	1.0
	mg/L
	2:311 using ICP-MS
	21 Oct 19      14:15hrs
	UKAS
	+/- 5%

	S1
	pH
	N/a
	7.40
9.80
	pH units
	2:721 using meter
	30 Oct 19      14:00hrs 15 Nov 19       11:00hrs
	UKAS
	+/- 0.5



[1] 	The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] 	Where a reference number is given this refers to Wessex Water UKAS accredited lab (0905) documented in-house methods to meet the requirements of the Environment Agency MCERTS Performance Standard – sampling and chemical testing of untreated sewage, sewage effluent and trade effluent and the instrument used. In other cases the principal technique is stated, e.g. colorimetry.
[3] 	For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   
[4] 	The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.
[5] 	The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated
[6] 	‘Ammonia un-ionised as N’ calculated using Ammonia Calculator located on https://www.svl.net/2016/01/unionized-amonia-calculator/ using Total Ammonia = 156mg/L, pH = 7.8 and Temperature = 21.6oC.




Signed ……     A Morris           ……Alex Morris…………………………….  		Date…………16/01/20……………..		
	(Authorised to sign as representative of the Operator)

