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	Permit Number: 

Facility: 
	EPR/BJ9703IM 

Flint Paper Mill 
	Operator: 

Form Number: 
	Kimberly Clarke Ltd 

Performance1 / 30/09/18 




Reporting of other performance indicators for the period 01/01/2019 to 31/12/2019 (annually)


	Parameter

Water
	Units

Total m3/p.a
	
m3/t
	Methodology
Measured or Calculated

	Water Inputs to the Mill 3 
	
	
	

	Surface water (actual not licensed) eg: river water 
	NA
	
	

	Groundwater (actual not licensed) eg: borehole water 
	NA
	
	

	Mains water (only report if used in the paper or pulp manufacturing process) 
	391,905
	14.2 m3 / t
	Measured

	Other water (eg; if rainwater harvesting is practised) 
	0
	
	

	Water used in manufacturing 3 
	
	
	

	Cooling water (once through or hybrid systems) 
	NA
	
	

	Process water 
	As above 391,905
	14.2 m3 / t
	Measured

	Other water used in manufacturing 
	0
	
	

	Other inputs of water/moisture 
	
	
	

	Pulp or other fibre or wood at X% moisture content2 
	NA
	
	

	Waste paper for recycling at 10% moisture content2 
	3864.4 m3
	0.14 m3/ t
	Calculated

	Water outputs 3 
	-
	
	

	Waste Water discharged to surface waters 
NB; this figure should be the one used to report water usage per tonne as per BREF benchmarks under BATC No.5 and should exclude site drainage and cooling water 
	
346,867 m3
	
12.6 m3/t
	
Measured

	Waste water discharged to sewer 
	0
	
	

	Losses to evaporation 
	8221.8 m3
	0.3 m3/t
	Measured

	Losses in final product at 6% moisture content2 
	1644.3 m3
	0.06 m3/t
	Measured

	Losses in major waste stream outputs at 55% moisture content such as sludge2 
	13,465 m3
	0.55 m3/t
	Measured

	Losses in major waste stream outputs at 50% moisture content such as rejects (EWC 03 03 07)2 
	1531.8m3
	0.5 m3/t
	Measured





	

	Parameter 

Waste 
	Units 

Total tonnes/p.a
	Measured or Calculated


	Waste/raw material Inputs (other than those reported via quarterly waste returns)
	
	

	Pulp
	NA
	

	Starch & main fillers
	NA
	

	Other significant raw material inputs if >1000 tonnes
	NA
	

	
	
	

	Waste/raw material outputs (other than those reported via quarterly waste returns)
	Via waste returns
	

	
	
	

	
	
	

	Production (Net annual production reported as total as defined in the BREF BATCs1)
	27,406 t
	measured

	
	
	

	
	
	




Notes: 
1. (i) For paper mills: the unpacked, saleable production after the last slitter winder, i.e. before converting. (ii) For off-line coaters: production after coating. (iii) For tissue mills: saleable production after the tissue machine before any rewinding processes and excluding any core. (iv) for market pulp mills: production after packing (ADt). (v) For integrated mills: Net pulp, production refers to the production after packing (ADt) plus the pulp transferred to the paper mill (pulp calculated at 90 % dryness, i.e. air dry). Net paper production: same as (i) 

2. X% & Y% moisture content. Is defined as the average moisture content over the 12 month period. Monitoring frequency and test method (in the absence of any EN standard test method) determined by each mill but to be noted on the return for each input/output. 
3. All parameters in bold text are required to be reported on, others are optional.
Operator’s comments: 








Signed ………Jan Partridge…………………………………………………….                          Date……28.1.2020………………….. 
(Authorised to sign as representative of Operator)



