

Permit Number: EPR/TP3639BH			Operator: Celsa Manufacturing (UK) Limited

Facility: Tremorfa Melt Shop			Form Number: Air1 / 07/02/2020
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Particulate Matter
	5 mg/m3
	Daily average (Maximum)
	
	BS ISO 10155
	(month)
	

	A4
	Particulate Matter
	Ringleman Shade 1
	Daily average (Maximum)
	
	BS 2742
	
	

	
	
	
	
	
	
	
	

















Permit Number: EPR/TP3639BH			Operator: Celsa Manufacturing (UK) Limited

Facility: Tremorfa Melt Shop			Form Number: Air2 / 07/02/2020
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	
	Particulate Matter
	5 mg/m3
	
	
	BS EN 13284-1
	
	

	
	Carbon  monoxide
	No limit set
	Hourly average
	
	BS EN 15058
	
	

	
	Oxides of nitrogen (NO and NO2 expressed as NOx)
	25 mg/m3

	

	

	BS EN 14792

	

	

	
	Sulphur dioxide
	25 mg/m3

	15 minute average
	

	BS EN 14791
	

	

	
	PCDD/F
	0.1ng/m3
	6-8 hours random sampling during steady state conditions
	
	BS EN 1948:1-3
	
	

	
	VOC
	20 mg/m3

	
	
	BS EN 12319
	
	

	
	Metals
	No limit set
	
	
	BS EN 14385
	
	

	
	Mercury
	0.05 mg/m3
	Spot samples for at least four hours
	
	BS EN 13211
	
	

	
	PAH
	No limit set
	
	
	ISO 11338:1-2
	
	

	
	PCB
	No limit set
	
	
	BS EN 1948:4
	
	

	A2
	Particulates
	10 mg/m3
	
	

	
	

	

	
	
	
	
	
	
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: EPR/TP3639BH		               Operator: Celsa Manufacturing (UK) Limited

Facility: Tremorfa Melt Shop		            Form Number: Water1 / 07/02/2020
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	Discharge to soakaway on plan 3 in schedule 7. 
15 – Sampling Point and Discharge Consented Point 1.

	pH
	
	Spot sample
	
	BS ISO 10523
	
	

	
	Electrical conductivity
	
	Spot sample
	
	BS EN 27888 ISO 7888
	
	

	
	Biological Oxygen Demand
	
	Spot sample
	
	BS EN 1899
	
	

	
	Oxygen Levels
	
	Spot sample
	
	To be agreed in writing with NRW
	
	

	
	Suspended Solids
	
	Spot sample
	
	BS EN 872
	
	

	
	Chemical Oxygen Demand
	
	Spot sample
	
	BS ISO 15705
	
	

	
	Volatile Organic Compounds
	
	Spot sample
	
	BS EN ISO 15680
	
	

	
	Semi Volatile Organic Compounds
	
	Spot sample
	
	To be agreed in writing with NRW
	
	

	
	Total petroleum Hydrocarbons C6-C40
	
	
	
	SCA blue book 77 ISBN 0117517283 2002 or other ISO, BS or SCA blue book method as approved by Natural Resources Wales
	
	

	
	Fully Speciated Total Petroleum Hydrocarbons
	
	Spot sample
	
	To be agreed in writing with NRW
	
	

	
	Iron
	
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Cadmium
	
	Spot sample
	
	BS EN ISO 5961
	
	

	
	Copper
	
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Nickle
	
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Lead
	
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Zinc
	
	Spot sample
	
	BS EN ISO 11885 
	
	

	
	
	
	
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..



	(Authorised to sign as representative of Operator)


































Permit Number: EPR/TP3639BH		               Operator: Celsa Manufacturing (UK) Limited
[bookmark: _GoBack]Facility: Tremorfa Melt Shop                                   Form Number: Sewer1 / 07/02/2020
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Total hydrocarbons
	5 mg/l
	Spot sample
	
	SCA blue book 77 ISBN 0117517283 2002 or other ISO, BS or SCA blue book method as approved by Natural Resources Wales
	
	

	
	Suspended solids
	20 mg/l
	
	
	BS EN 872 or other method approved by NRW
	
	

	
	pH
	6-10
	
	
	BS ISO 10523
	
	

	
	Nickel
	0.5 mg/l
	
	
	BS EN ISO 11885
	
	

	
	Arsenic
	0.01 mg/l
	
	
	BS ISO 17378
	
	

	
	Cadmium
	0.05 mg/l
	
	
	BS EN ISO 5961
	
	

	
	Total Chromium
	0.5 mg/l
	
	
	BS EN 1233
	
	

	
	Zinc
	2 mg/l
	
	
	BS EN ISO 11885
	
	

	
	Mercury
	0.02 mg/l
	
	
	BS EN 12846
	
	

	
	Iron
	5 mg/l
	
	
	BS EN ISO 11885
	
	

	
	Flow
	No Limit Set
	
	
	Flow meter
	
	

	S2
	Total hydrocarbons
	5 mg/l
	
	
	SCA blue book 77 ISBN 0117517283 2002 or other ISO, BS or SCA blue book method as approved by Natural Resources Wales
	
	

	
	Suspended solids
	20 mg/l
	
	
	BS EN 872 or other method approved by NRW
	
	

	
	pH
	6-10
	
	
	BS ISO 10523
	
	

	
	Nickel
	0.5 mg/l
	
	
	BS EN ISO 11885
	
	

	
	Arsenic
	0.01 mg/l
	
	
	BS ISO 17378
	
	

	
	Cadmium
	0.05 mg/l
	
	
	BS EN ISO 5961
	
	

	
	Total Chromium
	0.5 mg/l
	
	
	BS EN 1233
	
	

	
	Zinc
	2 mg/l
	
	
	BS EN ISO 11885
	
	

	
	Mercury
	0.02 mg/l
	
	
	BS EN 12846
	
	

	
	Iron
	5 mg/l
	
	
	BS EN ISO 11885
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
(Authorised to sign as representative of Operator)
