[bookmark: _GoBack]Schedule 6 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.
Part A 
	Permit Number
	EPR/BJ9703IM

	Name of operator
	Kimberly-Clark Limited

	Location of Installation
	Coleshill Paper Mill, Aber Road, Flint, Flintshire, CH6 5EX

	Time and date of the detection 
	06/08/2019



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	06/08/2019

	Reference or description of the location of the event 
	Final Discharge point – Kimberly Clark Flint

	Description of where any release into the environment took place
	Discharge into the estuary

	Substances(s) potentially released
	TSS

	Best estimate of the quantity or rate of  release of substances
	Total volume of discharge 1025.2m3

	Measures taken, or intended to be taken, to stop any emission
	No measures taken as discharge had taken place then sample analysed. Repeat sample taken from the TET are returning in consent results.

	Description of the failure or accident.
	TSS exceeds IPPC limit of 85 mg/l 



	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	W2

	Parameter(s)
	TSS

	Limit
	80 mg/l

	Measured value and uncertainty
	85 mg/l

	Date and time of monitoring
	06/08/2019

	Measures taken, or intended to be taken, to stop the emission
	No measures taken as discharge had taken place then sample analysed. Repeat sample taken from the TET are returning in consent results.

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	TSS
	Without delay

	
	

	
	

	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	Sample measured from sampler at discharge

	Substances(s) detected
	TSS

	Concentrations of substances detected
	85 mg/l

	Date of monitoring/sampling
	06/08/2019 04:32



Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	 

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	



	Name*
	Jan Partridge

	Post
	Site Process Engineer Environment and Quality

	Signature
	J. Partridge

	Date
	06/08/2019


* authorised to sign on behalf of Kimberley Clark
