Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Aug 19-C…
Reporting of ……Ground Water…… monitoring for the period for … August 2019…
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C1


	Am Nitrogen


	TBA


	Aug  - 19
	0.0570
	25
	10/8/19
	10.6



	C1


	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C1


	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C1


	Chloride
	TBA


	Aug  - 19
	153
	25
	10/8/19
	21.5



	C1


	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C1


	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C2
	Am Nitrogen


	TBA


	Aug  - 19
	<0.0300
	25
	10/8/19
	10.6



	C2
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C2
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C2
	Chloride


	TBA


	Aug  - 19
	43.3
	25
	10/8/19
	21.5



	C2
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C2
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C3
	Am Nitrogen


	TBA


	Aug  - 19
	<0.0300
	25
	10/8/19
	10.6



	C3
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C3
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C3
	Chloride


	TBA


	Aug  - 19
	35.3
	25
	10/8/19
	21.5



	C3
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C3
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C4
	Am Nitrogen


	TBA


	Aug  - 19
	<0.0300
	25
	10/8/19
	10.6



	C4
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C4
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C4
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C4
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C4
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C5
	Am Nitrogen


	TBA


	Aug  - 19
	0.0380
	25
	10/8/19
	10.6



	C5
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C5
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C5
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C5
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C5
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C6
	Am Nitrogen


	TBA


	Aug  - 19
	7.73
	25
	10/8/19
	10.6



	C6
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C6
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C6
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C6
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C6
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C8
	Am Nitrogen


	TBA


	Aug  - 19
	8.03
	25
	10/8/19
	10.6



	C8
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C8
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C8
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C8
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C8
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C10
	Am Nitrogen


	TBA


	Aug  - 19
	13.2
	25
	10/8/19
	10.6



	C10
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C10
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C10
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C10
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C10
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C12
	Am Nitrogen


	TBA


	Aug  - 19
	23.7
	25
	10/8/19
	10.6



	C12
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C12
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C12
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C12
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C12
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C14
	Am Nitrogen


	TBA


	Aug  - 19
	17.1
	25
	10/8/19
	10.6



	C14
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C14
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C14
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C14
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C14
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C16
	Am Nitrogen


	TBA


	Aug  - 19
	1.49
	25
	10/8/19
	10.6



	C16
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C16
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C16
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C16
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C16
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C17
	Am Nitrogen


	TBA


	Aug  - 19
	No Sample
	25
	10/8/19
	10.6



	C17
	Cadmium


	1 ug/l 
	Aug  - 19
	No Sample
	34
	10/8/19
	7.83



	C17
	Nickel


	0.22 ug/l


	Aug  - 19
	No Sample
	34
	10/8/19
	8.82



	C17
	Chloride


	TBA


	Aug  - 19
	No Sample
	25
	10/8/19
	21.5



	C17
	MP Xylene


	1 ug/l 
	Aug  - 19
	No Sample
	54
	10/8/19
	

	C17
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	No Sample
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C18
	Am Nitrogen


	TBA


	Aug  - 19
	0.0340
	25
	10/8/19
	10.6



	C18
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C18
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C18
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C18
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C18
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C19
	Am Nitrogen


	TBA


	Aug  - 19
	0.113
	25
	10/8/19
	10.6



	C19
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C19
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C19
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C19
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C19
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C20
	Am Nitrogen


	TBA


	Aug  - 19
	<0.0300
	25
	10/8/19
	10.6



	C20
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C20
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C20
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C20
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C20
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C21
	Am Nitrogen


	TBA


	Aug  - 19
	7.62
	25
	10/8/19
	10.6



	C21
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C21
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C21
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C21
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C21
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	C22
	Am Nitrogen


	TBA


	Aug  - 19
	<0.0300
	25
	10/8/19
	10.6



	C22
	Cadmium


	1 ug/l 
	Aug  - 19
	
	34
	10/8/19
	7.83



	C22
	Nickel


	0.22 ug/l


	Aug  - 19
	
	34
	10/8/19
	8.82



	C22
	Chloride


	TBA


	Aug  - 19
	
	25
	10/8/19
	21.5



	C22
	MP Xylene


	1 ug/l 
	Aug  - 19
	
	54
	10/8/19
	

	C22
	Mecoprop


	0.1 ug/l 
	Aug  - 19
	
	1214
	10/8/19
	14.6




1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

4. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………4/2/20…………..     



(Authorised to sign as representative of Operator)
