Permit Reference Number: VP3339PD					Operator: Morganite Electrical Carbon Ltd

Installation: Electrical Carbon Swansea				Form Number: A1

Reporting of Emissions to Air for the period from	January ’20	to	December ‘20;		April ’20	to	June ‘20
	Emissions to Air

	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
(mg/m3)
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty (mg/m3)
[5]

	A10
	Lead
	2
	0.051
	BS EN 14385:2004
	10:55 – 11:57; 22/01/2020
	UKAS/MCERTS
	0.051

	A10
	Copper
	2
	0.585
	BS EN 14385:2004
	10:55 – 11:57; 22/01/2020
	UKAS/MCERTS
	0.085

	A10
	Antimony
	2
	0.001
	BS EN 14385:2004
	10:55 – 11:57; 22/01/2020
	UKAS/MCERTS
	0.0001

	A10
	Lead
	2
	0.030
	BS EN 14385:2004
	09:14 – 10:16; 28/04/2020
	UKAS/MCERTS
	0.003

	A10
	Copper
	2
	1.34
	BS EN 14385:2004
	09:14 – 10:16; 28/04/2020
	UKAS/MCERTS
	0.15

	A10
	Antimony
	2
	0.001
	BS EN 14385:2004
	09:14 – 10:16; 28/04/2020
	UKAS/MCERTS
	0.0001

	A10
	Lead
	2
	
	BS EN 14385:2004
	
	UKAS/MCERTS
	

	A10
	Copper
	2
	
	BS EN 14385:2004
	
	UKAS/MCERTS
	

	A10
	Antimony
	2
	
	BS EN 14385:2004
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	UKAS/MCERTS
	

	A10
	Lead
	2
	
	BS EN 14385:2004
	
	UKAS/MCERTS
	

	A10
	Copper
	2
	
	BS EN 14385:2004
	
	UKAS/MCERTS
	

	A10
	Antimony
	2
	
	BS EN 14385:2004
	
	UKAS/MCERTS
	

	A27
	Sulphur dioxide
	2900
	
	BS ISO 7935:1992
	
	UKAS/MCERTS
	

	A28
	Sulphur dioxide
	2900
	
	BS ISO 7935:1992
	
	UKAS/MCERTS
	

	A61
	Sulphur dioxide
	2900
	
	BS ISO 7935:1992
	
	UKAS/MCERTS
	

	A27
	Oxides of nitrogen (as NO2)
	150
	
	BS ISO 14792:2005
	
	UKAS/MCERTS
	

	A28
	Oxides of nitrogen (as NO2)
	150
	
	BS ISO 14792:2005
	
	UKAS/MCERTS
	

	A61
	Oxides of nitrogen (as NO2)
	150
	
	BS ISO 14792:2005
	
	UKAS/MCERTS
	

	A10
	Total particulate
	10
	3.1
	BS ISO 13284:2002
	09:45 – 10:47; 22/01/2020
	UKAS/MCERTS
	0.66

	A15
	Total particulate
	10
	
	BS ISO 13284:2002
	
	UKAS/MCERTS
	

	A19
	Total particulate
	10
	
	BS ISO 13284:2002
	
	UKAS/MCERTS
	

	A27
	Total particulate
	10
	
	BS ISO 13284:2002
	
	UKAS/MCERTS
	

	A28
	Total particulate
	10
	
	BS ISO 13284:2002
	
	UKAS/MCERTS
	

	A61
	Total particulate
	10
	
	BS ISO 13284:2002
	
	UKAS/MCERTS
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.
[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ……Mark Williamson………………………………  		Date…19/05/2020..… 	
	(Authorised to sign as representative of the Operator)
