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ALUN GRIFFITHS CONTRACTORS
Pont yr odyn cyclebridge 
ENVIRONMENTAL ACTION PLAN

ALUN GRIFFITHS (CONTRACTORS) LIMITED
The aim of this plan is to provide an initial strategy for pollution control together with protection wherever possible of the existing environment.
1. Control of run off into watercourses from construction activities during inclement weather.

During periods of heavy rainfall there will\ be no activity allowed on site likely to cause an increase in waterborne silts being allowed to escape into any existing watercourse. All storm gullies will be clearly marked and where necessary protected with sand bags/geotextile to avoid silt infiltration. Stock piled materials will be a minimum of 10m away from the water course.
2. Fuel and oil.

Fuels and oils will be stored in a properly bunded facility within the site compound. All refuelling with diesel and oil together with minor repairs will be carried out in such a manner as to minimise risk of spillage or leakage. Wherever possible no fuel storage, refuelling or repair work will be undertaken adjacent to the existing watercourses, drains or sewers.

3. Hazardous materials.

All hazardous materials required in the construction of the works will be stored in a secure compound away from watercourses, drains or sewers. 
Washing out of mixers, containers or tools will be undertaken within an area set aside for this purpose within a watertight skip or other suitable container. Skips or containers will be removed at regular intervals and emptied at a licensed waste facility. 
Care will be taken to ensure that no contamination of watercourses can occur through accidental spillage. Appropriate spill kits will be available and surface water gullies will be bunded where required to minimise risk of pollution. 

4. Dust.

Dust is unlikely to be a major cause for concern with all concrete/ masonry cutting equipment being fitted with water feed to the blade. Any cutting will be restricted to specific covered locations within the working area. Dust from plant movements will be controlled by use of towed water bowsers as required.
5. Vibration.

Construction activities planned near to adjacent buildings likely to cause noticeable vibration are too kept to minimum. A detailed internal survey is to be provided by the Client prior to works commencing. 
6. Spillage of cementitious materials.

No washing out of concrete mixer trucks will be allowed on site adjacent to any watercourse, drain or sewer. Small concrete/cement mixers used during construction activities will be washed out into designated areas and deposited in skips or other watertight containers provided as in Item 3. Barrows will also be washed out into the skips. 

Construction work requiring incorporation of concrete or cement will be sheeted over in the event of rain and always at the end of each shift in order to prevent wash off and possible pollution.
7. Access onto/off the site.

Wherever practicable the site will be contained within the confines of a temporary fence, which will serve both as a secure barrier against accidental trespass by members of the public, Trust employees etc and a construction access corridor to which all construction activity will be confined.
The site will be signed such that all people will be directed to safe routes and particular no go areas highlighted. (I.e. Danger - Deep Excavations Keep Out)
All visitors will be directed to the site office where they must report and receive suitable site induction prior to entering the working area.

8. Noise.

All activities will be undertaken with due regard to the sensitivity of the surrounding area particularly the close proximity of noise sensitive buildings and noise will be kept to a minimum. All plant and vehicles will be required to turn off engines when not in use. 
9.  Exhaust pollution.

All vehicles will be regularly serviced and inspected by a competent person to ensure that fumes, etc from engines are kept to a minimum. Any plant found not to meet the standard required on site will be repaired/replaced immediately.
