


Permit Number: 	SP3537VQ					Operator: 		Biogen Bryn Pica Ltd

Facility:		Bryn Pica Anaerobic Digestion Site	Form Number: 	 Air1 / 17/08/2022
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY effective from 17th August 2022
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	500 mg/m3
	Hourly mean
	
	BS EN 14792
	
	

	A1
	Carbon monoxide
	1400 mg/m3
	Hourly mean
	
	BS EN 15058
	
	

	A1
	Total Volatile Organic Compounds (VOCs)
	1000 mg/m3
	Hourly mean
	
	BS EN12619:1999 or 13526:2002
	
	

	A1
	Sulphur Dioxide
	350 mg/m3
	Hourly mean
	
	BS EN 14791
	
	

	A2
	Oxides of nitrogen (NO and NO2 expressed as NO2)[5]
	No limit set
	Hourly mean
	
	BS EN 14792
	
	

	A2
	Carbon monoxide[5]
	No limit set
	Hourly mean
	
	BS EN 15058
	
	

	A2
	Total Volatile Organic Compounds (VOCs)[5]
	No limit set
	Hourly mean
	
	BS EN12619:1999 or 13526:2002
	
	

	A5
	Ammonia (NH3)[6]
	20 mg/Nm3
	Every 6 months
	
	EN ISO 21877
	
	

	A5
	Hydrogen sulphide (H2S)[6]
	No Set Limit
	Every 6 months
	
	US EPA Method 11 (Impinger method), and CEN TS 13649 (Charcoal tube), US EPA Method 15
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Monitoring of flare emissions is only necessary when the flare operated in excess of 10% of the time
[6] Where emissions are unlikely to impact on sensitive receptors, operators can choose whether to monitor for odour or ammonia and hydrogen sulphide.   Operators will need to justify that their choice demonstrates the continued efficacy of their abatement equipment and that the environment is protected.


Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	SP3537VQ						Operator: 		Biogen Bryn Pica Ltd

Facility:		Bryn Pica Anaerobic Digestion Site		Form Number: 	Water1 / 14/01/2021
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Oil and grease
	None visible
	Periodic (prior to discharge)
	
	
	
	



1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
1. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
1. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
1. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

Permit Number: 	SP3537VQ					Operator: 		Biogen Bryn Pica Ltd

Facility:		Bryn Pica Anaerobic Digestion Site	Form Number: 	WaterUsage1 / 14/01/2021

Reporting of Water Usage for the year YYYY 

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments:







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	SP3537VQ					Operator: 		Biogen Bryn Pica Ltd

[bookmark: _GoBack]Facility:		Bryn Pica Anaerobic Digestion Site	Form Number: 	Energy1 / 14/01/2021

Reporting of Energy Usage for the year YYYY 

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments:









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	SP3537VQ					Operator: 		Biogen Bryn Pica Ltd

Facility:		Bryn Pica Anaerobic Digestion Site	Form Number: 	Performance1 / 17/08/2022

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY effective from 17th August 2022

	Parameter
	
	Units 

	
	
	

	Total raw material used 
	tonnes

	Total amounts of waste treated
	tonnes

	Biogas produced by AD Facility
	m3

	Power output - electricity
	MWh

	Energy efficiency
	MWh/m3 biogas

	Electrical energy exported to the grid
	MWh

	Electrical energy drawn from the grid
	MWh

	Operational time of emergency flare
	%

	Amount of gas sent to emergency flare
	m3

	Generation of residue waste
	Tonnes

	Generation of wastewater
	m3

	Amount of biogas combusted in the CHP unit per day
	m3/day



	Operator’s comments:








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)  





