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Under condition 8.26 of the Gwynt y Mor Operations & Maintenance Marine Licence, 11/52/ML/4, GYMOWF must ensure vessel traffic adheres to an agreed vessel routing plan when undertaking works.  The vessel routing plan is required to mitigate the potential impacts of vessel induced disturbance on Common Scoter.  
The Operational Phase Vessel Routing Plan agreed with Natural Resources Wales shall be adhered to between October and March annually throughout the operation and maintenance phase.  Figure 1 shows the operational route for CTVs to follow in winter (October to March) from the Port of Mostyn to the central and eastern areas of the GYMOWF site. The previous route followed the Welsh Channel from the Port of Mostyn before tracking out along the South Hoyle Channel.  However the amended route travels north of the West Hoyle Spit, tracking out via the Mid Hoyle Channel and passing North Hoyle Offshore Wind Farm on a more direct route to the eastern array of the GYMOWF site.
Figure 1 – Approved operational phase vessel route during winter period (October to March)
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