[bookmark: _GoBack][bookmark: _Hlk56081816]Permit Number: 	KP3636HB				Operator: 		Egan Waste Services Limited

Facility:		The Recycling Centre		Form Number: 	Sewer1 / 17/08/2022
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty[4]

	S1 Interceptor
	Adsorbable organically bound halogens (AOX)
	1 mg/l
	None specified
	
	EN ISO 9562
	
	

	
	Benzene, toluene, ethylbenzene, xylene (BTEX)
	None set
	
	
	EN ISO 15680
	
	

	
	Free cyanide (CN-)
	0.1 mg/l
	
	
	Various EN standards available (i.e. EN ISO 14403-1 and -2)
	
	

	
	Hydrocarbon oil index (HOI)
	10 mg/l
	
	
	EN ISO 9377-2 
	
	

	
	Arsenic (As)
	0.1 mg/l
	
	
	Various EN standards available (e.g. EN ISO 11885, EN ISO 17294-2, EN ISO 15586)
	
	

	
	Cadmium (Cd)
	0.1 mg/l
	
	
	
	
	

	
	Chromium (Cr)
	0.3 mg/l
	
	
	
	
	

	
	Copper (Cu)
	0.5 mg/l
	
	
	
	
	

	
	Nickel (Ni)
	1 mg/l
	
	
	
	
	

	
	Lead (Pb)
	0.3 mg/l
	
	
	
	
	

	
	Zinc (Zn)
	2 mg/l
	
	
	
	
	

	
	Manganese (Mn)
	None set
	
	
	
	
	

	
	Hexavalent chromium (Cr(VI))
	None set
	
	
	Various EN standards available (i.e. EN ISO 10304-3, EN ISO 23913)
	
	

	
	Mercury (Hg)
	10 μg/l
	
	
	Various EN standards available (i.e. EN ISO 17852, EN ISO 12846)
	
	

	
	PFOA
	None set
	
	
	No EN standard available
	
	

	
	PFOS
	None set
	
	
	No EN standard available
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………………………………………….  		Date……………………   	
	(Authorised to sign as representative of Operator)
