Permit Number: 	PP3430UL 								Operator: 	SRCL Limited

Facility: 	Bridgend Clinical Waste Treatment Plant and Transfer Station	Form Number: 	Air1 / 17/08/2022
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty [4]

	A1
	Dust
	5 mg/Nm3
	None set
	
	EN 13284-1
	
	

	A1
	NH3
	None set
	None set
	
	No EN standard available 
	
	

	A1
	TVOC
	None set
	None set
	
	EN 12619 
	
	

	A2
	Dust
	5 mg/Nm3
	None set
	
	EN 13284-1
	
	

	A2
	NH3
	None set
	None set
	
	No EN standard available 
	
	

	A2
	TVOC
	None set
	None set
	
	EN 12619 
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	PP3430UL 								Operator: 	SRCL Limited

Facility: 	Bridgend Clinical Waste Treatment Plant and Transfer Station	Form Number: 	Sewer1 / 17/08/2022
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty [4]

	S1
	Flow
	None set
	None set
	
	To be agreed with the regulator
	
	

	S1
	Arsenic (As)
	0.05 mg/l
	None set
	
	Various EN standards available (e.g. EN ISO 11885, EN ISO 17294-2, EN ISO 15586)
	
	

	S1
	Cadmium (Cd)
	0.05 mg/l
	None set
	
	
	
	

	S1
	Chromium (Cr)
	0.15 mg/l
	None set
	
	
	
	

	S1
	Copper (Cu)
	0.5 mg/l
	None set
	
	
	
	

	S1
	Lead (Pb)
	0.1 mg/l
	None set
	
	
	
	

	S1
	Nickel (Ni)
	0.5 mg/l
	None set
	
	
	
	

	S1
	Zinc (Zn)
	1 mg/l
	None set
	
	
	
	

	S1
	Mercury (Hg)
	5 μg/l
	None set
	
	Various EN standards available (i.e. EN ISO 17852, EN ISO 12846)
	
	

	S1
	PFOA
	None set
	None set
	
	No EN standard available
	
	

	[bookmark: _GoBack]S1
	PFOS
	None set
	None set
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

