[bookmark: _GoBack]Permit Number: 	VP3030BX 				Operator: 		Befesa Salt Slags Limited

Facility:		Whitchurch Salt Slags		Form Number: 	Air 1 / 14/09/2018

Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY

	Emission Point
	Substance / Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty[4]

	A1
	Particulate Matter
	12 mg/m3
	1 hour period
	
	BS EN 13284-1 2002
	
	

	A2
	Ammonia
	9 mg/m3
	1 hour period
	
	BS EN 14791 
	
	

	A4
	Hydrogen sulphide
	None set
	Spot sample
	
	ISO 17025 accredited 
	
	

	A5
	Ammonia
	9 mg/m3
	1 hour period
	
	BS EN 14791 
	
	

	A6
	Ammonia
	9 mg/m3
	1 hour period
	
	BS EN 14791 
	
	

	A7
	Ammonia
	9 mg/m3
	1 hour period
	
	BS EN 14791 
	
	

	A7
	Phosphine (PH3)
	0.5 mg/Nm3
	1 hour period
	
	BS EN 14791
	
	

	A7
	Hydrogen Sulphide (H2S)
	2 mg/Nm3
	1 hour period
	
	US EPA Method 11
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. 
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography. 
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.    
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

Signed …………………………………………………………….	Date………………………...
	(authorised to sign as representative of Operator)


1
Permit Number: 	VP3030BX 				Operator: 		Befesa Salt Slags Limited

Facility:		Whitchurch Salt Slags		Form Number: 	Air 2 / 14/09/2018

Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample
Date and Times [3]
	Uncertainty [4]

	A1
	Particulate Matter
	5 mg/m3 
	1 hour period 
	 
	BS EN 13284-1 2002 
	 
	 

	A2
	Ammonia 
	9 mg/m3 
	1 hour period 
	 
	BS EN 14791 
	 
	 

	A2
	Phosphine (PH3)
	0.5 mg/Nm3
	1 hour period
	
	BS EN 14791
	
	

	A2
	Hydrogen Sulphide (H2S)
	2 mg/Nm3
	1 hour period
	
	US EPA Method 11
	
	

	A4
	Hydrogen Sulphide (H2S)
	None set 
	Spot sample 
	 
	ISO 17025 accredited 
	 
	 

	A5
	Ammonia 
	9 mg/m3 
	1 hour period 
	 
	BS EN 14791 
	 
	 

	A5
	Phosphine (PH3)
	0.5 mg/Nm3
	1 hour period
	
	BS EN 14791
	
	

	A5
	Hydrogen Sulphide (H2S)
	2 mg/Nm3
	1 hour period
	
	US EPA Method 11
	
	

	A6
	Ammonia 
	9 mg/m3 
	1 hour period 
	 
	BS EN 14791 
	 
	 

	A6
	Phosphine (PH3)
	0.5 mg/Nm3
	1 hour period
	
	BS EN 14791
	
	

	A6
	Hydrogen Sulphide (H2S)
	2 mg/Nm3
	1 hour period
	
	US EPA Method 11
	
	

	A7
	Ammonia 
	9 mg/m3 
	1 hour period 
	 
	BS EN 14791 
	 
	 

	A7
	Phosphine (PH3)
	0.5 mg/Nm3
	1 hour period
	
	BS EN 14791
	
	

	A7
	Hydrogen Sulphide (H2S)
	2 mg/Nm3
	1 hour period
	
	US EPA Method 11
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values. 
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography. 
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.    
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

Signed …………………………………………………………….	Date………………………...
	(authorised to sign as representative of Operator)



4
Permit Number: 	VP3030BX 				Operator: 		Befesa Salt Slags Limited

Facility:		Whitchurch Salt Slags		Form Number: 	WaterUsage1 / 14/09/2018

Reporting of Water Usage for the year YYYY 

	Water Source 
	Usage (m3/year 
	Specific Usage  
(m3/tonne of material processed) 

	 
	 
	 

	Mains Water 
	 
	 

	Recovered Water 
	 
	 

	 
	 
	 

	 
	 
	 

	 
	 
	 

	TOTAL WATER USAGE 
	 
	 




Operator’s comments: 
 
 
 
 

Signed …………………………………………………………….	Date………………………...
	(authorised to sign as representative of Operator)

1
Permit Number: 	VP3030BX 				Operator: 		Befesa Salt Slags Limited

Facility:		Whitchurch Salt Slags		Form Number: 	Energy 1 / 14/09/2018
 
Reporting of Energy Usage for the year YYYY

	Energy Source
	Energy Usage
	Specific Usage
(MWh/tonne of material processed)

	
	Quantity
	Primary Energy (MWh)
	

	
	
	
	 

	Electricity * 
	MWh
	
	 

	Kerosene 
	MWh
	
	 

	LPG 
	tonnes
	
	 

	
	
	
	 

	
	
	
	 

	TOTAL
	-
	 
	 



* Conversion factor for delivered electricity to primary energy = 2.4 
 
Operator’s comments: 
 
 
 
 
 
 
Signed …………………………………………………………….	Date………………………...
	(authorised to sign as representative of Operator)

1
Permit Number: 	VP3030BX 				Operator: 		Befesa Salt Slags Limited

Facility:		Whitchurch Salt Slags		Form Number: 	Performance 1 / 14/09/2018
 
Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY 
 
	Parameter 
	 
	Units  

	Total waste produced per tonne of material processed 
	tonnes 

	 
	 

	 
	 

	 
	 



Operator’s comments: 
 
 
 
 


Signed …………………………………………………………….	Date………………………...
	(authorised to sign as representative of Operator) 
