Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V013

	Name of operator
	Hanson Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	17.30  21.08.18


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	21.8.18 @ 17.30

	Reference or description of the location of the event 
	Raw mill building

	Description of where any release into the environment took place
	Atmosphere

	Substances(s) potentially released
	Dust particulates

	Best estimate of the quantity or rate of  release of substances
	Dust release identified at 17.25.Estimated 50 kg’s escaped from building locally onto the site

	Measures taken, or intended to be taken, to stop any emission
	Raw mill was shut down within 2 minutes of visual detection of dust escape. The local area within the building has been visually inspected for potential leak paths/routes and the procedure for running both the mill and the main bag filter system checked for any faults or indications of any problem. Main bag filter was checked for blockages visually and by the kiln burner from the control room via his operating procedures for running the mill and main bag filter system. Once satisfied there was no further risk the system was started again.

	Description of the failure or accident.
	Dust escaped by an unknown source/fault.  Data is being collected and further investigation will take place and details passed onto the relevant person(s)


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	D Pritchard

	Post
	Shift Manager

	Signature
	

	Date
	22/08/17


* authorised to sign on behalf of Castle Cement Limited
