Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V016

	Name of operator
	Hanson Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	10.00 05.01.2021


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	10.00 05.01.2021

	Reference or description of the location of the event 
	PHT Level 9, Cyclone 1 expansion joint holed

	Description of where any release into the environment took place
	Visually confirmed at location stated above

	Substances(s) potentially released
	Very small amount of dust

	Best estimate of the quantity or rate of release of substances
	Less than 5kg’s

	Measures taken, or intended to be taken, to stop any emission
	Further investigation required

	Description of the failure or accident.
	Cyclone 1 expansion joint is holed


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	HCl
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The expansion joint was inspected during the October 2020 kiln stop. The outcome of the inspection was that a temporary repair was required and a full replacement was required in the next kiln shutdown.  This temporary repair was completed during the stop.
Following the repair, the kiln ran through with no issues with the joint until 5th January 2021.
Once identified and the schedule 5 notification reported, a controlled runout of all equipment was initiated in preparation for annual shutdown.


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	A further repair took place during January kiln stop due to adverse weather conditions and the expansion joint was fully replaced during the March shutdown.



	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The kiln system was runout and annual shutdown was executed.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	05/01/2019

22/03/2019

29/03/2019

15/08/2019

29/08/2019

21/09/2019

23/10/2019

28/10/2019

15/12/2019

23/12/2019

09/02/2020

07/03/2020

23/04/2020

26/04/2020

10/07/2020

23/08/2020

30/08/2020

29/10/2020


	Name
	Stewart Mitchell

	Post
	Quality and Environment Manager

	Signature
	S. Mitchell

	Date
	07/06/2021


* authorised to sign on for and on behalf of Castle Cement Limited
