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Part A 
	Permit Number
	PP3139GB

	Name of Operator
	Enovert North Limited

	Location of Installation
	Bangor Road
Johnstown
Wrexham
LL14 6ET

	Time and date of the detection
	When data entered onto database

	b) Notification requirements for breach of a limit

	To be notified within 24 hours of detection unless otherwise specified

	Emission point reference/source
	Leachate Head
Limit: >2m 
	Sample Point
	Date
	Leachate Head (m)

	HAF LMP2AR
	30/06/2021
	29.74

	HAF LMP4b
	30/06/2021
	12.44

	HAF LC4
	30/06/2021
	1.82 “inc” offset

	HAF LMP1AR
	30/06/2021
	0.90 “inc” offset

	HAF LC3
	30/06/2021
	1.67 “inc” offset




	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	Leachate Levels will continue to be monitored in accordance with Table S3.1 in Environmental Permit PP3139GB.


Part B
	Any more accurate information on the matters for notification under Part A.
	In June 1653 m3 of leachate was tankered off site for treatment. 
The levels in LMP2AR are considered to be perched due to the design of the well casing with perforations at different levels allowing leachate to enter the chamber at various heights. The pump in LMP2AR had to be removed to allow the well to be raised and waste to be tipped around it. When the dip was taken the pump in LMP2AR had been removed to allow the well to be raised and waste to be tipped around it.   
As stated in the previous S5’s (HAF288 & HAF290) the manual dips in LMP4b are thought to be due to perched levels. The level has increased by 0.17m since May.  The transducer readings in LC3 and LC4 are between the pump set points of 0.2 and 2mtr.
Transducer readings have been provided for LMP1AR, LC4 and LC3, where access is unsafe for the monitoring technician. 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment or harm which has been or may be caused by the emission
	 


	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	Please see previous notifications.

	Name*
	Elizabeth Forrest

	Post
	Environmental Data Analyst

	Date
	12.07.2021


* authorised to sign on behalf of Enovert North Ltd
	
	
	



