


Permit Number: 	YP3937SH			Operator: 		Mekatek Limited

Facility:		Amex Park			Form Number: 	Water1 / 17/08/22
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty [4]

	W1
	Total suspended solids (TSS)
	60 mg/l
	Monthly analysis of bulk daily sample.
	
	As per EN 872 and Technical Guidance Note (Monitoring) M18: Monitoring of discharges to water and sewer or other method as agreed in writing with the Regulator.
	
	

	
	Total ammonium as N 
	20mg/l (winter period) [5]
	Spot sample
	
	As per Technical Guidance Note (Monitoring) M18: Monitoring of discharges to water and sewer or other method as agreed in writing with the Regulator.
	
	

	
	
	15mg/l (summer period) [6
	
	
	
	
	

	
	Biochemical oxygen demand (5 day)
	75mg/l (winter period) [5]
	Spot sample
	
	
	
	

	
	
	40 mg/l (summer period) [6
	
	
	
	
	

	
	Oils and grease
	No visible release
	Visual inspection
	
	
	
	

	
	Temperature
	≤24ºC
	Spot readings
	
	
	
	

	
	pH
	6 to 8.5 
	Continuous
	
	
	
	

	
	Flow
	39l/second
	Continuous
	
	
	
	

	
	
	2500m³/day
	
	
	
	
	

	
	Cadmium and its compounds as Cd
	0.05mg
	Monthly analysis of bulk daily sample
	
	Various EN standards available (e.g. EN ISO 11885, EN ISO 17294-2, EN ISO 15586)
	
	

	
	Chromium and its compounds as Cr
	0.15mg
	
	
	
	
	

	
	Copper and its compounds as Cu
	0.5mg
	
	
	
	
	

	
	Lead and its compounds as Pb
	0.1mg
	
	
	
	
	

	
	Nickel and its compounds as Ni
	0.5mg
	
	
	
	
	

	
	Zinc and its compounds as Zn
	1mg
	
	
	
	
	

	
	Mercury and its compounds as Hg
	5 ug/l
	
	[bookmark: _GoBack]
	Various EN standards available (i.e. EN ISO 17852, EN ISO 12846)
	
	

	
	Free cyanide (CN-)
	0.1mg
	None set
	
	Various EN standards available (i.e. EN ISO 14403-1 and -2)
	
	

	
	
	
	
	
	
	
	

	
	Phenol index
	0.3mg
	None set
	
	EN ISO 14402
	
	

	
	Total nitrogen (Total N)
	25 mg/l
	None set
	
	EN 12260, EN ISO 11905-1
	
	

	
	Total organic carbon (TOC)
	60 mg/l
	None set
	
	EN 1484
	
	

	
	Total phosphorus (Total P)
	2 mg/l
	None set
	
	Various EN standards available (i.e. EN ISO 15681-1 and -2, EN ISO 6878, EN ISO 11885)
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Winter period is defined as 01 October to 31 March.
[6] summer period is defined as 01 April to 30 September


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

