Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
……
Reporting of ……LEACHATE…… monitoring for the period for April 2021
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL1
	Am Nitrogen
	1370
	Apr-21
	No sample
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL1
	Cadmium
	0.1
	Apr-21
	No sample
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL1
	Nickel
	0.1
	Apr-21
	No sample
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL1
	Chloride
	13713
	Apr-21
	No sample
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL1
	MP Xylene
	0.029
	Apr-21
	No sample
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL1
	Mecoprop
	0.032
	Apr-21
	No sample
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL2
	Am Nitrogen
	1370
	Apr-21
	No sample
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL2
	Cadmium
	0.1
	Apr-21
	No sample
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL2
	Nickel
	0.1
	Apr-21
	No sample
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL2
	Chloride
	13713
	Apr-21
	No sample
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL2
	MP Xylene
	0.029
	Apr-21
	No sample
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL2
	Mecoprop
	0.032
	Apr-21
	No sample
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL3
	Am Nitrogen
	1370
	Apr-21
	No sample
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL3
	Cadmium
	0.1
	Apr-21
	No sample
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL3
	Nickel
	0.1
	Apr-21
	No sample
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL3
	Chloride
	13713
	Apr-21
	No sample
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL3
	MP Xylene
	0.029
	Apr-21
	No sample
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL3
	Mecoprop
	0.032
	Apr-21
	No sample
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL4
	Am Nitrogen
	1370
	Apr-21
	200
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL4
	Cadmium
	0.1
	Apr-21
	<0.11
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL4
	Nickel
	0.1
	Apr-21
	8.7
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL4
	Chloride
	13713
	Apr-21
	279
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL4
	MP Xylene
	0.029
	Apr-21
	<1.0
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL4
	Mecoprop
	0.032
	Apr-21
	7.0
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL5
	Am Nitrogen
	1370
	Apr-21
	99.1
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL5
	Cadmium
	0.1
	Apr-21
	<0.11
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL5
	Nickel
	0.1
	Apr-21
	11.6
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL5
	Chloride
	13713
	Apr-21
	536
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL5
	MP Xylene
	0.029
	Apr-21
	<1.0
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL5
	Mecoprop
	0.032
	Apr-21
	<0.1
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL6
	Am Nitrogen
	1370
	Apr-21
	170
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL6
	Cadmium
	0.1
	Apr-21
	<0.11
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL6
	Nickel
	0.1
	Apr-21
	15.5
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL6
	Chloride
	13713
	Apr-21
	262
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL6
	MP Xylene
	0.029
	Apr-21
	<1.0
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL6
	Mecoprop
	0.032
	Apr-21
	20.6
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL7
	Am Nitrogen
	1370
	Apr-21
	<0.01
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL7
	Cadmium
	0.1
	Apr-21
	<0.11
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL7
	Nickel
	0.1
	Apr-21
	22.7
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL7
	Chloride
	13713
	Apr-21
	2,450
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL7
	MP Xylene
	0.029
	Apr-21
	<1.0
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL7
	Mecoprop
	0.032
	Apr-21
	11.3
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL8
	Am Nitrogen
	1370
	Apr-21
	0.09
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL8
	Cadmium
	0.1
	Apr-21
	<0.11
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL8
	Nickel
	0.1
	Apr-21
	38.9
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL8
	Chloride
	13713
	Apr-21
	604
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL8
	MP Xylene
	0.029
	Apr-21
	<1.0
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL8
	Mecoprop
	0.032
	Apr-21
	5.7
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	SL9
	Am Nitrogen
	1370
	Apr-21
	No sample
	INORG-L12
	22nd Apr 21
	12.69



	
	
	
	
	
	
	
	

	SL8
	Cadmium
	0.1
	Apr-21
	No sample
	1450
	22nd Apr 21
	3.93

	
	
	
	
	
	
	
	

	SL9
	Nickel
	0.1
	Apr-21
	No sample
	METALS-L
	22nd Apr 21
	5.23


	
	
	
	
	
	
	
	

	SL9
	Chloride
	13713
	Apr-21
	No sample
	INORG-L13
	22nd Apr 21
	6.71



	
	
	
	
	
	
	
	

	SL9
	MP Xylene
	0.029
	Apr-21
	No sample
	ORG-L05
	22nd Apr 21
	7.66



	
	
	
	
	
	
	
	

	SL9
	Mecoprop
	0.032
	Apr-21
	No sample
	ORG-L17
	22nd Apr 21
	8.27



	
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………[image: image1.png]


……………….  

Date 30th July 2021     



(Authorised to sign as representative of Operator)

