PAN-015132 AP3499FY Opra review

Score changed from 46 to 47

Tonnages- 
changed to reflect legal limits in permit. 10 tonnes per day Hazardous waste limit= 10*365= 3650 tonnes, the rest of the 40,000 tonnes is allocated to the next highest risk waste input which is Non-hazardous Biological.

Location- 
Sensitivity of surface water: as there is a discharge from the site there needs to be an entry. As there is not a classified water course within 2km the default of "Grade 3 or 4" has been used.

