Permit Reference Number: EPR/NP3335GR/V008



Operator: Solutia UK Ltd.
Installation: Cefn Mawr (former ‘Flexsys’ Ruabon Works) 


Form Number: W1

Reporting of Emissions to Water (other than to Sewer) for the period from ………01/07/2021…………………….to……30/09/2021………………………

	Emissions to Water

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3] [6]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	W1-final discharge
	Maximum flow rate l/s
	92.5 l/s
	43.2 l/s
	On-line Electrochemical flow meter
	09/8/21
	
	

	
	Maximum discharge volume M3/day
	8000m3
	752 m3
	On-line Electrochemical flow meter
	06/7/21
	
	

	
	Total Tetrachloroethlene ug/l
	2.5 ug/l
	<3ug/l
	GCMS –TM15/PM10
	5/7/21
	
	+/-20%

	
	Total Organic Carbon mg/l
	No Limit
	3 mg/l
	TM60/PM0
	5/7/21
	
	+/- 10%

	
	Total iron mg/l
	5.0mg/l objective
	0.024 mg/l
	TM30/PM14
	5/7/21
	
	+/-5%

	
	Total Phenol mg/l
	0.2 mg/l
	<0.01 mg/l
	TM26/PM0
	5/7/21
	
	+/-20%

	
	
	
	
	
	
	
	

	
	Maximum weekly iron result mg/l
	5mg/l objective
	0.16mg/l
	Hach Lange DR3900
	31/8/20
	
	

	
	Iron sample comparison
	5mg/l objective
	In House 0.03mg/l

Offsite 0.024mg/l
	
	6/7/20
	
	

	
	Micro Pollutants: -
	
	
	
	
	
	

	
	Toluene ug/l
	No Limits
	<5 ug/l
	GCMS-TM15/PM10
	5/7/21
	
	+/- 20%

	
	p-Xylene ug/l
	No Limits
	<2ug/l
	GCMS-TM15/PM10
	5/7/21
	
	+/- 20%

	
	Ethylmorpholine ug/l
	No Limits
	<10 ug/l
	GCMS-TM15/PM10
	5/7/21
	
	+/- 20%

	
	Aniline ug/l
	No Limits
	<0.1 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	Ethoxybenzene ug/l
	No Limits
	<10 ug/l
	GCMS-TM15/PM10
	5/7/21
	
	+/- 20%

	
	o-cresol ug/l
	No Limits
	<0.01 ug/l
	GCMS-TM26/PM0
	5/7/21
	
	+/- 20%

	
	p-cresol ug/l
	No Limits
	<0.02 ug/l
	GCMS-TM26/PM0
	5/7/21
	
	+/- 20%

	
	2,4-DCP ug/l
	No Limits
	<0.5 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	Phenyliso ug/l
	No Limits
	<0.1 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	Benzothiazole ug/l
	No Limits
	<0.1 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	2,4,6 Trichlorophenol ug/l
	No Limits
	<1 ug/l
	GCMSTM16/PM30
	5/7/21
	
	+/- 20%

	
	TMQ ug/l 
	No Limits
	<0.1 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	Phthalimide ug/l
	No Limits
	<0.1 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	MMCD ug/l
	No Limits
	<0.5 ug/l
	GCMS-TM16/PM30
	5/7/21
	
	+/- 20%

	
	Acetone (DMK)
	No Limits
	<50 ug/l
	GCMS-TM83/PM10
	5/7/21
	
	+/- 20%


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) 

[6] This form is required to be submitted on a quarterly basis. For parameters which are required to be monitored on a twice-yearly basis, and which were monitored during the previous quarter, an entry of ‘nil’ shall be recorded against this parameter. 

Signed ……I.M.Biggs……………………………………………………….  

Date………30/09/2021………………..




(authorised to sign as representative of the Operator)

Date of form: 30/09/2021 

Date of form: 30/09/2021

