Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V016

	Name of operator
	Hanson Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	03.00:00 09/07/2021


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	03:00 09/07/2021

	Reference or description of the location of the event 
	Silo 6 penthouse

	Description of where any release into the environment took place
	atmosphere

	Substances(s) potentially released
	Cement dust

	Best estimate of the quantity or rate of release of substances
	Less than 50 kg’s

	Measures taken, or intended to be taken, to stop any emission
	Stopped milling into the silo, identified the problem and  Reassigned CM5 to another silo. Further investigation required.

	Description of the failure or accident.
	Over pressurisation 


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Silo 6 filter was inspected during the day of 9th July and 10 solenoids were found not pulsing. This situation allowed compressed air to continuously pass through the filter resulting in low air pressure and in turn loss of filter performance. 

Of the 10 solenoids identified as faulty, 1 solenoid was replaced and the other 9 were repaired.


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	An interlock has been implemented to stop the milling process to silo 6 if the compressed air pressure to the filter is low for more than 10 seconds. 


	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Mill 5 was reassigned to another silo prevent any pollution.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	15/08/2019
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15/12/2019

23/12/2019

09/02/2020

07/03/2020

23/04/2020

26/04/2020
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31/01/2021
09/04/2021

15/06/2021
25/06/2021


	Name
	Stewart Mitchell

	Post
	Quality and Environment Manager

	Signature
	S. Mitchell

	Date
	13/12/2021


* authorised to sign on for and on behalf of Castle Cement Limited
