Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V016

	Name of operator
	Hanson Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	16/09/2021 13:03hrs


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	16/09/2021 13:01

	Reference or description of the location of the event 
	Dust room chute from kiln to dust room


	Description of where any release into the environment took place
	Visually just below the kiln inlet from the change over from round pipe to square chute on the dust room chute

	Substances(s) potentially released
	Dust

	Best estimate of the quantity or rate of release of substances
	50kg

	Measures taken, or intended to be taken, to stop any emission
	Door/cover re fitted on the dust room chute from the kiln to the dust room

	Description of the failure or accident.
	Door had been left off from cleaning the dust room chute.


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The cover described in the Part A is part of the chute from the kiln to the dust room located on level 1 of the PHT. The cover had been removed for cleaning earlier in the week and, although re-seated, was not bolted down.


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The cover is now bolted down and has also been added to the kiln pre-start checklist to confirm in place and secured prior to a kiln start.

Prior to this incident the chute was checked only to confirm clear but now the cover will be checked as well.


	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The area was cleaned by vacuumation. 

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	21/09/2019

23/10/2019

28/10/2019

15/12/2019

23/12/2019

09/02/2020

07/03/2020

23/04/2020

26/04/2020

10/07/2020

23/08/2020

30/08/2020

29/10/2020

05/01/2021

31/01/2021

09/04/2021

15/06/2021

25/06/2021

09/07/2021

02/08/2021

17/08/2021
20/08/2021

10/09/2021


	Name
	Stewart Mitchell

	Post
	Quality and Environment Manager

	Signature
	S. Mitchell

	Date
	13/12/2021


* authorised to sign on for and on behalf of Castle Cement Limited
