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Belt-clean manure out on conveyor in direction shown
House 2
16,000 hens in a multi-tier system Ventilation will be upgraded with the installation of six uncapped high velocity roof extraction fans, approximate positions shown
.  
Vehicle access to site
Generator with integral diesel store
Service area for egg packing, with freezer for carcass storage

House 1
16,000 hens in a single tier system.  Ventilation will be upgraded with the installation of six uncapped high velocity roof extraction fans, approximate positions shown
Summary and Key
A free range egg production site with three poultry houses and a total of 56,000 laying hen places
Belt-clean manure out on conveyor in direction shown
House 3
24,000 hens (sub-divided internally into 2 x 12,000) in a multi-tier system.  High velocity roof extraction fans (10) will be fitted, approximate positions shown
North
Feed bins


