LLWYN ISAF – September 218 SAMPLING


Schedule 6 – Notification
This page outlines the information that the operator must provide.

Units of measurement in the information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A

	Permit number
	YP3138UJ

	Name of operator
	Gwynedd Council

	Location of installation
	Llwyn Isaf Landfill, Gwynedd Council, Clynnog Fawr,

	
	Gwynedd, LL54 5DF

	Time and date of detection
	12/09/18 (site reading) 28/09/18 (lab reading)


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or technique, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection


	Date and Time of the event
	

	Reference or description of the location of the event
	

	Description of where any release into the environment took place
	

	Substance(s) potentially released
	

	Best estimate of the quality or rate of release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of limit 

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/source
	SW D (discharge)

	Parameter(s)
	Dissolved oxygen

	Limit
	80%

	Measured value and uncertainty
	76.20% (site) and  61.70% (lab reading)

	Date and time of monitoring
	12.09.18

	Measures taken, or intended to be taken, to stop the emission
	


	Time periods for notification following detection of a breach of a limit 

	Parameter
	Notification period

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substance(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B to be supplied as soon as practicable

	Any more accurate information on the matters for notification under Part A
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Currently, there is no water discharging into the Desach at location SW D (discharge). A site reading will be taken once there is a supply of water.
Please note there have been exceptionally dry conditions at the site. We were unable to get a sample in July and sampling in September was delayed at this location due to the lack of water. 

Table S3.3 – point source emissions to water 

On the 17.10.18 an on-site compliant measurement for dissolved oxygen at SW D (discharge) was recorded at 95.80%, in excess of the 80% limit specified in the permit. 


	The dates of any unauthorised emissions from the installation in the proceeding 24 months
	


	Name *
	Susan Francis

	Post
	Assistant Engineer

	Signature
	

	Date
	18.10.18


* authorised to sign on behalf of Gwynedd Council

Permit number YP3134UJ

Llwyn Isaf Landfill


