AB CONNECTORS
Review of Fugitive Emissions

January to December 2014
PC 4.1.4
Permit Number BV7443IP

Annual Review of Fugitive Emissions

Previous 12 months January to December 2013 

No fugitive emissions reported

January to December 2014
No fugitive releases reported

2014 Environmental Incident Reports

24/02/14
Cutting oil leak from drainage valve on swarf skip in bunded hard standing area. Drip tray placed under valve until valve repaired by Graig metals.
11.11.14
Oil mist fire inside Gildermeister CNC turning machine. Fire contained inside machine extinguished by AB Connectors employees using dry powder fire extinguisher. Factory evacuated, Fire Brigade in attendance and declared area safe after inspecting machine.

Trade effluent and Stack Emission Results 2014
Emissions to sewer and stack emissions within permitted limits

Reviews and Improvements to Further Minimise the Risk of Fugitive Emissions

· Skip hard standing area – Skips for the collection of metal swarf have been changed to covered skips to reduce water ingress. Cleaning and maintenance of Oil Interceptor recorded in log (see attached).

      Reduction in volume of oil/ coolant stored in area due to introduction of automatic coolant dosing system situated on factory floor.
      Two large tanks for the collection of waste oil/coolant have been removed. Waste coolant is now transferred into 1000 l IBC on shop floor.
· Chemical Storage area – Quantity of waste material / empty containers held in storage shed has been reduced due to introduction of fortnightly collection of wastes by Ecotechnology Ltd.
· Bund/drip tray installed under two nitric acid process tanks on zinc plating line
· Security of large chemical storage area improved by adding metal grating to bottom of wall/door panels. 
· Front wall of bunded area in large chemical storage area repaired and a metal plate installed to protect from damage by forklift truck (see photo)
· Filter media has been placed into the two large vents in the side of the Plating shop building to reduce the amount of particulate material being dragged in by the extraction system. (see photo)

· Security – To reduce the potential for unauthorised access to chemicals, pumps and valves within the Plating Department, all external doors have been changed to steel security doors. All internal doors to the Plating Department locked/ bolted at end of shift. A card key system for access into the department has been installed to prevent unauthorised access during the day while plant is running
· Spill response training to be organised for personnel in all departments (now completed)

· Fire marshal training to be organised for selected personnel in all departments. Weekly audit checks then to be carried out  (now completed)

· Waste stream information boards and waste stream flow charts updated
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1. Filter Media for vent                 2. Vent in side of building

    showing trapped debris
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3. Metal plate protecting edge of bunded
 storage area
