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Non-Technical Summary

Dolidre poultry unit comprises of two fan ventilated poultry house, with planning permission being sought for an additional one house which will give an overall floor area of 6086 m², under current legislative/welfare stocking density, equates to approx 140,000 bird places.
Birds will be housed at day old and de populated at around thirty-five to fourty-nine days of age with approximately seven days empty, which will give between 6 to 8.5 cycles per annum, this will be done on an all out all in basis.

Before bird arrival the houses will be pre-warmed with Biomass indirect heating with a gas-fired space heaters, or gas brooders back up. Floors will be covered to a minimum depth of 2 cm of bulk wood shavings. Temperature and humidity will be closely monitored on a daily basis to achieve a target level of 21º C and a relative humidity of 60-65%, this should achieve litter with a dry matter content of between 60-70%, which is important to minimising emissions. Ventilation is controlled by a negative pressure system. The poultry houses are fitted with roof mounted extraction fans, and sidewall air inlets. Water is via a nipple drinking system fitted with cups to reduce leakage and spills leading to drier litter.

Birds will be fed a minimum of three diets during their growth, with gradually reducing levels of protein and phosphorous as bird age increases.

Feed is delivered from the company UKASTA accredited feed mill and blown into bulk feed bins situated at the ends of the houses, from the feed bins the feed is augered into the houses and distributed to the birds via a pan feeding system.

At depletion the litter will be removed from the site, with approximately 50% being retained for spreading on the farms own land, and the remainder being sold. The farm will then be pressure washed disinfected, dried out prior to the cycle beginning again.

All wash waters will be collected and contained in underground sealed tanks.

Fallen stock during the production cycle will be collected and recorded daily, and stored in sealed secure containers awaiting collection by a licensed renderer.
The above measures are designed to reduce emissions, trees and hedges will trap dust particles reducing odour. Ammonia emissions will be reduced by reduced protein feed, maintaining good litter conditions with a dry matter content above 70%. Containment of wash waters will prevent pollutants being released to the environment.

Management plans in place to reduce odour, noise and manure spreading.

Records of tonnages of litter and wash water removal are recorded, along with assurance letters of compliance to the DEFRA codes of good agricultural practises, and sufficient available spreading land.

