
Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V013

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	05.30 - 11.30 18.9.18


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	05.30 – 11.30 18.9.18

	Reference or description of the location of the event 
	Breach of daily NOX emission from main stack, kiln 4

	Description of where any release into the environment took place
	Main stack, kiln 4

	Substances(s) potentially released
	NOx

	Best estimate of the quantity or rate of  release of substances
	531mg/Nm3 as opposed to daily max of 450mg/Nm3

	Measures taken, or intended to be taken, to stop any emission
	Stop kiln

	Description of the failure or accident.
	Indications within the kiln control room were that there was a problem with the ammonia flow. After thorough checks were carried out on both the PHT/ammonia system it was found that the ammonia storage system tank level indicator was showing an incorrect amount in storage and was virtually empty. 


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	Main stack, Kiln 4

	Parameter(s)
	High NOx level

	Limit
	450 mg/Nm3

	Measured value and uncertainty
	531mg/Nm3

	Date and time of monitoring
	Picked up on daily average of 24 hr monitoring for 18/9/18

	Measures taken, or intended to be taken, to stop the emission
	Kiln stopped

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	Main stack, kiln 4

	Substances(s) detected
	NOx

	Concentrations of substances detected
	531mg/Nm3 as opposed to daily allowance of 450mg/Nm3

	Date of monitoring/sampling
	18.9.18


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	Richie Amos

	Post
	Duty Shift Manager

	Signature
	Richie Amos

	Date
	18/09/2018


* authorised to sign on behalf of Castle Cement Limited
