Permit Number: 
EPR/EP3230BW


Operator: 

EnviroWales Limited
Facility:

Rassau Recycling Facility

Form Number: 
Sewer1 / 15/04/2014
Reporting of emissions to sewer for the period from Jan 1st 2014 to December 31st 2014
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	S1
	Flow
	350m3/day
	Daily average
	280.29
	Meter MCERTs
	30/5/14
	8%

	S1
	Suspended solids
	400 mg/l
	Weekly average
	19.8
	BS EN 872
	31/7/14
	

	S1
	Hydrocarbon oil
	No visible staining
	Daily samples
	0
	SCA blue book 77
	daily
	

	S1
	pH max
	11
	-
	9.5
	BS ISO 10523
	3/10/14
	

	S1
	pH min
	6
	
	6.6
	
	17/4/14
	

	S1
	Sulphate
	2000 mg/l
	Weekly average
	1931
	SCA blue book 136
	20/3/14
	

	S1
	Antimony and its compounds (as Sb)
	2.5 mg/l
	Weekly average
	.56
	BS EN ISO 15586
	4/9/14
	

	S1
	Arsenic and its compounds (as As)
	2.5 mg/l
	Weekly average
	.0365
	BS EN ISO 11969
	4/9/14
	

	S1
	Cadmium and its compounds (as Cd)
	0.25 mg/l
	Weekly average
	.144
	BS EN ISO 5961
	13/11/14
	

	S1
	Copper and its compounds (as Cu)
	12.5 mg/l
	Weekly average
	.0746
	BS 6068-2.29
	20/3/14
	

	S1
	Lead and its compounds (as Pb)
	5 mg/l
	Weekly average
	.4835
	BS EN ISO 15586
	29/5/14
	

	S1
	Mercury and its compounds (as Hg)
	0.125 mg/l
	Weekly average
	.00029
	BS EN 1483
	21/8/14
	

	S1
	Nickel and its compounds (as Ni)
	12.5 mg/l
	Weekly average
	.204
	BS 6068-2.29
	25/9/14
	

	S1
	Zinc and its compounds (as Zn)
	12.5 mg/l
	Weekly average
	1.03
	BS 6068-2.29
	13/11/14
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
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Signed  

Date……22nd Jan 2015.   


(Authorised to sign as representative of Operator)

