[bookmark: _GoBack]Permit Number: 	EP3230BW				Operator: 		Envirowales Limited

Facility:		Rassau Recycling Facility		Form Number: 	 Air1 / 02/11/17
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Sulphuric acid mist
	1 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	US EPA Method 8
	
	

	A1
	Dust
	5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 13284-1
	
	

	A1
	Arsenic, Cadmium, Mercury, Thallium and Selenium and their compounds expressed as As, Cd, Hg, Tl and Se

	0.5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A1
	Antimony, Copper, Lead, Nickel, Tellurium, Tin and Zinc and their compounds expressed as  Sb, Cu, Pb, Ni, Te, Sn and Zn

	2 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A2
	Dust
	5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 13284-1
	
	

	A2
	Dust
	5 mg/m3

	Monthly average

	
	BS EN 13284-1 and EN 14181

	
	

	
	
	
	
	
	
	
	

	A2
	Dust
	10 mg/m3
	Daily average
	
	BS EN 13284-1 and EN 14181
	
	

	
	
	
	
	
	
	
	

	A2
	Sulphur dioxide
	500 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14791
	
	

	A2
	Sulphur dioxide
	500 mg/m3
	Monthly average

	
	BS EN 14181
	
	

	
	
	
	
	
	
	
	

	A2
	Sulphur dioxide
	500 mg/m3
	Daily average
	
	BS EN 14791
	
	

	A2
	Hydrogen chloride
	10 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 1911
	
	


	A2
	Arsenic, Cadmium, Mercury, Thallium and Selenium and their compounds expressed as As, Cd, Hg, Tl and Se
	0.5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A2
	Antimony, Copper, Lead, Nickel, Tellurium, Tin and Zinc and their compounds expressed as  Sb, Cu, Pb, Ni, Te, Sn and Zn
	2 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A2
	Dioxins and furans (ITEQ)
	0.1 ng/m3
	Periodic over minimum 6 hours, maximum 8 hour period
	
	BS EN 1948 Parts 1, 2 and 3
	
	

	A2
	Oxides of nitrogen
	100 mg/m3
	Periodic over minimum 6 hours, maximum 8 hour period
	
	BS EN 14792
	
	

	A2
	Oxides of nitrogen
	100 mg/m3
	Monthly average
	
	BS EN 14181
	
	

	A2
	Oxides of nitrogen
	200 mg/m3
	Daily average 
	
	BS EN 14181
	
	

	A2
	Carbon monoxide
	1000 mg/m3
	Periodic over minimum 6 hours, maximum 8 hour period
	
	BS EN 15058
	
	

	A2
	Carbon monoxide
	1000 mg/m3
	Monthly average
	
	BS EN 15267-3 and EN 14181
	
	

	A2
	Volatile organic compounds (as Carbon)
	50 mg/m3
	Periodic over minimum 6 hours, maximum 8 hour period
	
	BS EN 12619
	
	

	A2
	Volatile organic compounds (as Carbon)
	50 mg/m3
	Monthly average
	
	BS EN 12619
	
	

	A2
	Volatile organic compounds (as Carbon)
	100 mg/m3
	Daily average 
	
	BS EN 12619
	
	

	A3
	Dust
	5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 13284-1
	
	

	A3
	Dust
	5 mg/m3
	Monthly average
	
	BS EN 13284-1 and EN 14181
	
	

	A3
	Dust
	10 mg/m3
	Daily average
	
	BS EN 13284-1 and EN 14181
	
	

	A3
	Sulphur dioxide
	500 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14791
	
	

	A3
	Hydrogen chloride
	10 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 1911
	
	

	A3
	Arsenic, Cadmium, Mercury, Thallium and Selenium and their compounds expressed as As, Cd, Hg, Tl and Se
	0.5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A3
	Antimony, Copper, Lead, Nickel, Tellurium, Tin and Zinc and their compounds expressed as  Sb, Cu, Pb, Ni, Te, Sn and Zn
	2 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A3
	Dioxins and furans (ITEQ)
	0.1 ng/m3
	Periodic over minimum 6 hours, maximum 8 hour period
	
	BS EN 1948 Parts 1, 2 and 3
	
	

	A3
	Oxides of nitrogen
	100 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 15267
	
	

	A3
	Carbon monoxide
	150 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 15058
	
	

	A3
	Volatile organic compounds (as Carbon)
	50 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 12619
	
	

	A4
	Dust
	5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 13284-1
	
	

	A4
	Dust
	5 mg/m3
	Monthly average
	
	BS EN 13284-1 and EN 14181
	
	

	A4
	Dust
	10 mg/m3
	Daily average
	
	BS EN 13284-1 and EN 14181
	
	

	A4
	Arsenic, Cadmium, Mercury, Thallium and Selenium and their compounds expressed as As, Cd, Hg, Tl and Se
	0.5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A4
	Antimony, Copper, Lead, Nickel, Tellurium, Tin and Zinc and their compounds expressed as  Sb, Cu, Pb, Ni, Te, Sn and Zn
	2 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A5
	Sulphur dioxide
	50 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14791
	
	

	A5
	Oxides of nitrogen
	100 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 15267
	
	

	A5
	Carbon monoxide
	150 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 15058
	
	

	A5
	Volatile organic compounds (as Carbon)
	50 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 12619
	
	

	A6
	Lead and its compounds expressed as Pb
	2 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14385
	
	

	A6
	Dust
	5 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 13284-1
	
	

	A6
	Sulphur dioxide
	500 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 14791
	
	

	A6
	Oxides of nitrogen
	100 mg/m3
	Periodic over minimum 30 minutes, maximum 8 hour period
	
	BS EN 15267
	
	

	A7
	Dust
	No visible emission
	N/A
	
	N/A
	
	

	A8
	Dust
	No visible emission
	N/A
	
	N/A
	
	

	Ambient air monitor located at Garnlydan School at 316600, 212400
	Particulate matter 
	N/A
	Continuous
	
	EN12341:2014
	
	

	Ambient air monitor located at Garnlydan School at 316600, 212400
	Lead
	N/A
	Continuous
	
	EN12341:2014
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	EP3230BW				Operator: 		Envirowales Limited

Facility:		Rassau Recycling Facility		Form Number: 	Sewer1 / 02/11/17
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Biological oxygen demand
	10 mg/l
	Spot sample
	
	BS EN 1899-1
	
	

	S1
	Arsenic and its compounds expressed as
	2.5 mg/l
	Spot sample
	
	BS EN ISO 17294-2
	
	




[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

