Permit Reference Number:

Installation:

Operator:
Permit Reference Number: BX72821S

Installation: InBev Magor Brewery

Operator: InBev UK Ltd

rm Number : A1

Reporting of Emissions to Air for the period from …1st January to 30th June 2015
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	A5
	Oxides of nitrogen as NO2
	350mg/m3 [7]
	Not operational
	BS ISO 10849:1996
	Not operational
	Mcerts MC 050056/00
	Not operational

	A5
	Carbon monoxide
	350mg/m3 [7]
	Not operational
	BS ISO 12039
	Not operational
	Mcerts MC 050056/00
	Not operational

	A5
	Oxygen
	None
	Not operational
	BS ISO 12039
	Not operational
	
	Not operational

	A5
	Temperature
	None
	Not operational
	
	Not operational
	
	Not operational

	A6
	Oxides of nitrogen as NO2
	350mg/m3 [7]
	Not operational
	BS ISO 10849:1996
	Not operational
	Mcerts MC 050056/00
	Not operational

	A6
	Carbon monoxide
	350mg/m3 [7]
	Not operational
	BS ISO 12039
	Not operational
	Mcerts MC 050056/00
	Not operational

	A6
	Oxygen
	None
	Not operational
	BS ISO 12039
	Not operational
	
	Not operational

	A6
	Temperature
	None
	Not operational
	
	Not operational
	
	Not operational

	A5
	Oxides of nitrogen as NO2
	350mg/m3 [7]
	Not operational
	BS ISO 10849:1996
	Not operational
	Mcerts MC 050056/00
	Not operational

	A5
	Carbon monoxide
	350mg/m3 [7]
	Not operational
	BS ISO 12039
	Not operational
	Mcerts MC 050056/00
	Not operational

	A5
	Oxygen
	None
	Not operational
	BS ISO 12039
	Not operational
	
	Not operational

	A5
	Temperature
	None
	Not operational
	
	Not operational
	
	Not operational

	A6
	Oxides of nitrogen as NO2
	350mg/m3 [7]
	Not operational
	BS ISO 10849:1996
	Not operational
	Mcerts MC 050056/00
	Not operational

	A6
	Carbon monoxide
	350mg/m3 [7]
	Not operational
	BS ISO 12039
	Not operational
	Mcerts MC 050056/00
	Not operational

	A6
	Oxygen
	None
	Not operational
	BS ISO 12039
	Not operational
	
	Not operational

	A6
	Temperature
	None
	Not operational
	
	Not operational
	
	Not operational


Form Number : A1

[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.}

[6] Corrected to 273K, 101.3kPa, 3% oxygen, dry

[7] Corrected to 273K, 101.3kPa, 15% oxygen, dry

Signed …………Kathryn Fowler………………………………………………….  

Date………16/7/2015   



(authorised to sign as representative of the Operator)

Form Number : W1

Reporting of Emissions to Water (other than to Sewer) for the period from 1st April to 30th June 2015
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/

Certification [4]
	Uncertainty

[5]

	W2
	Flow
	10,000m3/day
	5738
	Continuous / cumulative – AAB flow meter
	5th May 2015
	MCerts accredited
	+/- 1.04 %

	W2
	Flow
	126 litres/s
	61.6
	Spot – AAB flow meter
	5th May 2015
	MCerts accredited
	+/- 1.04 %

	W2
	pH
	5 – 9 [6]
	7.0 – 8.7
	Continuous sample 
	22nd June 2015 – 22nd June 2015

	EA approved (IP 18)
	+/- 0.05 pH

	W2
	Temperature
	30°C
	27.4
	Continuous sample – knick in line meter
	4th June 2015
	EA approved (IP 18)
	+/- 1 degree C

	W2
	BOD
	200mg/l
	8
	SCA Blue Book 130
ISBN 0117522120
	13th June 2015
	UKAS Lab 1314
	20.1%

	W2
	COD
	450mg/l
	79
	SCA Blue Book 97
ISBN 0117519154
	22nd June 2015
	UKAS Lab 1314
	5.8%

	W2
	Suspended Solids
	150mg/l
	75
	SCA Blue Book 105
ISBN 011751957X
	15th June 2015
	UKAS Lab 1314
	19.7%

	W2
	Total cadmium & its compounds
	0.005mg/l

(as annual average)
	
	
	
	
	

	W2
	Total chromium & its compounds
	0.015mg/l

(as annual average)
	
	
	
	
	

	W2
	Total copper & its compounds
	0.01mg/l

(as annual average)
	
	
	
	
	

	W2
	Total mercury & its compounds
	0.0005mg/l

(as annual average)
	
	
	
	
	

	W2
	Total nickel & its compounds
	0.03mg/l

(as annual average)
	
	
	
	
	

	W2
	Total zinc & its compounds
	0.07mg/l

(as annual average)
	
	
	
	
	

	W2
	Total arsenic & its compounds
	0.025mg/l

(as annual average)
	
	
	
	
	

	W2
	Total iron & its compounds
	None
	
	
	
	
	

	W2
	Total cadmium & its compounds
	9150g
	
	
	
	
	

	W2
	Total mercury & its compounds
	915g
	
	
	
	
	


Form Number : W1

[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

[6] The emission limit values for {pH} are expressed as {minimum and maximum individual values}.

Signed ……………Kathryn Fowler……………………………………………….  

Date………16/7/2015………………..




(authorised to sign as representative of the Operator)

	Parameter
	
	               Result (ppm)
	

	
	
	
	

	Hydrogen sulphide content at outlet of hydrogen sulphide scrubber
	409 (Jan 2015)
	

	Hydrogen sulphide content at entry to gas engine
	409 (Jan 2015)
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


Reporting of biogas quality for the year 1st January to 30th June 2015 ………….

Permit Number: 
EPR/BX7282IS


Operator: 

Inbev UK Ltd

Facility:

Magor Brewery


Form Number: 
Gas1
Date of form 

19/07/11

	Operator’s comments :

The issue with the H2S readings has since been resolved.  

This was discussed at regular intervals, and the root cause was anomalies within the SCADA software that could cause the readings to go off scale. 




The result given is the maximum result over the reporting period

Signed ……………………Kathryn Fowler……………………………………….  

Date………16/7/2015………………..   



(Authorised to sign as representative of Inbev UK Ltd)

Permit Reference Number: AannnnAA

Date of Form: dd/mm/yy

Permit Reference Number: BX7282IS

Date of Form: 01/06/05

