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Design and Build Measures 
SPTS’ Ringland Way site (the “installation”) was designed so that, in general, decommissioning activities should avoid any risk of pollution. With the exception of the drainage water interceptors, there are no underground storage tanks at the installation. All gas storage vessels and associated pipework are located above ground. The only subsurface pipework at the installation relates to the drainage water and supply systems. Asbestos materials were not used in the construction of the installation, confirmed by a third party inspection performed in January 2015.
In the Event of Site Closure 

In the event of a closure SPTS will appoint a project management team to manage and oversee the closure and decommissioning of the entire installation.  Without limitation and in no particular order, the following actions would take place
· All SPTS machine systems and associated equipment located within the Manufacturing Cleanroom, R&D areas and Training locations are to be safely decommissioned and either relocated to other SPTS sites or dismantled and recycled or scrapped. All contaminated parts are to be disposed via a specialist hazardous waste contractor. 
·  All bottled gas cylinders on the installation should be isolated from the supply panels, decommissioned and made available for collection by the relevant gas supplier.
· All gas pipework infrastructures on the installation should be Nitrogen purged and decommissioned.

· The bulk LN2 & oxygen tanks (and associated equipment) should be isolated, decommissioned and removed from the installation by the third party suppliers of such tanks.
· All Gas Reactor Columns should be cleaned, decommissioned and relocated to other sites or re-sold to the supplier.

· The clean room “Wet Bench” should be cleared of all chemicals and disposed of by a specialist hazardous waste contractor. The Wet bench will be dismantled and scrapped via the hazardous waste supplier.
· The red diesel drum for the back-up generator and the waste oil drum, currently stored in the locked bund will be disposed of via the specialist hazardous waste contractor.
· All plant room services to be shutdown and decommissioned. Chillers and air conditioning units should have all refrigerant decanted and removed from installation. Process Cooling Water system and cooling towers should be treated and drained.  

· All other locations including the canteen, machine shop, storage rooms and office locations should be cleared of all equipment, stock and furniture which should either be sold, recycled or scrapped. All areas to be left clear.
· Main Stores should be cleared and stored parts relocated to other SPTS sites, sold or scrapped.  

· Waste Disposal – All waste to be segregated into the usual waste streams and collected by the current waste contractor.  Hazardous waste will be labelled and recorded and put to tender with specialist hazardous waste contractors.
· Sampling – SPTS has robust procedures in place in relation to pollution prevention and control, emergency preparedness and response, and ensures that no releases are made to air, land and water.  However, should sampling be required following any closure of the installation, SPTS will co-operate in arranging this.  SPTS commits to take remedial action should any pollution occur as a result of the installation closure activities.
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