Brynrorin Farm existing Poultry House -  Housing/Management Review –05/04/2015
Housing

Brynrorin farm poultry unit comprises of a single purpose built free range poultry house.

Construction was completed in 2009. Building is of steel construction with internal support posts. Dwarf walls are of concrete mass construction and regularly checked for integrity as per the maintenance schedule. Ventilation is currently natural ventilation, this will be changed to high velocity roof mounted extraction fans, and this will give far better dispersion of odour associated with low level release natural ventilation.
With the change to high velocity roof extraction the house ventilation will be operated with slight negative pressure ensuring no fugitive releases from side inlets or pop holes.   
Concrete base was laid over a plastic membrane to prevent moisture rising and conversely prevent any liquid or seepage contaminating groundwater.

Building is integrally sound preventing any ingress of rainwater.

Roof structure is sound, with no plans for refurbishment in the immediate future, any refurbishments will assess levels and condition of the insulation and upgrade accordingly.

Guttering and downspouts are of adequate size for the roof span, and regularly cleaned and inspected.

Routine maintenance schedule ensures that the poultry houses are kept up to BAT.

Housing Overview

	Description
	Condition
	BAT

	Structure in good condition
	Satisfactory
	Yes

	Damp proof membrane
	Satisfactory
	Yes

	Insulation Levels
	Satisfactory (100mm)
	Yes

	Concrete Floors
	Satisfactory
	Yes

	Forced ventilation with littered floor
	Satisfactory
	Yes

	Nipple drinker system
	Satisfactory
	Yes


Management

No heating is required for the layer birds as they generate enough of their own heat.
Ventilation will be by means of roof-mounted fans, routinely serviced by a qualified electrician. (ACP requirement)

Drinkers are of the Nipple type with drip cups fitted to minimise wastage, ensuring litter remains friable with dry matter content in the region of 65%. This will minimise the ammonia emissions during the egg production process.

All litter and wash waters are exported off site for use on operator controlled land in strict accordance with the farms manure management plan. 
General management techniques conform to the standards in How to Comply (chapter 6). These techniques are comprehensively covered under the ACP assurance scheme to which the site is an accredited member.

An electrical service is carried out prior to the placement of each flock, along with regular calibration of controls and sensors.

Management techniques fully provide the welfare needs of the poultry, and minimise emissions to the environment.

House Management

	Topic
	Standard
	BAT

	Ventilation
	Level controlled
	Yes

	Temperature
	Level controlled
	Yes

	Humidity
	Level controlled
	Yes

	Feeders
	Satisfactory
	Yes

	Drinker system
	Monitored Daily
	Yes

	Litter
	Friability maintained
	Yes

	Wash waters
	Fully contained
	Yes

	Manure management
	Exported offsite
	Yes

	Feed
	Supplied by UKASTA reg Feedmill
	Yes

	
	
	


