Non-Technical Summary Fford Fawr Farm
The poultry operations at Fford Fawr Farm, consists of five fan ventilated poultry houses of various sizes. This will give a bird placing of approximately 186,700, under the current legislative/welfare stocking density. All houses have concrete floors with adequate levels of insulation. The houses are between 25 and 3 years old.

Birds will be housed at day old and de populated at around thirty-three to thirty-nine days of age with approximately seven days empty, which will give 7.5 cycles per annum, this will be done on an all out all in basis.

Before bird arrival the houses will be pre-warmed by hot water radiators, existing LPG heating system will be retained as back up. Floors will be covered to a minimum depth of 2 cm of bulk wood shavings. Temperature and humidity will be closely monitored on a daily basis to achieve a target level of 21º C and a relative humidity of 60-65%, this should achieve litter with a dry matter content of between 60-70%, which is important to minimising emissions. Ventilation is controlled by a negative pressure system using roof-mounted fans with sidewall vent inlets. Water is via a nipple drinking system fitted with cups to reduce leakage and spills leading to drier litter.

Birds will fed a minimum of three diets during their growth, with gradually reducing levels of protein and phosphorous to increasing bird age.

Feed is delivered from the company UKASTA accredited feed mill and blown into bulk feed bins situated at the ends of the houses, from the feed bins the feed is augered into the houses and distributed to the birds via a pan feeding system.

At depletion the litter will be removed from the site for use on the farm or sold. The farm will then be pressure washed disinfected, dried out prior to the cycle beginning again. All wash waters are contained in underground sealed tanks.

Fallen stock during the production cycle will be collected and recorded daily. These will be collected by a licensed collection agent under the National Fallen Stock Scheme.

Emissions from the installation will include ammonia, odour, noise and dust.

Lower ammonia emissions will be achieved by the reduction of protein in the feed.

Modern spill proof drinker system together with correct ventilation will give a lower moisture level in the litter, which reduces odour.

Containment of wash waters will prevent pollution to watercourse or land.

Tree/shrub planting around the site will trap dust particles, and also screen noise.

