Permit Reference Number: SP3531SK





Operator: Tradebe Ltd

Installation: Gwent Waste Management Centre




Form Number: S1
Reporting of Emissions to Sewer for the period from …………01/04/2015…………….to………30/06/2015……………

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Ammonia un-ionised as N [6]
	N/a
	246
	mg/L
	Welsh Water
	30 Apr 15     12:57hrs
	UKAS
	+/- 3%

	S1
	Cyanide
	N/a
	1
	mg/L
	Colorimetry
	26 Jun 15     10:30hrs
	-
	+/- 3%

	S1
	Suspended solids
	N/a
	1222
	mg/L
	Welsh Water
	02 Apr 15     11:40hrs

	UKAS
	+/- 1%

	S1
	Flow
	N/a
	14
	L/s
	Mag Flow
	30 Jun 15     11:02hrs
	MCerts
	+/- 2%

	S1
	Lead & its compounds (Total Pb)
	N/a
	<0.1
	mg/L
	Welsh Water
	17 Jun 15     12:27hrs

	UKAS
	+/- 5%

	S1
	Nickel & its compounds (Total Ni)
	N/a
	2.6
	mg/L
	Welsh Water
	10 Jun 15     10:17hrs
	UKAS
	+/- 5%

	S1
	Zinc & its compounds (Total Zn)
	N/a
	1.4
	mg/L
	Welsh Water
	08 Apr 15     14:27hrs

	UKAS
	+/- 5%

	S1
	Chromium & its compounds (Total Cr)
	N/a
	2.4
	mg/L
	Welsh Water
	21 May 15     11:30hrs

	UKAS
	+/- 5%

	S1
	Copper & its compounds (Total Cu)
	N/a
	1.6
	mg/L
	Welsh Water
	07 May 15     13:12hrs

	UKAS
	+/- 5%

	S1
	pH
	N/a
	7.5
11.7
	pH units
	Welsh Water
	24 Jun 15     11:33hrs
24 Apr 15     14:00hrs
	UKAS
	+/- 0.5


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated

[6] 
‘Ammonia un-ionised as N’ calculated using Ammonia Calculator located on http://www.hbuehrer.ch/Rechner/Ammonia.html using Total Ammonia = 255mg/L, pH = 10.9 and Temperature = 18oC.
Signed ……[image: image1.emf]……Mark Griffiths…………………………….  

Date…………27 Jul 15……………..




(Authorised to sign as representative of the Operator)

