Permit Reference Number: SP3531SK





Operator: Tradebe Ltd

Installation: Gwent Waste Management Centre




Form Number: S1
Reporting of Emissions to Sewer for the period from …………01/01/2015…………….to………31/03/2015……………

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Ammonium as N
	N/a
	230
	mg/L
	Welsh Water
	18 Feb 15     12:45hrs
	UKAS
	+/- 3%

	S1
	Cyanide
	N/a
	1
	mg/L
	Colorimetry
	19 Feb 15     11:06hrs
	-
	+/- 3%

	S1
	Suspended solids
	N/a
	260
	mg/L
	Welsh Water
	05 Mar 15     12:11hrs

	UKAS
	+/- 1%

	S1
	Flow
	N/a
	18.6
	L/s
	Mag Flow
	30 Jan 15     11:21hrs
	MCerts
	+/- 2%

	S1
	Lead & its compounds (Total Pb)
	N/a
	<0.2
	mg/L
	Welsh Water
	05 Mar 15     12:11hrs

	UKAS
	+/- 5%

	S1
	Nickel & its compounds (Total Ni)
	N/a
	1.2
	mg/L
	Welsh Water
	05 Mar 15     12:11hrs
	UKAS
	+/- 5%

	S1
	Zinc & its compounds (Total Zn)
	N/a
	1.8
	mg/L
	Welsh Water
	04 Feb 15     12:34hrs

	UKAS
	+/- 5%

	S1
	Chromium & its compounds (Total Cr)
	N/a
	0.7
	mg/L
	Welsh Water
	07 Jan 15     13:05hrs

	UKAS
	+/- 5%

	S1
	Copper & its compounds (Total Cu)
	N/a
	3.2
	mg/L
	Welsh Water
	12 Feb 15     12:09hrs

	UKAS
	+/- 5%

	S1
	pH
	N/a
	9.20
11.0
	pH units
	Welsh Water
	12 Feb 15     12:09hrs
05 Mar 15     12:11hrs
	UKAS
	+/- 0.5


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated

Signed ……[image: image1.emf]……Mark Griffiths…………………………….  

Date…………09 Apr 15……………..




(Authorised to sign as representative of the Operator)

