Permit Reference Number: SP3531SK





Operator: Tradebe Ltd

Installation: Gwent Waste Management Centre




Form Number: S1
Reporting of Emissions to Sewer for the period from …………01/07/2016…………….to………30/09/2016……………

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Ammonia un-ionised as N [6]
	N/a
	35.4
	mg/L
	2:550 using Aquachem 600
	15 Jul 16      10:13hrs
	UKAS
	+/- 3%

	S1
	Cyanide

	N/a
	1
	mg/L
	Colorimetry
	27 Jul 16      09:55hrs
	-
	+/- 3%

	S1
	Suspended solids

	N/a
	1037
	mg/L
	2:724 using gravimetry
	19 Aug 16      13:58hrs
	UKAS
	+/- 1%

	S1
	Flow

	N/a
	1.98
	L/s
	Mag Flow
	26 Jul 16      11:38hrs
	MCERTS
	+/- 2%

	S1
	Lead & its compounds (Total Pb)
	N/a
	<0.2
	mg/L
	2:311 using ICP-MS
	19 Aug 16      13:58hrs
	UKAS
	+/- 5%

	S1
	Nickel & its compounds (Total Ni)
	N/a
	3.9
	mg/L
	2:311 using ICP-MS
	27 Jul 16      10:00hrs
	UKAS
	+/- 5%

	S1
	Zinc & its compounds (Total Zn)
	N/a
	3.4
	mg/L
	2:311 using ICP-MS
	21 Jul 16      09:30hrs
	UKAS
	+/- 5%

	S1
	Chromium & its compounds (Total Cr)
	N/a
	1.3
	mg/L
	2:311 using ICP-MS
	27 Sep 16      11:53hrs
	UKAS
	+/- 5%

	S1
	Copper & its compounds (Total Cu)
	N/a
	2.5
	mg/L
	2:311 using ICP-MS
	27 Jul 16      10:00hrs
	UKAS
	+/- 5%

	S1
	pH
	N/a
	7.55
10.22
	pH units
	2:721 using meter
	06 Sep 16      13:10hrs 13 Sep 16      14:00hrs
	UKAS
	+/- 0.5


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where a reference number is given this refers to Wessex Water UKAS accredited lab (0905) documented in-house methods to meet the requirements of the Environment Agency MCERTS Performance Standard – sampling and chemical testing of untreated sewage, sewage effluent and trade effluent and the instrument used. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated

[6] 
‘Ammonia un-ionised as N’ calculated using Ammonia Calculator located on http://www.hbuehrer.ch/Rechner/Ammonia.html using Total Ammonia = 229mg/L, pH = 8.6 and Temperature = 22oC.
Signed ……[image: image1.emf]……Mark Griffiths…………………………….  

Date…………28 Oct 16……………..




(Authorised to sign as representative of the Operator)

