Permit Reference Number: SP3531SK





Operator: Tradebe Ltd

Installation: Gwent Waste Management Centre




Form Number: S1
Reporting of Emissions to Sewer for the period from …………01/07/2016…………….to………30/09/2016……………

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Ammonia un-ionised as N [6]
	N/a
	35.4
	mg/L
	Welsh Water
	15 Jul 16      10:13hrs
	UKAS
	+/- 3%

	S1
	Cyanide

	N/a
	1
	mg/L
	Colorimetry
	27 Jul 16      09:55hrs
	-
	+/- 3%

	S1
	Suspended solids

	N/a
	1037
	mg/L
	Welsh Water
	19 Aug 16      13:58hrs
	UKAS
	+/- 1%

	S1
	Flow

	N/a
	1.98
	L/s
	Mag Flow
	26 Jul 16      11:38hrs
	MCERTS
	+/- 2%

	S1
	Lead & its compounds (Total Pb)
	N/a
	<0.2
	mg/L
	Welsh Water
	19 Aug 16      13:58hrs
	UKAS
	+/- 5%

	S1
	Nickel & its compounds (Total Ni)
	N/a
	3.9
	mg/L
	Welsh Water
	27 Jul 16      10:00hrs
	UKAS
	+/- 5%

	S1
	Zinc & its compounds (Total Zn)
	N/a
	3.4
	mg/L
	Welsh Water
	21 Jul 16      09:30hrs
	UKAS
	+/- 5%

	S1
	Chromium & its compounds (Total Cr)
	N/a
	1.3
	mg/L
	Welsh Water
	27 Sep 16      11:53hrs
	UKAS
	+/- 5%

	S1
	Copper & its compounds (Total Cu)
	N/a
	2.5
	mg/L
	Welsh Water
	27 Jul 16      10:00hrs
	UKAS
	+/- 5%

	S1
	pH
	N/a
	7.55
10.22
	pH units
	Welsh Water
	06 Sep 16      13:10hrs 13 Sep 16      14:00hrs
	UKAS
	+/- 0.5


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated

[6] 
‘Ammonia un-ionised as N’ calculated using Ammonia Calculator located on http://www.hbuehrer.ch/Rechner/Ammonia.html using Total Ammonia = 229mg/L, pH = 8.6 and Temperature = 22oC.
Signed ……[image: image1.emf]……Mark Griffiths…………………………….  

Date…………28 Oct 16……………..




(Authorised to sign as representative of the Operator)

