Schedule 6 - Notification 

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission.  Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	PPC Permit
	LP3630MR

	Name of operator
	CEMEX UK Materials Limited

	Location of Installation
	Whitehall Landfill, Old Port Road, Wenvoe, 

	
	Cardiff, Glamorgan CF5 6AW

	Time and date of the detection 
	14th  October  2016

	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	

	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	BH1                                            

	Parameter(s)
	Iron                                           Ammoniacal Nitrogen as N                              

	Limit
	200 µg/l                                      0.39 mg/l

                                 

	Measured value and uncertainty
	358 µg/l    (Retest   <120 µg/l)      0.92 mg/l    Retest not requested due to stability time limitations

	Date and time of monitoring
	Monthly sampling  04/10/2016

	Measures taken, or intended to be taken, to stop the emission
	Continue with routine monthly monitoring. 


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	Carbon Dioxide or methane in external boreholes 
	24 hours

	Emissions to groundwater
	24 hours


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The retest result for the iron appears to suggest the original result was unreliable. An additional sample will be collected in November in order to confirm. 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	N/A

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	N/A


	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	02nd January  2014, 14th July  2014, 28th August 2014, 17th September  2014, 15th October 2014, 14th November  2014, 11th December 2014, 12th January 2015, 21st July 2015  01st  October 2015 02th  November 2015

	Name*
	Karen Magee

	Post
	Data Co-ordinator

	Signature


	[image: image1.emf]


	Date
	14th  October  2016


* authorised to sign on behalf of CEMEX UK Materials Ltd
