Schedule 6 - Notification 

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission.  Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	PPC Permit
	LP3630MR

	Name of operator
	CEMEX UK Materials Limited

	Location of Installation
	Whitehall Landfill, Old Port Road, Wenvoe, 

	
	Cardiff, Glamorgan CF5 6AW

	Time and date of the detection 
	02nd October 2015

	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	

	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	GM10

	Parameter(s)
	Carbon dioxide

	Limit
	6.0% 

	Measured value and uncertainty
	6.3% 

	Date and time of monitoring
	Monitored 01/10/15

	Measures taken, or intended to be taken, to stop the emission
	The Landfill gas monitoring action plan has been invoked.  The previous readings at this borehole have been checked and were found to be within limits. Future results will be checked and if breached then monitoring frequency will increase.  


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	Carbon Dioxide or methane in external boreholes 
	24 hours

	Emissions to groundwater
	24 hours


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The Landfill gas monitoring action plan has been invoked.  The previous readings at this borehole have been checked and were found to be within limits. Future results will be checked and if breached then monitoring frequency will increase.  

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	

	Name*
	Karen Magee

	Post
	Data Co-ordinator

	Signature
	[image: image1.emf]


	Date
	02nd October 2015


* authorised to sign on behalf of CEMEX UK Materials Ltd
