Permit Reference Number : UP3237CP



Operator : Solway Foods Ltd
Installation : Rogerstone Park





Form Number : A1

Reporting of Emissions to Air for the period from Jan 1st 2014………………………….to…Dec 31st 2014
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	A1
	NOx
	----
	4.35
	BS EN 14792:2005
	02/12/14  12:15-13:15
	UKAS/MCERTS
	3%

	A1
	CO
	​​​​----
	18.11
	BS EN 15058:2006
	02/12/14  12:15-13:15
	UKAS/MCERTS
	4%

	A1
	Particulates
	----
	2.33
	BS EN 13284-1
	02/12/14  11:40-12:37
	UKAS/MCERTS
	15%

	A2
	NOx
	​​​​----
	112.37
	BS EN 14792:2005
	04/12/14  08:50-19:50
	UKAS/MCERTS
	3%

	A2
	CO
	----
	12.92
	BS EN 15058:2006
	04/12/14  08:50-19:50
	UKAS/MCERTS
	4%

	A2
	Particulates
	​​​​----
	13.48
	BS EN 13284-1
	04/12/14  08:50-19:50
	UKAS/MCERTS
	15%

	A3
	NOx
	----
	106.16
	BS EN 14792:2005
	08/01/15  10:00-11:00
	UKAS/MCERTS
	3%

	A3
	CO
	​​​​----
	0.72
	BS EN 15058:2006
	08/01/15  10:00-11:00
	UKAS/MCERTS
	3%

	A3
	Particulates
	----
	0.5
	BS EN 13284-1
	08/01/15  09:46-10:46
	UKAS/MCERTS
	87%

	A4
	NOx
	​​​​----
	108.06
	BS EN 14792:2005
	08/01/15  11:30-12:30
	UKAS/MCERTS
	3%

	A4
	CO
	----
	1.40
	BS EN 15058:2006
	08/01/15  11:30-12:30
	UKAS/MCERTS
	3%

	A4
	Particulates
	​​​​----
	0.55
	BS EN 13284-1
	08/01/15  11:31-12:31
	UKAS/MCERTS
	87%

	A5
	NOx
	----
	1.25
	BS EN 14792:2005
	08/01/15  13:15-13:55
	UKAS/MCERTS
	87%

	A5
	CO
	​​​​----
	117.07
	BS EN 15058:2006
	08/01/15  13:05-13:42
	UKAS/MCERTS
	3%

	A5
	Particulates
	----
	1.25
	BS EN 13284-1
	08/01/15  13:15-13:55
	UKAS/MCERTS
	87%

	A6
	NOx
	​​​​----
	16.41
	BS EN 14792:2005
	03/12/14   09:05-10:05
	UKAS/MCERTS
	4%

	A6
	CO
	----
	48.91
	BS EN 15058:2006
	03/12/14   09:05-10:05
	UKAS/MCERTS
	3%

	A6
	Particulates
	​​​​----
	2.58
	BS EN 13284-1
	03/12/14   09:03-10:03
	UKAS/MCERTS
	15%

	A7
	NOx
	----
	2.77
	BS EN 14792:2005
	03/12/14   12:50-13:50
	UKAS/MCERTS
	4%

	A7
	CO
	​​​​----
	269.42
	BS EN 15058:2006
	03/12/14   12:50-13:50
	UKAS/MCERTS
	3%

	A7
	Particulates
	----
	2.64
	BS EN 13284-1
	03/12/14   12:450-13:43
	UKAS/MCERTS
	5%


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 
Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)

Permit Reference Number : UP3237CP




Operator : Solway Foods Ltd
Installation : Rogerstone Park






Form Number : S1

Reporting of Emissions to Sewer for the period from Jan 1st 2014………………………….to…Dec 31st 2014
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	S1
	pH
	
	6.4
	
	
	
	

	S1
	Flow Rate
	
	1541m3/day
	Welsh Water 
	Fortnightly
	
	

	S1
	COD
	
	1131
	Chemical Oxygen Demand (dichromate Value) of Polluted and waste waters 1986 (2nd Edition)
	1st Jan 14-31st Dec 14
	Hmso isbn:011 7519154
	3.5% High Standard

	S1
	Suspended solids
	
	520
	Suspended,Settleable & total dissolved Solids in waters and effluents 1980
	1st Jan 14-31st Dec 14
	Hmso isbn 01751957x
	19.7% High Standard

	S1
	Cadmium
	0.01 mg/l [6]
	0.0000215
	Mass Balance Calc
	1st Jan 14-31st Dec 14
	Msds Data
	

	S1
	Mercury
	0.0001 mg/l [6]
	0.0000606
	Mass Balance Calc
	1st Jan 14-31st Dec 14
	Msds Data
	

	S1
	Cadmium and its compounds
	2800 g/year[6]
	13.49 g/year
	Mass Balance Calc
	1st Jan 14-31st Dec 14
	Msds Data
	

	S1
	Mercury and its compounds
	330 g/year [6]
	37.98 g/year
	Mass Balance Calc
	1st Jan 14-31st Dec 14
	Msds Data
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated). 

[6] The emission limit values for cadmium and mercury are expressed as maximum individual values.
Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)

Permit Reference Number :  UP3237CP




Operator : Solway Foods Ltd
Installation : Rogerstone Park






Form Number : R1

Reporting of Waste Disposal and Recovery for the year Jan 1st 2014………………………….to…Dec 31st 2014
	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	1) Non -Hazardous Wastes (packed and loose food to AD Plant)
	AD Plant
	5576
	5576
	
	
	Total non hazardous waste
	Total hazardous waste
	Total waste per unit output

	Category 3 waste unfit for human consumption non-haz. Waste (sludge/ETP skip/potato sludge) 
	AD Plant
	8,303
	8,303
	
	2011
	15254
	1.4
	0.60

	Other non-haz. wastes
	Recycling
	685
	685
	
	2012
	13,324
	3
	0.58

	Total non-haz. waste
	
	14564
	14564
	
	2013
	15366
	5.33
	0.59

	
	
	
	
	
	2014
	14564
	2.9
	0.54

	Total Haz. Waste
	Recovered
	2.9
	2.9
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	TOTAL WASTE
	-
	14566.9
	14566.9
	
	
	
	
	


	Operator’s comments :

All food (aside from recycling waste streams which are exported from site) are sent to the AD Plant. The Plant ran into difficulties at the end of the year. SSE are still responsible for our waste streams and were directing it, directly from our site, to alternative AD recipients. 
Recycling streams sent from site include paper, office cartridges, cardboard, plastic, metal and wooden pallets. 

Hazardous waste is minimal and generated through engineering practices. The small amount this year includes waste oil, ammonia contained in water, and lighting tubes. All hazardous waste documentation is retained in the Services Engineering department, as site export through a single point is deemed the most efficient method of control. 


Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)

Permit Reference Number : UP3237CP




Operator : Solway Foods Ltd
Installation : Rogerstone Park






Form Number : WU1
Reporting of Water Usage for the year Jan 1st 2014………………………….to…Dec 31st 2014
	Water Source
	Usage

(m3)
	Specific Usage 

(m3/t)

	
	
	

	
	
	

	Mains water
	
	

	2011
	558874
	22.02

	2012
	501772
	21.93

	2013
	579250
	22.43

	2014
	626567
	23.18

	
	
	


	Operator’s comments: Increased production has resulted in an increase in mains water consumption. Increase in water also due to some hygiene cleaning schedules improvements or extra requirements. 



Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)

Permit Reference Number : UP3237CP




Operator : Solway Foods Ltd
Installation : Rogerstone Park






Form Number : E1

Reporting of Energy Usage for the year Jan 1st 2014………………………….to…Dec 31st 2014
	Energy Source
	Energy Usage
	CO2
Produced

(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2

 produced
	CO2 per unit output

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	2011
	124,600
	22,275
	0.88

	Electricity *
	MWh (23,938,500)
	57,452,400
	9543
	
	2012
	111278
	20,029
	0.88

	Natural Gas
	tonnes
	70,396,074
	13,375
	
	2013
	119543
	21,477
	0.83

	
	
	
	
	
	2014
	127848
	22,918
	0.84

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	TOTAL
	-
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4
	Operator’s comments :

Co2 primary Electricity MWh *0.1661 = tonnes Co2

Co2 Natural gas           MWh *0.19     = tonnes Co2




Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)
Permit Reference Number : UP3237CP





Operator : Solway Foods Ltd
Installation : Rogerstone Park







Form Number : PI1

Reporting of Performance Indicators for the year Jan 1st 2014………………………….to…Dec 31st 2014
	Annual Production/Treatment

	Production of frozen and chilled produce
	tonnes

	
	27,021


Environmental Performance Indicators

	Parameter
	Annual Average
	Units
	
	Trends in Environmental Performance
	
	
	

	
	
	
	
	Year
	Parameter
	
	
	
	
	

	Effluent discharged to sewer
	20.82
	M3/tonnes
	
	
	Effluent discharged to sewer
	Water use
	Non-hazardous waste
	Hazardous waste

	Water use
	23.20
	M3/tonnes
	
	
	
	
	
	

	Non-hazardous waste
	0.54
	Tonne/Tonne
	
	2011
	18.18
	22.02
	0.59
	0.00005

	Hazardous waste
	0.0001
	Tonne/Tonne
	
	2012
	18.71
	21.93
	0.58
	0.00013

	
	
	
	
	2013
	19.72
	22.43
	0.58
	0.00027

	
	
	
	
	2014
	20.82
	23.20
	0.54
	0.00027


	Operator’s comments: Hazardous waste comprising fluorescent tubes, ammonia contaminated water and oil, machine and hydraulic oil.



Signed Alica Thomas (Site Environment Manager) 



 

Date: 27th January 2015   

(authorised to sign as representative of the Operator)
BN3774IE

15/03/05

UP3237CP

27/01/14


